AVRCP PICS for the PTS tool.

PTS version: 6.1

* - different than PTS defaults
# - not yet implemented/supported

M - mandatory if such role selected
O - optional

		Roles
-------------------------------------------------------------------------------
Parameter Name    Selected	Description
-------------------------------------------------------------------------------
TSPC_AVRCP_1_1    True (*)	Role: Controller (CT) (C.1)
TSPC_AVRCP_1_2    True (*)	Role: Target (TG) (C.1)
-------------------------------------------------------------------------------
C.1: Mandatory to support at least one of the defined roles.
-------------------------------------------------------------------------------


		Controller Features
-------------------------------------------------------------------------------
Parameter Name    Selected	Description
-------------------------------------------------------------------------------
TSPC_AVRCP_2_1    False (*)	CT: Initiating connection establishment (M)
TSPC_AVRCP_2_2    False (*)	CT: Accepting connection establishment for
						control initiated by TG (M)
TSPC_AVRCP_2_3    False (*)	CT: Initiating connection release (M)
TSPC_AVRCP_2_4    False (*)	CT: Accepting connection release for control
							initiated by TG (M)
TSPC_AVRCP_2_5    False		CT: Sending UNIT INFO (O)
TSPC_AVRCP_2_6    False		CT: Sending SUBUNIT INFO (O)
TSPC_AVRCP_2_7    False		CT: Sending PASS THROUGH command category 1
					(C.1)
TSPC_AVRCP_2_8    False		CT: Sending PASS THROUGH command category 2
					(C.1)
TSPC_AVRCP_2_9    False		CT: Sending PASS THROUGH command category 3
					(C.1)
TSPC_AVRCP_2_10   False		CT: Sending PASS THROUGH command category 4
					(C.1)
TSPC_AVRCP_2_11   False		CT: Get Capabilities (O)
TSPC_AVRCP_2_12   False		CT: List Player Application Setting
					Attributes (C.9)
TSPC_AVRCP_2_13   False		CT: List Player Application Setting Values (O)
TSPC_AVRCP_2_14   False		CT: Get Current Player Application Setting
					(C.10)
TSPC_AVRCP_2_15   False		CT: Set Player Application Setting Value (C.10)
TSPC_AVRCP_2_16   False		CT: Get Player Application Setting
						Attribute Text (O)
TSPC_AVRCP_2_17   False		CT: Get Player Application Setting Value Text
					(O)
TSPC_AVRCP_2_18   False		CT: Inform Displayable Character Set (O)
TSPC_AVRCP_2_19   False		CT: Inform Battery Status of CT (O)
TSPC_AVRCP_2_20   False		CT: Get Element Attributes (O)
TSPC_AVRCP_2_21   False		CT: Get Play Status (O)
TSPC_AVRCP_2_22   False		CT: Register Notification (C.11)
TSPC_AVRCP_2_23   False		CT: Request Continuing Response (C.2)
TSPC_AVRCP_2_24   False		CT: Abort Continuing Response (C.2)
TSPC_AVRCP_2_25   False		CT: Next Group (C.12)
TSPC_AVRCP_2_26   False		CT: Previous Group (C.12)
TSPC_AVRCP_2_27   False		CT: Media Player Selection (O)
TSPC_AVRCP_2_28   False		CT: SetAddressedPlayer (O)
TSPC_AVRCP_2_29   False		CT: GetFolderItems(MediaPlayerList) (C.5)
TSPC_AVRCP_2_29b  False		CT: GetTotalNumberOfItems(MediaPlayerList) (C.5)
TSPC_AVRCP_2_30   False		CT: EVENT_AVAILABLE_PLAYERS_CHANGED (O)
TSPC_AVRCP_2_31   False		CT: EVENT_ADDRESSED_PLAYER_CHANGED (O)
TSPC_AVRCP_2_32   False		CT: Browsing (O)
TSPC_AVRCP_2_33   False		CT: SetBrowsedPlayer (C.4)
TSPC_AVRCP_2_34   False		CT: ChangePath (C.4)
TSPC_AVRCP_2_35   False		CT: GetFolderItems(Filesystem) (C.4)
TSPC_AVRCP_2_35b  False		CT: GetTotalNumberOfItems(Filesystem) (C.4)
TSPC_AVRCP_2_36   False		CT: GetItemAttributes (O)
TSPC_AVRCP_2_37   False		CT: PlayItem(Filesystem) (C.4)
TSPC_AVRCP_2_38   False		CT: EVENT_UIDS_CHANGED (O)
TSPC_AVRCP_2_39   False		CT: Searching (O)
TSPC_AVRCP_2_40   False		CT: Search (C.7)
TSPC_AVRCP_2_41   False		CT: GetFolderItems(Search Results) (C.7)
TSPC_AVRCP_2_41b  False		CT: GetTotalNumberOfItems(Search Results) (C.7)
TSPC_AVRCP_2_42   False		CT: PlayItem(SearchResultList) (C.7)
TSPC_AVRCP_2_43   False		CT: NowPlaying (C.8)
TSPC_AVRCP_2_44   False		CT: GetFolderItems(NowPlayingList) (C.8)
TSPC_AVRCP_2_44b  False		CT: GetTotalNumberOfItems(NowPlayingList) (C.8)
TSPC_AVRCP_2_45   False		CT: PlayItem(NowPlayingList) (C.8)
TSPC_AVRCP_2_46   False		CT: AddToNowPlaying (O)
TSPC_AVRCP_2_47   False		CT: EVENT_NOW_PLAYING_CONTENT_CHANGED (O)
TSPC_AVRCP_2_48   False		CT: Playable Folders (O)
TSPC_AVRCP_2_49   True (*)	CT: Absolute Volume (C.3)
TSPC_AVRCP_2_50   True (*)	CT: SetAbsoluteVolume (C.3)
TSPC_AVRCP_2_51   True (*)	CT: NotifyVolumeChange (C.3)
TSPC_AVRCP_2_52   False (*)	CT: Discoverable Mode (M)
TSPC_AVRCP_2_53   False		CT: PASSTHROUGH operation supporting press
					and hold (O)
TSPC_AVRCP_2_54   False		CT: Cover Art (O)
TSPC_AVRCP_2_55   False		CT: GetImageProperties (C.14)
TSPC_AVRCP_2_56   False		CT: GetImage (C.13)
TSPC_AVRCP_2_57   False		CT: GetLinkedThumbnail (C.13)
-------------------------------------------------------------------------------
C.1: Mandatory to support at least one of the defined categories
	(TSPC_AVRCP_2_7 through TSPC_AVRCP_2_10).
C.2: Mandatory to support at least one of TSPC_AVRCP_2_23 or TSPC_AVRC_2_24
			if TSPC_AVRCP_2_20 is supported, otherwise Optional.
C.3: Mandatory if TSPC_AVRCP_2_8 is supported, otherwise Excluded.
C.4: Mandatory if TSPC_AVRCP_2_32 is supported, otherwise Excluded.
C.5: Mandatory if TSPC_AVRCP_2_27 is supported, otherwise Excluded.
C.7: Mandatory if item TSPC_AVRCP_2_39 is supported, Excluded otherwise.
C.8: Mandatory if TSPC_AVRCP_2_32 is supported, otherwise Excluded.
C.9: Mandatory to support if Player Application Settings feature is supported.
	If any item TSPC_AVRCP_2_13 through TSPC_AVRCP_2_15 is supported it is
	required to claim support for this feature in accordance with Player
	Application Settings support requirements, otherwise Optional.
C.10: Mandatory to support either Get or Set Player Application Settings
	(TSPC_AVRCP_2_14 or TSPC_AVRCP_2_15) if List Player Application Setting
	Attributes (TSPC_AVRCP_2_12) is supported. Either TSPC_AVRCP_2_14
	or TSPC_AVRCP_2_15 must be supported if Player Application Settings
	feature is supported, in accordance with Player Application Settings
	support requirements.
C.11: Mandatory if TSPC_AVRCP_2_20 or TSPC_AVRCP_2_49 is supported, otherwise
	Optional.
C.12: Mandatory if Basic Group Navigation Feature supported. If any item
	TSPC_AVRCP_2_25 or TSPC_AVRCP_2_26 is supported it is mandatory to
	support both, in accordance with Basic Group Navigation support
	requirements, otherwise Excluded.
C.13: Mandatory to support at least one of the functions if TSPC_AVRCP_2_54
	(Cover Art) is support, otherwise Excluded.
C.14: Optional if TSPC_AVRCP_2_54 (Cover Art) is supported, otherwise Excluded.
-------------------------------------------------------------------------------


		Controller Profile Version
-------------------------------------------------------------------------------
Parameter Name    Selected	Description
-------------------------------------------------------------------------------
TSPC_AVRCP_2b_1   False		CT: AVRCP v1.0 (C.1)
TSPC_AVRCP_2b_2   False		CT: AVRCP v1.3 (C.1)
TSPC_AVRCP_2b_3   False		CT: AVRCP v1.4 (C.1)
TSPC_AVRCP_2b_4   False		CT: AVRCP v1.5 (C.1)
TSPC_AVRCP_2b_5   False		CT: AVRCP v1.6 (C.1)
-------------------------------------------------------------------------------
C.1: It is mandatory to support at least one of the profile versions if
	Controller role supported (SPC_AVRCP_1_1).
-------------------------------------------------------------------------------


		Operation_id of Category 1 for CT
-------------------------------------------------------------------------------
Parameter Name    Selected	Description
-------------------------------------------------------------------------------
TSPC_AVRCP_3_1    False		CT: category 1 - Operation id: 0 (C.1)
TSPC_AVRCP_3_2    False		CT: category 1 - Operation id: 1 (C.1)
TSPC_AVRCP_3_3    False		CT: category 1 - Operation id: 2 (C.1)
TSPC_AVRCP_3_4    False		CT: category 1 - Operation id: 3 (C.1)
TSPC_AVRCP_3_5    False		CT: category 1 - Operation id: 4 (C.1)
TSPC_AVRCP_3_6    False		CT: category 1 - Operation id: 5 (C.1)
TSPC_AVRCP_3_7    False		CT: category 1 - Operation id: 6 (C.1)
TSPC_AVRCP_3_8    False		CT: category 1 - Operation id: 7 (C.1)
TSPC_AVRCP_3_9    False		CT: category 1 - Operation id: 8 (C.1)
TSPC_AVRCP_3_10   False		CT: category 1 - Operation id: 9 (C.1)
TSPC_AVRCP_3_11   False		CT: category 1 - Operation id: dot (C.1)
TSPC_AVRCP_3_12   False		CT: category 1 - Operation id: enter (C.1)
TSPC_AVRCP_3_13   False		CT: category 1 - Operation id: clear (C.1)
TSPC_AVRCP_3_14   False		CT: category 1 - Operation id: sound_select
					(C.1)
TSPC_AVRCP_3_15   False		CT: category 1 - Operation id: input_select
					(C.1)
TSPC_AVRCP_3_16   False		CT: category 1 - Operation id:
					display_information (C.1)
TSPC_AVRCP_3_17   False		CT: category 1 - Operation id: help (C.1)
TSPC_AVRCP_3_18   False		CT: category 1 - Operation id: power (C.1)
TSPC_AVRCP_3_19   False		CT: category 1 - Operation id: play (C.1)
TSPC_AVRCP_3_20   False		CT: category 1 - Operation id: stop (C.1)
TSPC_AVRCP_3_21   False		CT: category 1 - Operation id: pause (C.1)
TSPC_AVRCP_3_22   False		CT: category 1 - Operation id: record (C.1)
TSPC_AVRCP_3_23   False		CT: category 1 - Operation id: rewind (C.1)
TSPC_AVRCP_3_24   False		CT: category 1 - Operation id: fast_forward
					(C.1)
TSPC_AVRCP_3_25   False		CT: category 1 - Operation id: eject (C.1)
TSPC_AVRCP_3_26   False		CT: category 1 - Operation id: forward (C.1)
TSPC_AVRCP_3_27   False		CT: category 1 - Operation id: backward (C.1)
TSPC_AVRCP_3_28   False		CT: category 1 - Operation id: angle (C.1)
TSPC_AVRCP_3_29   False		CT: category 1 - Operation id: subpicture (C.1)
TSPC_AVRCP_3_30   False		CT: category 1 - Operation id: F1 (C.1)
TSPC_AVRCP_3_31   False		CT: category 1 - Operation id: F2 (C.1)
TSPC_AVRCP_3_32   False		CT: category 1 - Operation id: F3 (C.1)
TSPC_AVRCP_3_33   False		CT: category 1 - Operation id: F4 (C.1)
TSPC_AVRCP_3_34   False		CT: category 1 - Operation id: vendor_unique
					(C.1)
-------------------------------------------------------------------------------
C.1: Mandatory to support at least one of these operation_ids if the device
	supports category 1 (TSPC_AVRCP_2_7).
-------------------------------------------------------------------------------


		Operation_id of category 2 for CT
-------------------------------------------------------------------------------
Parameter Name    Selected	Description
-------------------------------------------------------------------------------
TSPC_AVRCP_4_1    False		CT: category 2 - Operation id: 0 (C.1)
TSPC_AVRCP_4_2    False		CT: category 2 - Operation id: 1 (C.1)
TSPC_AVRCP_4_3    False		CT: category 2 - Operation id: 2 (C.1)
TSPC_AVRCP_4_4    False		CT: category 2 - Operation id: 3 (C.1)
TSPC_AVRCP_4_5    False		CT: category 2 - Operation id: 4 (C.1)
TSPC_AVRCP_4_6    False		CT: category 2 - Operation id: 5 (C.1)
TSPC_AVRCP_4_7    False		CT: category 2 - Operation id: 6 (C.1)
TSPC_AVRCP_4_8    False		CT: category 2 - Operation id: 7 (C.1)
TSPC_AVRCP_4_9    False		CT: category 2 - Operation id: 8 (C.1)
TSPC_AVRCP_4_10   False		CT: category 2 - Operation id: 9 (C.1)
TSPC_AVRCP_4_11   False		CT: category 2 - Operation id: dot (C.1)
TSPC_AVRCP_4_12   False		CT: category 2 - Operation id: enter (C.1)
TSPC_AVRCP_4_13   False		CT: category 2 - Operation id: clear (C.1)
TSPC_AVRCP_4_14   False		CT: category 2 - Operation id: sound_select
					(C.1)
TSPC_AVRCP_4_15   False		CT: category 2 - Operation id: input_select
					(C.1)
TSPC_AVRCP_4_16   False		CT: category 2 - Operation id:
					display_information (C.1)
TSPC_AVRCP_4_17   False		CT: category 2 - Operation id: help (C.1)
TSPC_AVRCP_4_18   False		CT: category 2 - Operation id: power (C.1)
TSPC_AVRCP_4_19   False		CT: category 2 - Operation id: volume_up (C.1)
TSPC_AVRCP_4_20   False		CT: category 2 - Operation id: volume_down (C.1)
TSPC_AVRCP_4_21   False		CT: category 2 - Operation id: mute (C.1)
TSPC_AVRCP_4_22   False		CT: category 2 - Operation id: F1 (C.1)
TSPC_AVRCP_4_23   False		CT: category 2 - Operation id: F2 (C.1)
TSPC_AVRCP_4_24   False		CT: category 2 - Operation id: F3 (C.1)
TSPC_AVRCP_4_25   False		CT: category 2 - Operation id: F4 (C.1)
TSPC_AVRCP_4_26   False		CT: category 2 - Operation id: vendor_unique
					(C.1)
-------------------------------------------------------------------------------
C.1: Mandatory to support at least one of these operation_ids if the device
	supports category 2 (TSPC_AVRCP_2_8).
-------------------------------------------------------------------------------


		Operation_id of category 3 for CT
-------------------------------------------------------------------------------
Parameter Name    Selected	Description
-------------------------------------------------------------------------------
TSPC_AVRCP_5_1    False		CT: category 3 - Operation id: 0 (C.1)
TSPC_AVRCP_5_2    False		CT: category 3 - Operation id: 1 (C.1)
TSPC_AVRCP_5_3    False		CT: category 3 - Operation id: 2 (C.1)
TSPC_AVRCP_5_4    False		CT: category 3 - Operation id: 3 (C.1)
TSPC_AVRCP_5_5    False		CT: category 3 - Operation id: 4 (C.1)
TSPC_AVRCP_5_6    False		CT: category 3 - Operation id: 5 (C.1)
TSPC_AVRCP_5_7    False		CT: category 3 - Operation id: 6 (C.1)
TSPC_AVRCP_5_8    False		CT: category 3 - Operation id: 7 (C.1)
TSPC_AVRCP_5_9    False		CT: category 3 - Operation id: 8 (C.1)
TSPC_AVRCP_5_10   False		CT: category 3 - Operation id: 9 (C.1)
TSPC_AVRCP_5_11   False		CT: category 3 - Operation id: dot (C.1)
TSPC_AVRCP_5_12   False		CT: category 3 - Operation id: enter (C.1)
TSPC_AVRCP_5_13   False		CT: category 3 - Operation id: clear (C.1)
TSPC_AVRCP_5_14   False		CT: category 3 - Operation id: channel up (C.1)
TSPC_AVRCP_5_15   False		CT: category 3 - Operation id: channel down
					(C.1)
TSPC_AVRCP_5_16   False		CT: category 3 - Operation id: previous channel
					(C.1)
TSPC_AVRCP_5_17   False		CT: category 3 - Operation id: sound_select
					(C.1)
TSPC_AVRCP_5_18   False		CT: category 3 - Operation id: input_select
					(C.1)
TSPC_AVRCP_5_19   False		CT: category 3 - Operation id:
					display_information (C.1)
TSPC_AVRCP_5_20   False		CT: category 3 - Operation id: help (C.1)
TSPC_AVRCP_5_21   False		CT: category 3 - Operation id: power (C.1)
TSPC_AVRCP_5_22   False		CT: category 3 - Operation id: angle (C.1)
TSPC_AVRCP_5_23   False		CT: category 3 - Operation id: subpicture(C.1)
TSPC_AVRCP_5_24   False		CT: category 3 - Operation id: F1 (C.1)
TSPC_AVRCP_5_25   False		CT: category 3 - Operation id: F2 (C.1)
TSPC_AVRCP_5_26   False		CT: category 3 - Operation id: F3 (C.1)
TSPC_AVRCP_5_27   False		CT: category 3 - Operation id: F4 (C.1)
TSPC_AVRCP_5_28   False		CT: category 3 - Operation id: vendor_unique
					(C.1)
-------------------------------------------------------------------------------
C.1: Mandatory to support at least one of these operation_ids if the device
	supports category 3 (TSPC_AVRCP_2_9).
-------------------------------------------------------------------------------


		Operation_id of category 4 for CT
-------------------------------------------------------------------------------
Parameter Name    Selected	Description
-------------------------------------------------------------------------------
TSPC_AVRCP_6_1    False		CT: category 4 - Operation id: select (C.1)
TSPC_AVRCP_6_2    False		CT: category 4 - Operation id: up (C.1)
TSPC_AVRCP_6_3    False		CT: category 4 - Operation id: down (C.1)
TSPC_AVRCP_6_4    False		CT: category 4 - Operation id: left (C.1)
TSPC_AVRCP_6_5    False		CT: category 4 - Operation id: right (C.1)
TSPC_AVRCP_6_6    False		CT: category 4 - Operation id: right up (C.1)
TSPC_AVRCP_6_7    False		CT: category 4 - Operation id: right down (C.1)
TSPC_AVRCP_6_8    False		CT: category 4 - Operation id: left up (C.1)
TSPC_AVRCP_6_9    False		CT: category 4 - Operation id: left down (C.1)
TSPC_AVRCP_6_10   False		CT: category 4 - Operation id: root menu (C.1)
TSPC_AVRCP_6_11   False		CT: category 4 - Operation id: setup menu (C.1)
TSPC_AVRCP_6_12   False		CT: category 4 - Operation id: contents menu
					(C.1)
TSPC_AVRCP_6_13   False		CT: category 4 - Operation id: favorite menu
					(C.1)
TSPC_AVRCP_6_14   False		CT: category 4 - Operation id: exit (C.1)
TSPC_AVRCP_6_15   False		CT: category 4 - Operation id: 0 (C.1)
TSPC_AVRCP_6_16   False		CT: category 4 - Operation id: 1 (C.1)
TSPC_AVRCP_6_17   False		CT: category 4 - Operation id: 2 (C.1)
TSPC_AVRCP_6_18   False		CT: category 4 - Operation id: 3 (C.1)
TSPC_AVRCP_6_19   False		CT: category 4 - Operation id: 4 (C.1)
TSPC_AVRCP_6_20   False		CT: category 4 - Operation id: 5 (C.1)
TSPC_AVRCP_6_21   False		CT: category 4 - Operation id: 6 (C.1)
TSPC_AVRCP_6_22   False		CT: category 4 - Operation id: 7 (C.1)
TSPC_AVRCP_6_23   False		CT: category 4 - Operation id: 8 (C.1)
TSPC_AVRCP_6_24   False		CT: category 4 - Operation id: 9 (C.1)
TSPC_AVRCP_6_25   False		CT: category 4 - Operation id: dot (C.1)
TSPC_AVRCP_6_26   False		CT: category 4 - Operation id: enter (C.1)
TSPC_AVRCP_6_27   False		CT: category 4 - Operation id: clear (C.1)
TSPC_AVRCP_6_28   False		CT: category 4 - Operation id:
					display_information (C.1)
TSPC_AVRCP_6_29   False		CT: category 4 - Operation id: help (C.1)
TSPC_AVRCP_6_30   False		CT: category 4 - Operation id: page up (C.1)
TSPC_AVRCP_6_31   False		CT: category 4 - Operation id: page down (C.1)
TSPC_AVRCP_6_32   False		CT: category 4 - Operation id: power (C.1)
TSPC_AVRCP_6_33   False		CT: category 4 - Operation id: F1 (C.1)
TSPC_AVRCP_6_34   False		CT: category 4 - Operation id: F2 (C.1)
TSPC_AVRCP_6_35   False		CT: category 4 - Operation id: F3 (C.1)
TSPC_AVRCP_6_36   False		CT: category 4 - Operation id: F4 (C.1)
TSPC_AVRCP_6_37   False		CT: category 4 - Operation id: vendor_unique
					(C.1)
-------------------------------------------------------------------------------
C.1: Mandatory to support at least one of these operation_ids if the device
	supports category 4 (TSPC_AVRCP_2_10).
-------------------------------------------------------------------------------


		Target Features
-------------------------------------------------------------------------------
Parameter Name    Selected	Description
-------------------------------------------------------------------------------
TSPC_AVRCP_7_1    True (*)	TG: Initiating connection establishment for
					Control (O)
TSPC_AVRCP_7_2    True		TG: Accept connection establishment for Control
					initiated by CT (M)
TSPC_AVRCP_7_3    True (*)	TG: Initiating connection release (M)
TSPC_AVRCP_7_4    True		TG: Accepting connection release (M)
TSPC_AVRCP_7_5    True		TG: Receiving UNIT INFO (M)
TSPC_AVRCP_7_6    True		TG: Receiving SUBUNIT INFO (M)
TSPC_AVRCP_7_7    True (*)	TG: Receiving PASS THROUGH command category 1
					(C.1)
TSPC_AVRCP_7_8    True (*)	TG: Receiving PASS THROUGH command category 2
					(C.1)
TSPC_AVRCP_7_9    False		TG: Receiving PASS THROUGH command category 3
					(C.1)
TSPC_AVRCP_7_10   False		TG: Receiving PASS THROUGH command category 4
					(C.1)
TSPC_AVRCP_7_11   True (*)	TG: Get Capabilities Response (C.3)
TSPC_AVRCP_7_12   False		TG: List Player Application Settings Attributes
					Response (C.14)
TSPC_AVRCP_7_13   False		TG: List Player Application Setting Values
					Response (C.14)
TSPC_AVRCP_7_14   False		TG: Get Current Player Application Settings
					Value Response (C.14)
TSPC_AVRCP_7_15   False		TG: Set Player Application Setting Value
					Response (C.14)
TSPC_AVRCP_7_16   False		TG: Get Player Application Setting Attribute
					Text Response (O)
TSPC_AVRCP_7_17   False		TG: Get Player Application Setting Value Text
					Response (O)
TSPC_AVRCP_7_18   False		TG: Inform Displayable Character Set Response
					(O)
TSPC_AVRCP_7_19   False		TG: Inform Battery Status Of CT Response (O)
TSPC_AVRCP_7_20   True (*)	TG: Get Element Attributes Response (C.3)
TSPC_AVRCP_7_21   True (*)	TG: Get Play Status Response (C.2)
TSPC_AVRCP_7_22   True (*)	TG: Register Notification Response (C.12)
TSPC_AVRCP_7_23   True (*)	TG: Notify Event Response:
					PLAYBACK_STATUS_CHANGED (C.4)
TSPC_AVRCP_7_24   True (*)	TG: Notify Event Response: TRACK_CHANGED (C.4)
TSPC_AVRCP_7_25   False		TG: Notify Event Response: TRACK_REACHED_END (O)
TSPC_AVRCP_7_26   False		TG: Notify Event Response: TRACK_REACHED_START
					(O)
TSPC_AVRCP_7_27   False		TG: Notify Event Response: PLAYBACK_POS_CHANGED
					(O)
TSPC_AVRCP_7_28   False		TG: Notify Event Response: BATT_STATUS_CHANGED
					(O)
TSPC_AVRCP_7_29   False		TG: Notify Event Response: SYSTEM_STATUS_CHANGED
					(O)
TSPC_AVRCP_7_30   False		TG: Notify Event Response:
					PLAYER_APPLICATION_SETTING_CHANGED (O)
TSPC_AVRCP_7_31   True (*)	TG: Request Continuing Response (C.2)
TSPC_AVRCP_7_32   True (*)	TG: Abort ContinuingResponse Response (C.2)
TSPC_AVRCP_7_34   False		TG: Next Group (C.15)
TSPC_AVRCP_7_35   False		TG: Previous Group (C.15)
TSPC_AVRCP_7_36   False		TG: Media Player Selection (C.8)
TSPC_AVRCP_7_37   False		TG: SetAddressedPlayer (C.8)
TSPC_AVRCP_7_38   False		TG: GetFolderItems(MediaPlayerList) (C.8)
TSPC_AVRCP_7_38b  False		TG: GetTotalNumberOfItems(MediaPlayerList) (C.8)
TSPC_AVRCP_7_39   False		TG: EVENT_AVAILABLE_PLAYERS_CHANGED (C.8)
TSPC_AVRCP_7_40   False		TG: EVENT_ADDRESSED_PLAYER_CHANGED (C.8)
TSPC_AVRCP_7_41   False		TG: Supports Multiple Players (O)
TSPC_AVRCP_7_42   False		TG: Browsing (O)
TSPC_AVRCP_7_42a  False		TG: Initiating connection establishment for
					browsing channel (O)
TSPC_AVRCP_7_43   False		TG: SetBrowsedPlayer (C.6)
TSPC_AVRCP_7_44   False		TG: ChangePath (C.6)
TSPC_AVRCP_7_45   False		TG: GetFolderItems(Filesystem) (C.6)
TSPC_AVRCP_7_45b  False		TG: GetTotalNumberOfItems(Filesystem) (C.6)
TSPC_AVRCP_7_46   False		TG: GetItemAttributes (C.6)
TSPC_AVRCP_7_47   False		TG: PlayItem(Filesystem) (C.6)
TSPC_AVRCP_7_48   False		TG: EVENT_UIDS_CHANGED (C.9)
TSPC_AVRCP_7_49   False		TG: Database Aware Players (O)
TSPC_AVRCP_7_50   False		TG: Searching (O)
TSPC_AVRCP_7_51   False		TG: Search (C.10)
TSPC_AVRCP_7_52   False		TG: GetFolderItems(Search Results) (C.10)
TSPC_AVRCP_7_52b  False		TG: GetTotalNumberOfItems(Search Results) (C.10)
TSPC_AVRCP_7_53   False		TG: PlayItem(SearchResultList) (C.10)
TSPC_AVRCP_7_54   False		TG: NowPlaying (C.11)
TSPC_AVRCP_7_55   False		TG: GetFolderItems(NowPlayingList) (C.11)
TSPC_AVRCP_7_55b  False		TG: GetTotalNumberOfItems(NowPlayingList) (C.11)
TSPC_AVRCP_7_56   False		TG: PlayItem(NowPlayingList) (C.11)
TSPC_AVRCP_7_57   False		TG: AddToNowPlaying (O)
TSPC_AVRCP_7_58   False		TG: EVENT_NOW_PLAYING_CONTENT_CHANGED (C.11)
TSPC_AVRCP_7_59   False		TG: Playable Folders (O)
TSPC_AVRCP_7_60   False		TG: Absolute Volume (C.5)
TSPC_AVRCP_7_61   False		TG: SetAbsoluteVolume (C.5)
TSPC_AVRCP_7_62   False		TG: NotifyVolumeChange (C.5)
TSPC_AVRCP_7_63   False		TG: Error Response (O)
TSPC_AVRCP_7_64   False		TG: General Reject (C.13)
TSPC_AVRCP_7_65   True		TG: Discoverable Mode (M)
TSPC_AVRCP_7_66   False		TG: PASSTHROUGH operation supporting press
					and hold (O)
TSPC_AVRCP_7_67   False		TG: Cover Art (O)
TSPC_AVRCP_7_68   False		TG: GetImageProperties (C.16)
TSPC_AVRCP_7_69   False		TG: GetImage (C.16)
TSPC_AVRCP_7_70   False		TG: GetLinkedThumbnail (C.16)
-------------------------------------------------------------------------------
C.1: Mandatory to support at least one of the categories. Supported
	operation_id's are shown in Table 8 to Table 11.
C.2: Mandatory if 7/20 is supported, otherwise Optional.
C.3: Mandatory if 7/7 is supported, otherwise Optional.
C.4: Mandatory if 7/22 and 7/20 is supported, otherwise Optional.
C.5: Mandatory if 7/8 is supported, otherwise Excluded.
C.6: Mandatory if 7/42 is supported, otherwise Excluded.
C.7: Mandatory if 7/36 is supported, otherwise Excluded.
C.8: Mandatory if (7/7 or 7/9) is supported, otherwise Excluded.
C.9: Mandatory if 7/49 is supported, otherwise Optional.
C.10: Mandatory if 7/50 is supported, otherwise Excluded.
C.11: Mandatory if 7/42 is supported, otherwise Optional.
C.12: Mandatory if 7/7 or (7/8 AND 7/60) or 7/9 is supported, otherwise Optional
C.13: Mandatory if 7/7 or 7/9 or 7/42 is supported, otherwise Optional.
C.14: Mandatory if Player Application Settings Feature supported. If any item
	7/12 – 7/15 is supported, all items 7/12 – 7/15 shall be supported,
	in accordance with Player Application Settings Feature support
	requirements, otherwise Excluded.
C.15: Mandatory if Basic Group Navigation Feature supported. If any item
	7/34 or 7/35 is supported it is mandatory to support both,
	in accordance with Basic Group Navigation support requirements,
	otherwise Excluded.
C.16: Mandatory if 7/67 (Cover Art) is supported, otherwise Excluded.
-------------------------------------------------------------------------------

		Target Profile Version
-------------------------------------------------------------------------------
Parameter Name    Selected	Description
-------------------------------------------------------------------------------
TSPC_AVRCP_7b_1   False		TG: AVRCP v1.0 (C.1)
TSPC_AVRCP_7b_2   False		TG: AVRCP v1.3 (C.1)
TSPC_AVRCP_7b_3   False		TG: AVRCP v1.4 (C.1)
TSPC_AVRCP_7b_4   True (*)	TG: AVRCP v1.5 (C.1)
TSPC_AVRCP_7b_5   False		TG: AVRCP v1.6 (C.1)
-------------------------------------------------------------------------------
C.1: It is mandatory to support at least one of the profile versions.
-------------------------------------------------------------------------------


		operation_id of category 1 for TG
-------------------------------------------------------------------------------
Parameter Name    Selected	Description
-------------------------------------------------------------------------------
TSPC_AVRCP_8_1    False		TG: category 1 - Operation id: 0 (O)
TSPC_AVRCP_8_2    False		TG: category 1 - Operation id: 1 (O)
TSPC_AVRCP_8_3    False		TG: category 1 - Operation id: 2 (O)
TSPC_AVRCP_8_4    False		TG: category 1 - Operation id: 3 (O)
TSPC_AVRCP_8_5    False		TG: category 1 - Operation id: 4 (O)
TSPC_AVRCP_8_6    False		TG: category 1 - Operation id: 5 (O)
TSPC_AVRCP_8_7    False		TG: category 1 - Operation id: 6 (O)
TSPC_AVRCP_8_8    False		TG: category 1 - Operation id: 7 (O)
TSPC_AVRCP_8_9    False		TG: category 1 - Operation id: 8 (O)
TSPC_AVRCP_8_10   False		TG: category 1 - Operation id: 9 (O)
TSPC_AVRCP_8_11   False		TG: category 1 - Operation id: dot (O)
TSPC_AVRCP_8_12   False		TG: category 1 - Operation id: enter (O)
TSPC_AVRCP_8_13   False		TG: category 1 - Operation id: clear (O)
TSPC_AVRCP_8_14   False		TG: category 1 - Operation id: sound select (O)
TSPC_AVRCP_8_15   False		TG: category 1 - Operation id: input select (O)
TSPC_AVRCP_8_16   False		TG: category 1 - Operation id: display
					information (O)
TSPC_AVRCP_8_17   False		TG: category 1 - Operation id: help (O)
TSPC_AVRCP_8_18   False		TG: category 1 - Operation id: power (O)
TSPC_AVRCP_8_19   True		TG: category 1 - Operation id: play (M)
TSPC_AVRCP_8_20   True		TG: category 1 - Operation id: stop (M)
TSPC_AVRCP_8_21   True (*)	TG: category 1 - Operation id: pause (O)
TSPC_AVRCP_8_22   False		TG: category 1 - Operation id: record (O)
TSPC_AVRCP_8_23   True (*)	TG: category 1 - Operation id: rewind (O)
TSPC_AVRCP_8_24   True (*)	TG: category 1 - Operation id: fast forward (O)
TSPC_AVRCP_8_25   False		TG: category 1 - Operation id: eject (O)
TSPC_AVRCP_8_26   True (*)	TG: category 1 - Operation id: forward (O)
TSPC_AVRCP_8_27   True (*)	TG: category 1 - Operation id: backward (O)
TSPC_AVRCP_8_28   False		TG: category 1 - Operation id: angle (O)
TSPC_AVRCP_8_29   False		TG: category 1 - Operation id: subpicture (O)
TSPC_AVRCP_8_30   False		TG: category 1 - Operation id: F1 (O)
TSPC_AVRCP_8_31   False		TG: category 1 - Operation id: F2 (O)
TSPC_AVRCP_8_32   False		TG: category 1 - Operation id: F3 (O)
TSPC_AVRCP_8_33   False		TG: category 1 - Operation id: F4 (O)
TSPC_AVRCP_8_33a  False		TG: category 1 - Operation id: F5 (O)
TSPC_AVRCP_8_34   False		TG: category 1 - Operation id: vendor unique (O)
-------------------------------------------------------------------------------


		operation_id of category 2 for TG
-------------------------------------------------------------------------------
Parameter Name    Selected	Description
-------------------------------------------------------------------------------
TSPC_AVRCP_9_1    False		TG: category 2 - Operation id: 0 (O)
TSPC_AVRCP_9_2    False		TG: category 2 - Operation id: 1 (O)
TSPC_AVRCP_9_3    False		TG: category 2 - Operation id: 2 (O)
TSPC_AVRCP_9_4    False		TG: category 2 - Operation id: 3 (O)
TSPC_AVRCP_9_5    False		TG: category 2 - Operation id: 4 (O)
TSPC_AVRCP_9_6    False		TG: category 2 - Operation id: 5 (O)
TSPC_AVRCP_9_7    False		TG: category 2 - Operation id: 6 (O)
TSPC_AVRCP_9_8    False		TG: category 2 - Operation id: 7 (O)
TSPC_AVRCP_9_9    False		TG: category 2 - Operation id: 8 (O)
TSPC_AVRCP_9_10   False		TG: category 2 - Operation id: 9 (O)
TSPC_AVRCP_9_11   False		TG: category 2 - Operation id: dot (O)
TSPC_AVRCP_9_12   False		TG: category 2 - Operation id: enter (O)
TSPC_AVRCP_9_13   False		TG: category 2 - Operation id: clear (O)
TSPC_AVRCP_9_14   False		TG: category 2 - Operation id: sound select (O)
TSPC_AVRCP_9_15   False		TG: category 2 - Operation id: input select (O)
TSPC_AVRCP_9_16   False		TG: category 2 - Operation id: display
					information (O)
TSPC_AVRCP_9_17	  False		TG: category 2 - Operation id: help (O)
TSPC_AVRCP_9_18	  False		TG: category 2 - Operation id: power (O)
TSPC_AVRCP_9_19   True		TG: category 2 - Operation id: volume up (C.2)
TSPC_AVRCP_9_20   True		TG: category 2 - Operation id: volume down (C.2)
TSPC_AVRCP_9_21   False		TG: category 2 - Operation id: mute (O)
TSPC_AVRCP_9_24   False		TG: category 2 - Operation id: F1 (O)
TSPC_AVRCP_9_25   False		TG: category 2 - Operation id: F2 (O)
TSPC_AVRCP_9_26   False		TG: category 2 - Operation id: F3 (O)
TSPC_AVRCP_9_27   False		TG: category 2 - Operation id: F4 (O)
TSPC_AVRCP_9_27a  False		TG: category 2 - Operation id: F5 (O)
TSPC_AVRCP_9_28   False		TG: category 2 - Operation id: vendor unique (O)
-------------------------------------------------------------------------------
C.2: Mandatory to support if the device supports category 2 (TSPC_AVRCP_7_8).
-------------------------------------------------------------------------------


		operation_id of category 3 for TG
-------------------------------------------------------------------------------
Parameter Name    Selected	Description
-------------------------------------------------------------------------------
TSPC_AVRCP_10_1   False		TG: category 3 - Operation id: 0 (O)
TSPC_AVRCP_10_2   False		TG: category 3 - Operation id: 1 (O)
TSPC_AVRCP_10_3   False		TG: category 3 - Operation id: 2 (O)
TSPC_AVRCP_10_4   False		TG: category 3 - Operation id: 3 (O)
TSPC_AVRCP_10_5   False		TG: category 3 - Operation id: 4 (O)
TSPC_AVRCP_10_6   False		TG: category 3 - Operation id: 5 (O)
TSPC_AVRCP_10_7   False		TG: category 3 - Operation id: 6 (O)
TSPC_AVRCP_10_8   False		TG: category 3 - Operation id: 7 (O)
TSPC_AVRCP_10_9   False		TG: category 3 - Operation id: 8 (O)
TSPC_AVRCP_10_10  False		TG: category 3 - Operation id: 9 (O)
TSPC_AVRCP_10_11  False		TG: category 3 - Operation id: dot (O)
TSPC_AVRCP_10_12  False		TG: category 3 - Operation id: enter (O)
TSPC_AVRCP_10_13  False		TG: category 3 - Operation id: clear (O)
TSPC_AVRCP_10_14  False (*)	TG: category 3 - Operation id: channel up (C.3)
TSPC_AVRCP_10_15  False (*)	TG: category 3 - Operation id: channel down
					(C.3)
TSPC_AVRCP_10_16  False		TG: category 3 - Operation id: previous channel
					(O)
TSPC_AVRCP_10_17  False		TG: category 3 - Operation id: sound select (O)
TSPC_AVRCP_10_18  False		TG: category 3 - Operation id: input select (O)
TSPC_AVRCP_10_19  False		TG: category 3 - Operation id: display
					information (O)
TSPC_AVRCP_10_20  False		TG: category 3 - Operation id: help (O)
TSPC_AVRCP_10_21  False		TG: category 3 - Operation id: power (O)
TSPC_AVRCP_10_21a False		TG: category 3 - Operation id: angle (O)
TSPC_AVRCP_10_21b False		TG: category 3 - Operation id: subpicture (O)
TSPC_AVRCP_10_22  False		TG: category 3 - Operation id: F1 (O)
TSPC_AVRCP_10_23  False		TG: category 3 - Operation id: F2 (O)
TSPC_AVRCP_10_24  False		TG: category 3 - Operation id: F3 (O)
TSPC_AVRCP_10_25  False		TG: category 3 - Operation id: F4 (O)
TSPC_AVRCP_10_25a False		TG: category 3 - Operation id: F5 (O)
TSPC_AVRCP_10_26  False		TG: category 3 - Operation id: vendor unique (O)
-------------------------------------------------------------------------------
C.3: Mandatory to support if the device supports category 3 (TSPC_AVRCP_7_9).
-------------------------------------------------------------------------------


		operation_id of category 4 for TG
-------------------------------------------------------------------------------
Parameter Name    Selected	Description
-------------------------------------------------------------------------------
TSPC_AVRCP_11_1   False (*)	TG: category 4 - Operation id: select (C.4)
TSPC_AVRCP_11_2   False (*)	TG: category 4 - Operation id: up (C.4)
TSPC_AVRCP_11_3   False (*)	TG: category 4 - Operation id: down (C.4)
TSPC_AVRCP_11_4   False (*)	TG: category 4 - Operation id: left (C.4)
TSPC_AVRCP_11_5   False (*)	TG: category 4 - Operation id: right (C.4)
TSPC_AVRCP_11_6   False		TG: category 4 - Operation id: right up (O)
TSPC_AVRCP_11_7   False		TG: category 4 - Operation id: right down (O)
TSPC_AVRCP_11_8   False		TG: category 4 - Operation id: left up (O)
TSPC_AVRCP_11_9   False		TG: category 4 - Operation id: left down (O)
TSPC_AVRCP_11_10  False (*)	TG: category 4 - Operation id: root menu (C.4)
TSPC_AVRCP_11_11  False		TG: category 4 - Operation id: setup menu (O)
TSPC_AVRCP_11_12  False		TG: category 4 - Operation id: contents menu (O)
TSPC_AVRCP_11_13  False		TG: category 4 - Operation id: favorite menu (O)
TSPC_AVRCP_11_14  False		TG: category 4 - Operation id: exit (O)
TSPC_AVRCP_11_15  False		TG: category 4 - Operation id: 0 (O)
TSPC_AVRCP_11_16  False		TG: category 4 - Operation id: 1 (O)
TSPC_AVRCP_11_17  False		TG: category 4 - Operation id: 2 (O)
TSPC_AVRCP_11_18  False		TG: category 4 - Operation id: 3 (O)
TSPC_AVRCP_11_19  False		TG: category 4 - Operation id: 4 (O)
TSPC_AVRCP_11_20  False		TG: category 4 - Operation id: 5 (O)
TSPC_AVRCP_11_21  False		TG: category 4 - Operation id: 6 (O)
TSPC_AVRCP_11_22  False		TG: category 4 - Operation id: 7 (O)
TSPC_AVRCP_11_23  False		TG: category 4 - Operation id: 8 (O)
TSPC_AVRCP_11_24  False		TG: category 4 - Operation id: 9 (O)
TSPC_AVRCP_11_25  False		TG: category 4 - Operation id: dot (O)
TSPC_AVRCP_11_26  False		TG: category 4 - Operation id: enter (O)
TSPC_AVRCP_11_27  False		TG: category 4 - Operation id: clear (O)
TSPC_AVRCP_11_28  False		TG: category 4 - Operation id: disply (O)
TSPC_AVRCP_11_29  False		TG: category 4 - Operation id: help (O)
TSPC_AVRCP_11_30  False		TG: category 4 - Operation id: page up (O)
TSPC_AVRCP_11_31  False		TG: category 4 - Operation id: page down (O)
TSPC_AVRCP_11_32  False		TG: category 4 - Operation id: power (O)
TSPC_AVRCP_11_33  False		TG: category 4 - Operation id: F1 (O)
TSPC_AVRCP_11_34  False		TG: category 4 - Operation id: F2 (O)
TSPC_AVRCP_11_35  False		TG: category 4 - Operation id: F3 (O)
TSPC_AVRCP_11_36  False		TG: category 4 - Operation id: F4 (O)
TSPC_AVRCP_11_36a False		TG: category 4 - Operation id: F5 (O)
TSPC_AVRCP_11_37  False		TG: category 4 - Operation id: vendor unique (O)

TSPC_AVRCP_12_1   True		General discoverable mode (M)
TSPC_AVRCP_13_1   True		General discoverable mode (M)
TSPC_AVRCP_14_1   False		OBEX Connect operation (C.1)
TSPC_AVRCP_14_2   False		OBEX Get operation (C.1)
TSPC_AVRCP_14_3   False		OBEX Disconnect operation (C.1)
TSPC_AVRCP_15_1   False		OBEX Connect operation (C.1)
TSPC_AVRCP_15_2   False		OBEX Get operation (C.1)
TSPC_AVRCP_15_3   False		OBEX Disconnect operation (C.1)

TSPC_ALL          False		Enables all test cases when set to TRUE.
-------------------------------------------------------------------------------
C.4: Mandatory to support if the device supports category 4 (TSPC_AVRCP_7_10).
-------------------------------------------------------------------------------
