The Mesa 3D Graphics Library

# Mesa 18.1.4 Release Notes / July 13 2018

Mesa 18.1.4 is a bug fix release which fixes bugs found since the 18.1.3 release.

Mesa 18.1.4 implements the OpenGL 4.5 API, but the version reported by glGetString(GL_VERSION) or glGetIntegerv(GL_MAJOR_VERSION) / glGetIntegerv(GL_MINOR_VERSION) depends on the particular driver being used. Some drivers don't support all the features required in OpenGL 4.5. OpenGL 4.5 is only available if requested at context creation. Compatibility contexts may report a lower version depending on each driver.

## SHA256 checksums

    SHA256: 8acd42e4ac4d1e96ed22344073b3d4fef03d10f225f4eaf3f88c001dfc10e2db  mesa-18.1.4.tar.gz
    SHA256: 3061488b5d85504092cf4343816cfb2d96f2ad9bc2edec31fc96933d184cf58b  mesa-18.1.4.tar.xz

## New features

None

## Bug fixes

- Bug 106906 - Failed to recongnize keyword “sampler2DRect” and "sampler2DRectShadow"
- Bug 106928 - When starting a match Rocket League crashes on "Go"
- Bug 107193 - piglit.spec.arb_compute_shader.linker.bug-93840 fails

## Changes

Adam Jackson (1):

- glx: Don't allow glXMakeContextCurrent() with only one valid drawable

Dave Airlie (1):

- r600/sb: cleanup if_conversion iterator to be legal C++

Dylan Baker (2):

- docs: Add SHA256 sums to notes for 18.1.3
- Bump version for release

Iago Toral Quiroga (3):

- anv/cmd_buffer: make descriptors dirty when emitting base state address
- anv/cmd_buffer: clean dirty push constants flag after emitting push constants
- anv/cmd_buffer: never shrink the push constant buffer size

Ian Romanick (4):

- i965/vec4: Don't cmod propagate from CMP to ADD if the writemask isn't compatible
- intel/compiler: Relax mixed type restriction for saturating immediates
- i965/vec4: Properly handle sign(-abs(x))
- i965/fs: Properly handle sign(-abs(x))

Jason Ekstrand (3):

- intel/fs: Split instructions low to high in lower_simd_width
- anv: Be more careful about hashing pipeline layouts
- intel/fs: Mark LINTERP opcode as writing accumulator on platforms without PLN

Jose Maria Casanova Crespo (3):

- i965/fs: Register allocator shoudn't use grf127 for sends dest
- intel/compiler: grf127 can not be dest when src and dest overlap in send
- i965/fs: unspills shoudn't use grf127 as dest since Gen8+

Lionel Landwerlin (1):

- i965: fix clear color bo address relocation

Marek Olšák (3):

- radeonsi: fix memory exhaustion issue with DCC statistics gathering with DRI2
- glsl/cache: save and restore ExternalSamplersUsed
- st/dri: fix a crash in server_wait_sync

Neil Roberts (1):

- i965: Fix output register sizes when variable ranges are interleaved

Rhys Perry (1):

- nvc0/ir: fix TargetNVC0::insnCanLoadOffset()

Roland Scheidegger (1):

- r600/sb: fix crash in fold_alu_op3

Ross Burton (1):

- egl: fix build race in automake

Samuel Pitoiset (1):

- radv: fix emitting the view index on GFX9

Timothy Arceri (2):

- glsl: skip comparison opt when adding vars of different size
- nir: fix selection of loop terminator when two or more have the same limit

zhaowei yuan (1):

- glsl: Treat sampler2DRect and sampler2DRectShadow as reserved in ES2