# RUN: llvm-mc --disassemble %s -triple=x86_64-apple-darwin9 |& grep {invalid instruction encoding}

# This instruction would decode as movmskps if the vvvv field in the VEX prefix was all 1s.
0xc5 0xf0 0x50 0xc0
