title: Heat Conduction in 1D

The 1D heat conduction is configured by choosing the equation name to be
"heat_1d".
It takes one parameter, the heat conductivity "k".
The initial condition has to be provided for the temperature.
An example is provided with a [sinus distribution](sinus_temperature).
