Basic operations
Put or delete chips

- Select the chip from WAV list, and put it on the score
- Delete a chip
- Changing guide margin
- Put chip on the back channel

# Select the chip from WAV list, and put it on the score

(1) Go to the edit mode.()

(2) Select the chip you'd like to put from the WAV list.

(3) Left click on the score to put the chip.

# Delete a chip

In the edit mode(), Right click the chip to delete it.

In the select mode(), select the chips by dragging and push Del key to delete them.

# Changing guide margin

Change "Guide margin" to change the division of the bar to arrange chips

> Guide margin = 1/4 Guide margin 1/32

# Put chip on the back channel

Ctrl + Left click to put a chip onto the back channel. The chip on the back channel has a little shorter width.

### Remarks

- About the back channel, see also [Lane].