Advanced operations
Search

Click [Edit(E)] - [Find(F)] in the menubar to open Find dialog.

> Lane select
> Chip range
> Select from front chips
> Selrct from back chips
> Bar range

Specify the search conditions and click [Find]. The chips that satisfy conditions are selected.

## Lane select

If you want to limit the target lanes, check it.
And check the lane you'd like to use as target lanes. Click [All] to select all lanes. Click [None] to cancel all lanes.

## Chip range

To specify the range of chip number to search.
Specify "from" and "to" number. Both numbers are 36-decimal expression (01-ZZ). If you specify one of them, the chips would be specified which has that chip number. If you don't specify both of them, all ranges (01-ZZ) would be specified.

## Select from front chips

Check it if you want to select only front chips.

## Select from back chips

Check it if you want to select only back chips.

## Bar range

Specify bar ranges where you want to select.
Bar number should be 000-Z99 (the hundred's digit should be 0-9 and A-Z, and the ten's digit and the one's digit should be 0-9). If you specify one of them, the chips would be specified in that bar. If you don't specify both of them, all ranges (000-Z99) would be specified.