# mrcImageCircumferentialProjection

## Usage

    Usage: mrcImageCircumferentialProjection
    Options:
        [-i[nput]            In                  (NULL      )] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      )] :Essential :OutputDataFile
        [-dang               dang                (10        )] :Optional  :Delta Angle[degree]
        [-zmin               zmin                (0         )] :Optional  :Z Minimum[A]
        [-zmax               zmax                (100       )] :Optional  :Z Maximum[A]
        [-dz                 dz                  (10        )] :Optional  :Delta Z[A]
        [-rmin               rmin                (0         )] :Optional  :Radius Minimum[A]
        [-rmax               rmax                (200       )] :Optional  :Radius Maximum[A]
        [-threshold          threshold           (0         )] :Optional  :Set threshold value.  Averaged density is more than threshold value
        [-dr                 dr                  (10        )] :Optional  :Delta Radius[A]
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         )] :Optional  :Mode
    ----- Additional Usage -----
    x --> r
    y --> z
    --------- mode ---------
    0: Out Put Averaged Density (dataSum = dataSum / nang)
    1: Out Put Added    Density (dataSum = dataSum / nang *(2*PI*r))
    2: Out Put Averaged Density more than threshold (dataSum = dataSum / [nang number more than threshold value] *(2*PI*r))