# mrcImageFourierShellCorrelation

## Usage

    Usage: mrcImageFourierShellCorrelation
    Options:
        [-i1[input1]         In1                 (NULL      )] :Optional  :InputDataFile
        [-i2[input2]         In2                 (NULL      )] :Optional  :InputDataFile
        [-d[elta]            delta               (0         )] :Optional  :Interval of output data(1/A). Default 1/(Nx*size of pixel)
        [-z[position]        z                   (0         )] :Optional  :z position of reference file to correlate.For mode2=1 only
        [-L[owThreshold]     L                   (0         )] :Optional  :Low threshold for mode +2.
        [-H[ighThreshold]    H                   (0         )] :Optional  :High threshold for mode +2.
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         )] :Optional  :Mode
        [-M[ode2]            mode2               (0         )] :Optional  :Mode2
        [-I1[nput array of file]In1Array            (stdin     )] :Optional  :InputDataFiles
    ----- mode -----
    0: Fourier shell correlation.
    1: Fourier shell phase residual.
    +2: Correlation between L and H
    +4: Without equator.
    ----- mode 2 -----
    0: Correlation between same size images
    1: Correlation between 2D image and image extracted from 3D image.
    +2: Correlation between 2D different size images. In1 is compared with center of In2.