# mrcSinogramFETcalcSDforNormalize

## Usage

    Usage: mrcSinogramFETcalcSDforNormalize
    Options:
        [-i[nput]            In                  (NULL      )] :Optional  :InputFETDataFile
        [-s[elect]           Sm                  (1         )] :Optional  :selectFETfile
        [-l[ibrary]          Libl                (NULL      )] :Essential :SDlibraryFile
        [-o[utput]           Out                 (NULL      )] :Optional  :OutputSDdataFile
        [-o[ut]w[eight]      OW                  (NULL      )] :Optional  :OutputWeightdataFile
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         )] :Optional  :Mode
    ----- Additional Usage -----
    mode 0: SDfile writeout from liblary file
            Library(option -l) is Essential
    ow : weightfile writeout from liblary file when mode 0
    mode 1: to overwrite data library
            Essential options are: -sm, -i, -l
            if you want to make new data library,
            you have to make 2Dmrc-format pre-library file using tool "array2mrc"
            Array:  x=(number of feature + 1), y=6, z=0, data: all 0.0
    sm : 0 is noise-free refarence FETdata,
         1 is no-smoothing FET data
         17 or any other number is smoothed FET data