# mrcImageGaussSphere

## Usage

    Usage: mrcImageGaussSphere
    Options:
        [-o[utput]           Out                 (NULL      )] :Essential :OutputDataFile
        [-E[uler]A[ngle]     EA                  (YOYS      )Rot1                (0.0       )Rot2                (0.0       )Rot3                (0.0       )] :Optional  :Input: Gauss Sphere: Rotation
        [-centre             ShiftX              (0.0       )ShiftY              (0.0       )ShiftZ              (0.0       )] :Optional  :Input: Gauss Sphere: Centre
        [-sigmax             sigmax              (10        )] :Optional  :sigmax[A]
        [-sigmay             sigmay              (20        )] :Optional  :sigmay[A]
        [-sigmaz             sigmaz              (30        )] :Optional  :sigmaz[A]
        [-sigma_range        sigma_range         (3         )] :Optional  :x times
        [-weight             weight              (10        )] :Optional  :weight
        [-size               size                (5         )] :Optional  :Pixel Size[A]
        [-W[idth]            Width               (0         )] :Optional  :Width[A]
        [-H[ight]            Height              (0         )] :Optional  :Height[A]
        [-S[ection]          Section             (0         )] :Optional  :Section[A]
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (2         )] :Optional  :Mode
    Gauss Sphere is cutted at sigma_range*sigma
    Gauss Sphere = weight * exp ( - ((x^2 / sigmax^2)+(y^2 / sigmay^2)+(z^2 / sigmaz^2))
    mrcImageFileSize is (sigma_range*sigmax*2) x (sigma_range*sigmay*2) x (sigma_range*sigmaz*2)
    -----------------------------------------------------------------------------------
    -EA: for rotation
    -----------------------------------------------------------------------------------
    mode 0 char
    mode 2 float