# mrcSinogramFETnormalizedMap

## Usage

    Usage: mrcSinogramFETnormalizedMap
    Options:
        [-i[nput]            In                  (NULL      )] :Essential :InputFETlistFile
        [-o[utput]           OutFET              (NULL      )] :Essential :OutputFETmrcformat
        [-cl[ine]List        comList             (NULL      )] :Optional  :commonlineList
        [-O[utput]           OutMAP              (NULL      )] :Optional  :OutputMAPmrcformat
        [-w[eight]           Weight              (NULL      )] :Optional  :WeightForDistanceCalc
        [-atm[ode]           AAtm                (1         )] :Optional  :AAtestmode
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         )] :Optional  :Mode
    ----- Additional Usage -----
     "-O" option do not work at Oct.24,2007
     aatestmode 0: default, check whole distance
                1: check about all features
    mode 0: normal 1: PCA (Nov.1,2007)