# mrcImageDensityChangeEstimation

## Usage

    Usage: mrcImageDensityChangeEstimation
    Options:
        [-i[nput]            In                  (NULL      )] :Essential :Input: mrcImage
        [-i[nput]2           In2                 (NULL      )] :Essential :Input: mrcImage2
        [-o[utput]           Out                 (stdout    )] :Optional  :OutputDataFile
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         )] :Optional  :Mode
    ----- Additional Usage -----
    ----- Attention !!!-----
    In Eos system, positive values are regarded as density.
    If a pixel has a negative value, the value of the pixel is regarded as zero.lmrcImageDensityChangeEstimation Mode:
    2: CentreOfGravity
    4: Max
    8: SD around CentreOfGravity
    16: SD around Max