# mrcImageROI3D

## Usage

    Usage: mrcImageROI3D
    Options:
        [-i[nput]            In                  (NULL      )] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      )] :Essential :OutputDataFile
        [-x                  x1                  (0.0       )x2                  (0.0       )] :Optional  :from x1[pixel] to x2[pixel]
        [-y                  y1                  (0.0       )y2                  (0.0       )] :Optional  :from y1[pixel] to y2[pixel]
        [-z                  z1                  (0.0       )z2                  (0.0       )] :Optional  :from z1[pixel] to z2[pixel]
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         )] :Optional  :Mode
    ----- Additional Usage -----
    from z1 to z2