# llDataMultiCTFCompensation

## Usage

    Usage: llDataMultiCTFCompensation
    Options:
        [-i[nput]            In                  (NULL      )] :Essential :Input: FileList
        [-M[odel]            Ref                 (NULL      )] :Essential :Input: Model Data
        [-l[ayerLine]        llInfo              (NULL      )] :Essential :Input: Layer Line Information
        [-A[verageFile]      Ave                 (NULL      )] :Essential :Output: AverageFile
        [-o[utput]           OutParam            (NULL      )] :Optional  :Output: FittedParameter
        [-O[utput]           Out                 (NULL      )] :Optional  :Output: FileList:  PhaseShift of Each Filament
        [-o2[utput]          OutParam2           (NULL      )] :Optional  :Output: [phi, z] map
        [-P2[output]         OutParamP2          (NULL      )] :Optional  :Output: For P-P'
        [-N[oise]            Noise               (0.0       )] :Optional  :Noise Ratio
        [-t[ruePitch]        truePitch           (761.4     )] :Essential :truePitch[A]
        [-d[eltaR]           deltaR              (1.0       )] :Optional  :deltaR[A]
        [-r[adial]           rmin                (1.0       )rmax                (1.0       )dr                  (1.0       )] :Optional  :Radial[Ratio]
        [-p[hi]              phimin              (0.0       )phimax              (180.0     )dphi                (1.0       )] :Optional  :Phi [degree]
        [-z[shift]           zmin                (0.0       )zmax                (180.0     )dz                  (1.0       )] :Optional  :z [A]
        [-Rmax               Rmax                (0.1       )] :Optional  :Rmax [/A]
        [-MaxIter[ation]     MaxIter             (1         )] :Optional  :MaxIteration
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         )] :Optional  :Mode
    ---- InputFileFormat ----
    filename weight(NumberOfAveragedFile) deltaF[A] Cs[mm] kV[kV] ratioOfAmpToPhase
    ----- Mode -----
        0: |CTFi|/Sigma(SQR(CTFi))
        1:  CTFi /Sigma(SQR(CTFi))