# mrcImageRectangleGetByCorrelation

## Usage

    Usage: mrcImageRectangleGetByCorrelation
    Options:
        [-i[nput]            In                  (NULL      )] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      )] :Essential :OutputDataFile
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-r[eference]        Ref                 (NULL      )] :Optional  :ReferenceFile
        [-Nx[Number of x]    Nx                  (0         )] :Optional  :Nx:Default If Nx of inputfile is even Nx ,else Nx-1
        [-Ny[Number of y]    Ny                  (0         )] :Optional  :Ny:Default If Ny of inputfile is even Ny ,else Ny-1
        [-m[ode]             mode                (0         )] :Optional  :Mode
    ----- Additional Usage -----