# mrcImageSquare

## Usage

    Usage: mrcImageSquare
    Options:
        [-i[nput]            In                  (NULL      )] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      )] :Essential :OutputDataFile
        [-eps                eps                 (1e-15     )] :Optional  :Epsilon to consider zero. For mode 1 only
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         )] :Optional  :Mode
    ----- Additional Usage -----
    mode 0: Square
    mode 1: Square Root