# mrcFTMeridianEquatorRedece

## Usage

    Usage: mrcFTMeridianEquatorRedece
    Options:
        [-i[nput]            In                  (NULL      )] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      )] :Essential :OutputDataFile
        [-X                  MaxX                (-1        )] :Optional  :Max X to put zero (pixel).  Default is no operation.
        [-Y                  MaxY                (-1        )] :Optional  :Max Y to put zero (pixel).  Default is no operation.
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         )] :Optional  :Mode
    ----- Additional Usage -----