# mrcImageConnectivityNumberCalc

## Usage

    Usage: mrcImageConnectivityNumberCalc
    Options:
        [-i[nput]            In                  (NULL      )] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      )] :Essential :OutputDataFile
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         )] :Optional  :Mode
        [-f[orm]             form                (0         )] :Optional  :Form
        [-I[nvers]           invers              (0         )] :Optional  :Invers
    ----- Additional Usage -----
    mode   0 : Four Neighborhood. [default] : For 2 Dimension.
           1 : Eight Nieghborhood.          :
           2 : Eighteen Neighborhood.       : For 3 Dimension.

    form   0 : No change. [default]
           1 : Spread of pixel data 1.
           2 : Thin of pixel data 1.
           3 : Frame of image by data 1.

    invers 0 : The object is 1 value. [default]
           1 : The background is 1 value.