# mrcFETnormalizeBySD

## Usage

    Usage: mrcFETnormalizeBySD
    Options:
        [-i[nput]            In                  (NULL      )] :Essential :InputFileList
        [-i[nput]s[ample]    InSample            (NULL      )] :Optional  :FileListforSDcalc
        [-r[ead]SD           readSD              (NULL      )] :Optional  :readFETSDfile
        [-w[rite]SD          writeSD             (NULL      )] :Optional  :writeFETSDfile
        [-o[utput]           Out                 (NULL      )] :Optional  :OutputASmrcImage
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         )] :Optional  :Mode

    ----- Additional Usage -----
    -is  :[inputsample] is FileList for SDcalculation.
               use when the inputFileList is large
    -rSD : to use SDdata(without calculate) mrc format
    -wSD : write out the SDdata as mrc format
           this file can be used next normalize with "-rSD"command.
    -o   : save all normalized data into one mrcImage.
           do not use when the inputFileList is large