# eosPointRotation

## Usage

    Usage: eosPointRotation
    Options:
        [-i[nput]            In                  (stdin     ).as(inFile::ASCII       ) ] :Optional  :Input: eosPoint
        [-i[nput]t[ype]      InType              (3         ).as(Integer             ) ] :Optional  :Input: eosPointType
        [-o[utput]           Out                 (stdout    ).as(outFile::ASCII      ) ] :Optional  :Output: eosPoint
        [-o[utput]t[ype]     OutType             (3         ).as(Integer             ) ] :Optional  :Input: eosPointType
        [-E[uler]A[ngle]     EAMode              (YOYS      ).as(String              )
                             Rot1                (0.0       ).as(Real                )
                             Rot2                (0.0       ).as(Real                )
                             Rot3                (0.0       ).as(Real                ) ] :Optional  :Input: EulerAngleMode Rot1 Rot2 Rot3
        [-I[nput]            InList              (NULL      ).as(inFileList::ASCII   ) ] :Optional  :Input:  eosPointFileList
        [-O[uput]            OutList             (NULL      ).as(outFileList::ASCII  ) ] :Optional  :Output: eosPointFileList
        [-c[onfig]           configFile          (NULL      ).as(inFile              ) ] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         ).as(Integer             ) ] :Optional  :Mode
    ----- Additional Usage -----