# mrcImageStandardDeviation

## Usage

    Usage: mrcImageStandardDeviation
    Options:
        [-i[nput]            In                  (NULL      )] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      )] :Optional  :OutputDataFile
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-h[ighThreshold]    Hth                 (0         )] :Optional  :High threshold. Mode2=0 only.
        [-l[ow threshold]    Lth                 (0         )] :Optional  :Low threshold. Mode2=0 only.
        [-m[ode]             mode                (0         )] :Optional  :Mode
        [-M[ode2]            mode2               (0         )] :Optional  :Mode2
    ----- Additional Usage -----
    Input file is a list of mrc files.
    mode 0: Standard deviation
    mode 1: Variation
    mode2 0: Standard deviation or Variation in one mrcfile.
    mode2 1: Standard deviation or Variation of each pixel between mrcfiles.