# mrcImageSectionGet

## Usage

    Usage: mrcImageSectionGet
    Options:
        [-i[nput]            In                  (NULL      )] :Essential :InputDataFile
        [-o[utput]           Out                 (NULL      )] :Essential :OutputDataFile
        [-z                  z                   (0         )] :Optional  :z-Section number
        [-c[onfig]           configFile          (NULL      )] :Optional  :ConfigurationFile
        [-m[ode]             mode                (0         )] :Optional  :Mode
    ----- Additional Usage -----
    mode 0: Copy the selected section into a new area indicated by dst
    mode 1: Share the selected section between dst and src: replacement of pointers