### JJY Receivers

#### Synopsis

Address: 127.127.40.u
Reference ID: `JJY`
Driver ID: `JJY`
Serial Port: `/dev/jjyu`; 9600 baud, 8-bits, no parity, 1 stop bit

#### Description

This driver supports the following JJY receivers sold in Japan.

- Tristate Ltd. JJY01 http://www.tristate.ne.jp/rf-clock.htm (Japanese only)
  Time code format

  Command | Reply
  `date<CR><LF>` | `YYYY/MM/DD WWW<CR><LF>`
  `stim<CR><LF>` | `HH:MM:SS<CR><LF>`

- C-DEX Co.,Ltd. JST2000 http://www.c-dex.co.jp/ (Japanese only)
  Time code format

  Command | Reply
  `<ENQ>1J<ETX>` | `<STX>JYYMMDD HHMMSSS<ETX>`

JJY is the radio station which transmites the JST (Japan Standard Time) in long wave radio. The station JJY is operated by the Communication Research Laboratory. An operating announcement and some information are avaiable from http://www.crl.go.jp/ (English and Japanese)http://jjy.crl.go.jp/ (Written in Japanese only

The user is expected to provide a symbolic link to an available serial port device. This is typically performed by a command such as:

`ln -s /dev/ttyS0 /dev/jjy0`

Windows NT does not support symbolic links to device files. COMX: is the unit used by the driver, based on the refclock unit number, where unit 1 corresponds to COM1: and unit 3 corresponds to COM3:

#### Monitor Data

The driver writes each timecode as received to the `clockstats` file.

#### Fudge Factors

`time1 time`
  Specifies the time offset calibration factor, in seconds and fraction, with default 0.0.
`time2 time`
  Not used by this driver.
`stratum number`
  Specifies the driver stratum, in decimal from 0 to 15, with default 0.
`refid string`
  Specifies the driver reference identifier, an ASCII string from one to four characters, with default `WWVB`.
`flag1 0 | 1`
  Not used by this driver.
`flag2 0 | 1`
  Not used by this driver.
`flag3 0 | 1`
  Not used by this driver.
`flag4 0 | 1`
  Enable verbose `clockstats` recording if set.