## View and Operations

### Heatmap & 3D Display

#### Heatmap

Heatmap plots m/z on the X-axis and RT on the Y-axis and displays the different intensity levels using color difference.

##### Heatmap Zoom

1. Left-click at one end of the range in the heatmap and drag diagonally to the other end.

2. Release the left button.

   - Right-click in the heatmap to go back to the previous image.

Note:

- The 3D View of the same sample will also change to the scale used in the Heatmap View.