Overview | Package | Class | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

# Constant Field Values

Contents

- java.io.*
- java.lang.*
- javax.microedition.*
- lejos.devices.*
- lejos.nxt.*
- lejos.rcxcomm.*

java.io.*

java.io.File
`public static final byte` | `MAX_FILES` | `30`

java.lang.*

java.lang.Integer
`public static final int` | `MAX_RADIX` | `36`
`public static final int` | `MAX_VALUE` | `2147483647`
`public static final int` | `MIN_RADIX` | `2`
`public static final int` | `MIN_VALUE` | `-2147483648`

java.lang.Math
`public static final double` | `E` | `2.718281828459045`
`public static final double` | `NaN` | `0d/0d`
`public static final double` | `PI` | `3.141592653589793`

java.lang.Thread
`public static final int` | `MAX_PRIORITY` | `10`
`public static final int` | `MIN_PRIORITY` | `1`
`public static final int` | `NORM_PRIORITY` | `5`

javax.microedition.*

javax.microedition.lcdui.Alert
`public static final int` | `ALERT_TYPE_ALARM` | `3`
`public static final int` | `ALERT_TYPE_CONFIRMATION` | `4`
`public static final int` | `ALERT_TYPE_ERROR` | `2`
`public static final int` | `ALERT_TYPE_INFO` | `0`
`public static final int` | `ALERT_TYPE_WARNING` | `1`
`public static final int` | `FOREVER` | `-2`
`public static final String` | `STR_CONFIRM` | `"Yes"`
`public static final String` | `STR_DENY` | `"No"`

javax.microedition.lcdui.Choice
`public static final int` | `EXCLUSIVE` | `1`
`public static final int` | `IMPLICIT` | `3`
`public static final int` | `MULTIPLE` | `2`
`public static final int` | `POPUP` | `4`
`public static final int` | `TEXT_WRAP_DEFAULT` | `0`
`public static final int` | `TEXT_WRAP_OFF` | `2`
`public static final int` | `TEXT_WRAP_ON` | `1`

javax.microedition.lcdui.Command
`public static final int` | `BACK` | `2`
`public static final int` | `CANCEL` | `3`
`public static final int` | `EXIT` | `7`
`public static final int` | `HELP` | `5`
`public static final int` | `ITEM` | `8`
`public static final int` | `OK` | `4`
`public static final int` | `SCREEN` | `1`
`public static final int` | `STOP` | `6`

javax.microedition.lcdui.Display
`public static final int` | `CHAR_HEIGHT` | `8`
`public static final int` | `CHAR_WIDTH` | `6`
`public static final int` | `SCREEN_CHAR_DEPTH` | `8`
`public static final int` | `SCREEN_CHAR_WIDTH` | `16`
`public static final int` | `SCREEN_HEIGHT` | `64`
`public static final int` | `SCREEN_WIDTH` | `100`

javax.microedition.lcdui.Displayable
`public static final int` | `KEY_BACK` | `40`
`public static final int` | `KEY_ENTER` | `38`
`public static final int` | `KEY_LEFT` | `37`
`public static final int` | `KEY_RIGHT` | `39`

javax.microedition.lcdui.Graphics
`public static final int` | `BLACK` | `1`
`public static final int` | `DOTTED` | `2`
`public static final int` | `SOLID` | `0`
`public static final int` | `WHITE` | `0`

javax.microedition.lcdui.TextField
`public static final int` | `ANY` | `1`
`public static final int` | `DECIMAL` | `6`
`public static final int` | `EMAILADDR` | `2`
`public static final int` | `INITIAL_CAPS_SENTENCE` | `1536`
`public static final int` | `INITIAL_CAPS_WORD` | `1280`
`public static final int` | `NON_PREDICTIVE` | `1024`
`public static final int` | `NUMERIC` | `3`
`public static final int` | `PASSWORD` | `256`
`public static final int` | `PHONENUMBER` | `4`
`public static final int` | `SENSITIVE` | `768`
`public static final int` | `UNEDITABLE` | `512`
`public static final int` | `URL` | `5`

lejos.devices.*

lejos.devices.KeyEvent
`public static final int` | `ALT_DOWN_MASK` | `512`
`public static final int` | `ALT_GRAPH_DOWN_MASK` | `8192`
`public static final int` | `ALT_GRAPH_MASK` | `32`
`public static final int` | `ALT_MASK` | `8`
`public static final int` | `CTRL_DOWN_MASK` | `128`
`public static final int` | `CTRL_MASK` | `2`
`public static final int` | `META_DOWN_MASK` | `256`
`public static final int` | `META_MASK` | `4`
`public static final int` | `SHIFT_DOWN_MASK` | `64`
`public static final int` | `SHIFT_MASK` | `1`
`public static final int` | `VK_DOWN` | `40`
`public static final int` | `VK_LEFT` | `37`
`public static final int` | `VK_RIGHT` | `39`
`public static final int` | `VK_UP` | `38`

lejos.nxt.*

lejos.nxt.BasicMotorPort
`public static final int` | `PWM_BRAKE` | `1`
`public static final int` | `PWM_FLOAT` | `0`

lejos.nxt.Button
`public static final String` | `VOL_SETTING` | `"lejos.keyclick_volume"`

lejos.nxt.Flash
`public static final int` | `MAX_USER_PAGES` | `704`

lejos.nxt.LCD
`public static final int` | `CELL_HEIGHT` | `8`
`public static final int` | `CELL_WIDTH` | `6`
`public static final int` | `DISPLAY_CHAR_DEPTH` | `8`
`public static final int` | `DISPLAY_CHAR_WIDTH` | `16`
`public static final int` | `DISPLAY_DEPTH` | `8`
`public static final int` | `DISPLAY_WIDTH` | `100`
`public static final int` | `FONT_HEIGHT` | `8`
`public static final int` | `FONT_WIDTH` | `5`
`public static final int` | `NOOF_CHARS` | `128`
`public static final int` | `ROP_AND` | `-16777216`
`public static final int` | `ROP_ANDINVERTED` | `-65536`
`public static final int` | `ROP_ANDREVERSE` | `-16711936`
`public static final int` | `ROP_CLEAR` | `0`
`public static final int` | `ROP_COPY` | `65280`
`public static final int` | `ROP_COPYINVERTED` | `65535`
`public static final int` | `ROP_EQUIV` | `16777215`
`public static final int` | `ROP_INVERT` | `16711935`
`public static final int` | `ROP_NAND` | `-16776961`
`public static final int` | `ROP_NOOP` | `16711680`
`public static final int` | `ROP_NOR` | `-1`
`public static final int` | `ROP_OR` | `-256`
`public static final int` | `ROP_ORINVERTED` | `-16711681`
`public static final int` | `ROP_ORREVERSE` | `-65281`
`public static final int` | `ROP_SET` | `255`
`public static final int` | `ROP_XOR` | `16776960`
`public static final int` | `SCREEN_HEIGHT` | `64`
`public static final int` | `SCREEN_WIDTH` | `100`

lejos.nxt.NXTe
`public static final byte` | `NXTE_ADDRESS` | `40`

lejos.nxt.OpticalDistanceSensor
`public static final byte` | `CUSTOM` | `53`
`public static final byte` | `GP2D12` | `49`
`public static final byte` | `GP2D120` | `50`
`public static final byte` | `GP2YA02` | `52`
`public static final byte` | `GP2YA21` | `51`

lejos.nxt.Poll
`public static final short` | `ALL_BUTTONS` | `240`
`public static final short` | `ALL_SENSORS` | `15`
`public static final short` | `BUTTON_MASK_SHIFT` | `4`
`public static final short` | `ENTER_MASK` | `16`
`public static final short` | `ESCAPE_MASK` | `128`
`public static final short` | `LEFT_MASK` | `32`
`public static final short` | `RIGHT_MASK` | `64`
`public static final short` | `SENSOR1_MASK` | `1`
`public static final short` | `SENSOR2_MASK` | `2`
`public static final short` | `SENSOR3_MASK` | `4`
`public static final short` | `SENSOR4_MASK` | `8`
`public static final short` | `SERIAL_MASK` | `256`
`public static final short` | `SERIAL_SHIFT` | `8`

lejos.nxt.RCXLink
`public static final byte` | `BEEP` | `57`
`public static final int` | `DELAY` | `10`
`public static final int` | `EEPROM_BUFFER` | `120`
`public static final byte` | `LONG_RANGE_IR` | `4`
`public static final byte` | `MOTOR_A_FORWARD` | `33`
`public static final byte` | `MOTOR_A_REVERSED` | `37`
`public static final byte` | `MOTOR_B_FORWARD` | `41`
`public static final byte` | `MOTOR_B_REVERSED` | `45`
`public static final byte` | `MOTOR_C_FORWARD` | `49`
`public static final byte` | `MOTOR_C_REVERSED` | `53`
`public static final byte` | `POWER_OFF_RCX` | `7`
`public static final byte` | `RUN_PROGRAM_1` | `9`
`public static final byte` | `RUN_PROGRAM_2` | `13`
`public static final byte` | `RUN_PROGRAM_3` | `17`
`public static final byte` | `RUN_PROGRAM_4` | `21`
`public static final byte` | `RUN_PROGRAM_5` | `25`
`public static final byte` | `SHORT_RANGE_IR` | `1`
`public static final byte` | `STOP_ALL_PROGRAMS` | `29`

lejos.nxt.SensorConstants
`public static final int` | `MODE_ANGLESTEP` | `224`
`public static final int` | `MODE_BOOLEAN` | `32`
`public static final int` | `MODE_CELSIUS` | `160`
`public static final int` | `MODE_FARENHEIT` | `192`
`public static final int` | `MODE_PCTFULLSCALE` | `128`
`public static final int` | `MODE_PERIODCOUNTER` | `96`
`public static final int` | `MODE_RAW` | `0`
`public static final int` | `MODE_TRANSITIONCNT` | `64`
`public static final int` | `TYPE_ANGLE` | `4`
`public static final int` | `TYPE_CUSTOM` | `9`
`public static final int` | `TYPE_LIGHT_ACTIVE` | `5`
`public static final int` | `TYPE_LIGHT_INACTIVE` | `6`
`public static final int` | `TYPE_LOWSPEED` | `10`
`public static final int` | `TYPE_LOWSPEED_9V` | `11`
`public static final int` | `TYPE_NO_SENSOR` | `0`
`public static final int` | `TYPE_REFLECTION` | `3`
`public static final int` | `TYPE_SOUND_DB` | `7`
`public static final int` | `TYPE_SOUND_DBA` | `8`
`public static final int` | `TYPE_SWITCH` | `1`
`public static final int` | `TYPE_TEMPERATURE` | `2`

lejos.nxt.Sound
`public static final int` | `VOL_MAX` | `100`
`public static final String` | `VOL_SETTING` | `"lejos.volume"`

lejos.nxt.comm.Bluetooth
`public static final byte` | `BT_PENDING_INPUT` | `1`
`public static final byte` | `BT_PENDING_OUTPUT` | `2`
`public static final byte` | `MSG_ACCEPT_CONNECTION` | `9`
`public static final byte` | `MSG_ADD_DEVICE` | `5`
`public static final byte` | `MSG_ANY` | `-1`
`public static final byte` | `MSG_BEGIN_INQUIRY` | `0`
`public static final byte` | `MSG_CANCEL_INQUIRY` | `1`
`public static final byte` | `MSG_CLOSE_CONNECTION` | `8`
`public static final byte` | `MSG_CLOSE_CONNECTION_RESULT` | `26`
`public static final byte` | `MSG_CLOSE_PORT` | `29`
`public static final byte` | `MSG_CLOSE_PORT_RESULT` | `30`
`public static final byte` | `MSG_CONNECT` | `2`
`public static final byte` | `MSG_CONNECT_RESULT` | `19`
`public static final byte` | `MSG_CONNECTION_STATUS_RESULT` | `57`
`public static final byte` | `MSG_DUMP_LIST` | `7`
`public static final byte` | `MSG_GET_BRICK_STATUSBYTE` | `51`
`public static final byte` | `MSG_GET_BRICK_STATUSBYTE_RESULT` | `49`
`public static final byte` | `MSG_GET_CONNECTION_STATUS` | `56`
`public static final byte` | `MSG_GET_DISCOVERABLE` | `42`
`public static final byte` | `MSG_GET_DISCOVERABLE_RESULT` | `45`
`public static final byte` | `MSG_GET_FRIENDLY_NAME` | `41`
`public static final byte` | `MSG_GET_FRIENDLY_NAME_RESULT` | `44`
`public static final byte` | `MSG_GET_LINK_QUALITY` | `35`
`public static final byte` | `MSG_GET_LOCAL_ADDR` | `39`
`public static final byte` | `MSG_GET_LOCAL_ADDR_RESULT` | `40`
`public static final byte` | `MSG_GET_OPERATING_MODE` | `53`
`public static final byte` | `MSG_GET_PORT_OPEN` | `43`
`public static final byte` | `MSG_GET_PORT_OPEN_RESULT` | `46`
`public static final byte` | `MSG_GET_VERSION` | `47`
`public static final byte` | `MSG_GET_VERSION_RESULT` | `48`
`public static final byte` | `MSG_GOTO_DFU_MODE` | `58`
`public static final byte` | `MSG_HEARTBEAT` | `13`
`public static final byte` | `MSG_INQUIRY_RESULT` | `15`
`public static final byte` | `MSG_INQUIRY_RUNNING` | `14`
`public static final byte` | `MSG_INQUIRY_STOPPED` | `16`
`public static final byte` | `MSG_LINK_QUALITY_RESULT` | `36`
`public static final byte` | `MSG_LIST_DUMP_STOPPED` | `25`
`public static final byte` | `MSG_LIST_ITEM` | `24`
`public static final byte` | `MSG_LIST_RESULT` | `23`
`public static final byte` | `MSG_LOOKUP_NAME` | `4`
`public static final byte` | `MSG_LOOKUP_NAME_FAILURE` | `18`
`public static final byte` | `MSG_LOOKUP_NAME_RESULT` | `17`
`public static final byte` | `MSG_OPEN_PORT` | `3`
`public static final byte` | `MSG_OPEN_STREAM` | `11`
`public static final byte` | `MSG_OPERATING_MODE_RESULT` | `55`
`public static final byte` | `MSG_PIN_CODE` | `10`
`public static final byte` | `MSG_PIN_CODE_ACK` | `31`
`public static final byte` | `MSG_PORT_OPEN_RESULT` | `27`
`public static final byte` | `MSG_REMOVE_DEVICE` | `6`
`public static final byte` | `MSG_REQUEST_CONNECTION` | `22`
`public static final byte` | `MSG_REQUEST_PIN_CODE` | `21`
`public static final byte` | `MSG_RESET_INDICATION` | `20`
`public static final byte` | `MSG_SET_BRICK_STATUSBYTE` | `52`
`public static final byte` | `MSG_SET_BRICK_STATUSBYTE_RESULT` | `50`
`public static final byte` | `MSG_SET_DISCOVERABLE` | `28`
`public static final byte` | `MSG_SET_DISCOVERABLE_ACK` | `32`
`public static final byte` | `MSG_SET_FACTORY_SETTINGS` | `37`
`public static final byte` | `MSG_SET_FACTORY_SETTINGS_ACK` | `38`
`public static final byte` | `MSG_SET_FRIENDLY_NAME` | `33`
`public static final byte` | `MSG_SET_FRIENDLY_NAME_ACK` | `34`
`public static final byte` | `MSG_SET_OPERATING_MODE` | `54`
`public static final byte` | `MSG_START_HEART` | `12`

lejos.nxt.comm.BTConnection
`public static final int` | `AM_ALWAYS` | `1`
`public static final int` | `AM_DISABLE` | `0`
`public static final int` | `AM_OUTPUT` | `2`

lejos.nxt.comm.LCP
`public static final byte` | `BOOT` | `-105`
`public static final byte` | `CLOSE` | `-124`
`public static final byte` | `DELETE` | `-123`
`public static final byte` | `DELETE_USER_FLASH` | `-96`
`public static final byte` | `DIRECTORY_FULL` | `-4`
`public static final byte` | `FILE_NOT_FOUND` | `-122`
`public static final byte` | `FIND_FIRST` | `-122`
`public static final byte` | `FIND_NEXT` | `-121`
`public static final byte` | `GET_BATTERY_LEVEL` | `11`
`public static final byte` | `GET_CURRENT_PROGRAM_NAME` | `17`
`public static final byte` | `GET_DEVICE_INFO` | `-101`
`public static final byte` | `GET_FIRMWARE_VERSION` | `-120`
`public static final byte` | `GET_INPUT_VALUES` | `7`
`public static final byte` | `GET_OUTPUT_STATE` | `6`
`public static final byte` | `INSUFFICIENT_MEMORY` | `-5`
`public static final byte` | `KEEP_ALIVE` | `13`
`public static final byte` | `LS_GET_STATUS` | `14`
`public static final byte` | `LS_READ` | `16`
`public static final byte` | `LS_WRITE` | `15`
`public static final byte` | `MAILBOX_EMPTY` | `64`
`public static final byte` | `MESSAGE_READ` | `19`
`public static final byte` | `MESSAGE_WRITE` | `9`
`public static final byte` | `NOT_IMPLEMENTED` | `-3`
`public static final byte` | `NXJ_FIND_FIRST` | `-74`
`public static final byte` | `NXJ_FIND_NEXT` | `-73`
`public static final byte` | `OPEN_APPEND_DATA` | `-116`
`public static final byte` | `OPEN_READ` | `-128`
`public static final byte` | `OPEN_READ_LINEAR` | `-118`
`public static final byte` | `OPEN_WRITE` | `-127`
`public static final byte` | `OPEN_WRITE_DATA` | `-117`
`public static final byte` | `OPEN_WRITE_LINEAR` | `-119`
`public static final byte` | `PLAY_SOUND_FILE` | `2`
`public static final byte` | `PLAY_TONE` | `3`
`public static final byte` | `POLL` | `-94`
`public static final byte` | `POLL_LENGTH` | `-95`
`public static final byte` | `READ` | `-126`
`public static final byte` | `RESET_MOTOR_POSITION` | `10`
`public static final byte` | `RESET_SCALED_INPUT_VALUE` | `8`
`public static final byte` | `SET_BRICK_NAME` | `-104`
`public static final byte` | `SET_INPUT_MODE` | `5`
`public static final byte` | `SET_OUTPUT_STATE` | `4`
`public static final byte` | `START_PROGRAM` | `0`
`public static final byte` | `STOP_PROGRAM` | `1`
`public static final byte` | `STOP_SOUND_PLAYBACK` | `12`
`public static final byte` | `UNDEFINED_ERROR` | `-118`
`public static final byte` | `WRITE` | `-125`

lejos.nxt.comm.NXTProtocol
`public static final byte` | `ANGLE` | `4`
`public static final byte` | `ANGLESTEPSMODE` | `-32`
`public static final byte` | `BOOLEANMODE` | `32`
`public static final byte` | `BOOT` | `-105`
`public static final byte` | `BRAKE` | `2`
`public static final byte` | `CELSIUSMODE` | `-96`
`public static final byte` | `CLOSE` | `-124`
`public static final byte` | `CUSTOM` | `9`
`public static final byte` | `DELETE` | `-123`
`public static final byte` | `DELETE_USER_FLASH` | `-96`
`public static final byte` | `DIRECT_COMMAND_NOREPLY` | `-128`
`public static final byte` | `DIRECT_COMMAND_REPLY` | `0`
`public static final byte` | `FAHRENHEITMODE` | `-64`
`public static final byte` | `FIND_FIRST` | `-122`
`public static final byte` | `FIND_NEXT` | `-121`
`public static final byte` | `GET_BATTERY_LEVEL` | `11`
`public static final byte` | `GET_CURRENT_PROGRAM_NAME` | `17`
`public static final byte` | `GET_DEVICE_INFO` | `-101`
`public static final byte` | `GET_FIRMWARE_VERSION` | `-120`
`public static final byte` | `GET_INPUT_VALUES` | `7`
`public static final byte` | `GET_OUTPUT_STATE` | `6`
`public static final byte` | `HIGH_SPEED_BUFFER` | `1`
`public static final byte` | `KEEP_ALIVE` | `13`
`public static final byte` | `LIGHT_ACTIVE` | `5`
`public static final byte` | `LIGHT_INACTIVE` | `6`
`public static final byte` | `LOWSPEED` | `10`
`public static final byte` | `LOWSPEED_9V` | `11`
`public static final byte` | `LS_GET_STATUS` | `14`
`public static final byte` | `LS_READ` | `16`
`public static final byte` | `LS_WRITE` | `15`
`public static final byte` | `MESSAGE_READ` | `19`
`public static final byte` | `MESSAGE_WRITE` | `9`
`public static final byte` | `MODEMASK` | `-32`
`public static final byte` | `MOTOR_RUN_STATE_IDLE` | `0`
`public static final byte` | `MOTOR_RUN_STATE_RAMPDOWN` | `64`
`public static final byte` | `MOTOR_RUN_STATE_RAMPUP` | `16`
`public static final byte` | `MOTOR_RUN_STATE_RUNNING` | `32`
`public static final byte` | `MOTORON` | `1`
`public static final byte` | `NO_OF_SENSOR_TYPES` | `12`
`public static final byte` | `NO_SENSOR` | `0`
`public static final byte` | `OPEN_APPEND_DATA` | `-116`
`public static final byte` | `OPEN_READ` | `-128`
`public static final byte` | `OPEN_READ_LINEAR` | `-118`
`public static final byte` | `OPEN_WRITE` | `-127`
`public static final byte` | `OPEN_WRITE_DATA` | `-117`
`public static final byte` | `OPEN_WRITE_LINEAR` | `-119`
`public static final byte` | `PCTFULLSCALEMODE` | `-128`
`public static final byte` | `PERIODCOUNTERMODE` | `96`
`public static final byte` | `PLAY_SOUND_FILE` | `2`
`public static final byte` | `PLAY_TONE` | `3`
`public static final byte` | `POLL` | `-94`
`public static final byte` | `POLL_BUFFER` | `0`
`public static final byte` | `POLL_LENGTH` | `-95`
`public static final byte` | `RAWMODE` | `0`
`public static final byte` | `READ` | `-126`
`public static final byte` | `REFLECTION` | `3`
`public static final byte` | `REGULATED` | `4`
`public static final byte` | `REGULATION_MODE_IDLE` | `0`
`public static final byte` | `REGULATION_MODE_MOTOR_SPEED` | `1`
`public static final byte` | `REGULATION_MODE_MOTOR_SYNC` | `2`
`public static final byte` | `REPLY_COMMAND` | `2`
`public static final byte` | `RESET_MOTOR_POSITION` | `10`
`public static final byte` | `RESET_SCALED_INPUT_VALUE` | `8`
`public static final byte` | `SET_BRICK_NAME` | `-104`
`public static final byte` | `SET_INPUT_MODE` | `5`
`public static final byte` | `SET_OUTPUT_STATE` | `4`
`public static final byte` | `SLOPEMASK` | `31`
`public static final byte` | `SOUND_DB` | `7`
`public static final byte` | `SOUND_DBA` | `8`
`public static final byte` | `START_PROGRAM` | `0`
`public static final byte` | `STOP_PROGRAM` | `1`
`public static final byte` | `STOP_SOUND_PLAYBACK` | `12`
`public static final byte` | `SWITCH` | `1`
`public static final byte` | `SYSTEM_COMMAND_NOREPLY` | `-127`
`public static final byte` | `SYSTEM_COMMAND_REPLY` | `1`
`public static final byte` | `TEMPERATURE` | `2`
`public static final byte` | `TRANSITIONCNTMODE` | `64`
`public static final byte` | `WRITE` | `-125`

lejos.nxt.comm.USB
`public static final String` | `NAME` | `"lejos.usb_name"`
`public static final int` | `RAW` | `536870912`
`public static final int` | `RESET` | `1073741824`
`public static final String` | `SERIAL_NO` | `"lejos.usb_serno"`

lejos.nxt.debug.DebugInterface
`public static final int` | `DBG_EVENT_DISABLE` | `0`
`public static final int` | `DBG_EVENT_ENABLE` | `1`
`public static final int` | `DBG_EVENT_IGNORE` | `2`
`public static final int` | `DBG_EXCEPTION` | `1`
`public static final int` | `DBG_USER_INTERRUPT` | `2`

lejos.rcxcomm.*

lejos.rcxcomm.Opcode
`public static final byte` | `OPCODE_ABSOLUTE_VALUE` | `116`
`public static final byte` | `OPCODE_ABSOLUTE_VALUE_REPLY` | `-125`
`public static final byte` | `OPCODE_ADD_TO_VARIABLE` | `36`
`public static final byte` | `OPCODE_ADD_TO_VARIABLE_REPLY` | `-45`
`public static final byte` | `OPCODE_ALIVE` | `16`
`public static final byte` | `OPCODE_ALIVE_REPLY` | `-25`
`public static final byte` | `OPCODE_AND_VARIABLE` | `-124`
`public static final byte` | `OPCODE_AND_VARIABLE_REPLY` | `115`
`public static final byte` | `OPCODE_BRANCH_ALWAYS_FAR` | `114`
`public static final byte` | `OPCODE_BRANCH_ALWAYS_NEAR` | `39`
`public static final byte` | `OPCODE_CALL_SUBROUTINE` | `23`
`public static final byte` | `OPCODE_CLEAR_MESSAGE` | `-112`
`public static final byte` | `OPCODE_CLEAR_SENSOR_VALUE` | `-47`
`public static final byte` | `OPCODE_CLEAR_SENSOR_VALUE_REPLY` | `38`
`public static final byte` | `OPCODE_CLEAR_TIMER` | `-95`
`public static final byte` | `OPCODE_CLEAR_TIMER_REPLY` | `86`
`public static final byte` | `OPCODE_DATALOG_NEXT` | `98`
`public static final byte` | `OPCODE_DATALOG_NEXT_REPLY` | `-107`
`public static final byte` | `OPCODE_DECREMENT_LOOP_COUNTER_FAR` | `-110`
`public static final byte` | `OPCODE_DECREMENT_LOOP_COUNTER_NEAR` | `55`
`public static final byte` | `OPCODE_DELETE_ALL_SUBROUTINES` | `112`
`public static final byte` | `OPCODE_DELETE_ALL_SUBROUTINES_REPLY` | `-121`
`public static final byte` | `OPCODE_DELETE_ALL_TASKS` | `64`
`public static final byte` | `OPCODE_DELETE_ALL_TASKS_REPLY` | `-73`
`public static final byte` | `OPCODE_DELETE_FIRMWARE` | `101`
`public static final byte` | `OPCODE_DELETE_FIRMWARE_REPLY` | `-110`
`public static final byte` | `OPCODE_DELETE_SUBROUTINE` | `-63`
`public static final byte` | `OPCODE_DELETE_SUBROUTINE_REPLY` | `54`
`public static final byte` | `OPCODE_DELETE_TASK` | `97`
`public static final byte` | `OPCODE_DELETE_TASK_REPLY` | `-106`
`public static final byte` | `OPCODE_DIVIDE_VARIABLE` | `68`
`public static final byte` | `OPCODE_DIVIDE_VARIABLE_REPLY` | `-77`
`public static final byte` | `OPCODE_GET_BATTERY_POWER` | `48`
`public static final byte` | `OPCODE_GET_BATTERY_POWER_REPLY` | `-57`
`public static final byte` | `OPCODE_GET_MEMORY_MAP` | `32`
`public static final byte` | `OPCODE_GET_MEMORY_MAP_REPLY` | `-41`
`public static final byte` | `OPCODE_GET_VALUE` | `18`
`public static final byte` | `OPCODE_GET_VALUE_REPLY` | `-27`
`public static final byte` | `OPCODE_GET_VERSIONS` | `21`
`public static final byte` | `OPCODE_GET_VERSIONS_REPLY` | `-30`
`public static final byte` | `OPCODE_MASK` | `-9`
`public static final byte` | `OPCODE_MULTIPLY_VARIABLE` | `84`
`public static final byte` | `OPCODE_MULTIPLY_VARIABLE_REPLY` | `-93`
`public static final byte` | `OPCODE_OR_VARIABLE` | `-108`
`public static final byte` | `OPCODE_OR_VARIABLE_REPLY` | `99`
`public static final byte` | `OPCODE_PLAY_SOUND_REPLY` | `-90`
`public static final byte` | `OPCODE_PLAY_TONE` | `35`
`public static final byte` | `OPCODE_PLAY_TONE_REPLY` | `-44`
`public static final byte` | `OPCODE_POWER_OFF` | `96`
`public static final byte` | `OPCODE_POWER_OFF_REPLY` | `-105`
`public static final byte` | `OPCODE_REMOTE_COMMAND` | `-46`
`public static final byte` | `OPCODE_SEND_MESSAGE` | `-78`
`public static final byte` | `OPCODE_SET_DATALOG_SIZE` | `82`
`public static final byte` | `OPCODE_SET_DATALOG_SIZE_REPLY` | `-91`
`public static final byte` | `OPCODE_SET_DISPLAY` | `51`
`public static final byte` | `OPCODE_SET_DISPLAY_REPLY` | `-60`
`public static final byte` | `OPCODE_SET_LOOP_COUNTER` | `-126`
`public static final byte` | `OPCODE_SET_MESSAGE` | `-9`
`public static final byte` | `OPCODE_SET_MOTOR_DIRECTION` | `-31`
`public static final byte` | `OPCODE_SET_MOTOR_DIRECTION_REPLY` | `22`
`public static final byte` | `OPCODE_SET_MOTOR_ON_OFF` | `33`
`public static final byte` | `OPCODE_SET_MOTOR_ON_OFF_REPLY` | `-42`
`public static final byte` | `OPCODE_SET_MOTOR_POWER` | `19`
`public static final byte` | `OPCODE_SET_MOTOR_POWER_REPLY` | `-28`
`public static final byte` | `OPCODE_SET_POWER_DOWN_DELAY` | `-79`
`public static final byte` | `OPCODE_SET_POWER_DOWN_DELAY_REPLY` | `70`
`public static final byte` | `OPCODE_SET_PROGRAM_NUMBER` | `-111`
`public static final byte` | `OPCODE_SET_PROGRAM_NUMBER_REPLY` | `102`
`public static final byte` | `OPCODE_SET_SENSOR_MODE` | `66`
`public static final byte` | `OPCODE_SET_SENSOR_MODE_REPLY` | `-75`
`public static final byte` | `OPCODE_SET_SENSOR_TYPE` | `50`
`public static final byte` | `OPCODE_SET_SENSOR_TYPE_REPLY` | `-59`
`public static final byte` | `OPCODE_SET_TIME` | `34`
`public static final byte` | `OPCODE_SET_TIME_REPLY` | `-43`
`public static final byte` | `OPCODE_SET_TRANSMITTER_RANGE` | `49`
`public static final byte` | `OPCODE_SET_TRANSMITTER_RANGE_REPLY` | `-58`
`public static final byte` | `OPCODE_SET_VARIABLE` | `20`
`public static final byte` | `OPCODE_SET_VARIABLE_REPLY` | `-29`
`public static final byte` | `OPCODE_SIGN_VARIABLE` | `100`
`public static final byte` | `OPCODE_SIGN_VARIABLE_REPLY` | `-109`
`public static final byte` | `OPCODE_START_FIRMWARE_DOWNLOAD` | `117`
`public static final byte` | `OPCODE_START_FIRMWARE_DOWNLOAD_REPLY` | `-126`
`public static final byte` | `OPCODE_START_SUBROUTINE_DOWNLOAD` | `53`
`public static final byte` | `OPCODE_START_SUBROUTINE_DOWNLOAD_REPLY` | `-62`
`public static final byte` | `OPCODE_START_TASK` | `113`
`public static final byte` | `OPCODE_START_TASK_DOWNLOAD` | `37`
`public static final byte` | `OPCODE_START_TASK_DOWNLOAD_REPLY` | `-46`
`public static final byte` | `OPCODE_START_TASK_REPLY` | `-122`
`public static final byte` | `OPCODE_STOP_ALL_TASKS` | `80`
`public static final byte` | `OPCODE_STOP_ALL_TASKS_REPLY` | `-89`
`public static final byte` | `OPCODE_STOP_TASK` | `-127`
`public static final byte` | `OPCODE_STOP_TASK_REPLY` | `118`
`public static final byte` | `OPCODE_SUBTRACT_FROM_VARIABLE` | `52`
`public static final byte` | `OPCODE_SUBTRACT_FROM_VARIABLE_REPLY` | `-61`
`public static final byte` | `OPCODE_TEST_AND_BRANCH_FAR` | `-107`
`public static final byte` | `OPCODE_TEST_AND_BRANCH_NEAR` | `-123`
`public static final byte` | `OPCODE_TRANSFER_DATA` | `69`
`public static final byte` | `OPCODE_TRANSFER_DATA_REPLY` | `-78`
`public static final byte` | `OPCODE_UNLOCK_FIRMWARE` | `-91`
`public static final byte` | `OPCODE_UNLOCK_FIRMWARE_REPLY` | `82`
`public static final byte` | `OPCODE_UPLOAD_DATALOG` | `-92`
`public static final byte` | `OPCODE_UPLOAD_DATALOG_REPLY` | `83`
`public static final byte` | `OPCODE_WAIT` | `67`

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES