Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## lejos.nxt
Interface ADSensorPort

All Superinterfaces:
  BasicSensorPort, SensorConstants

All Known Subinterfaces:
  LegacySensorPort

All Known Implementing Classes:
  RemoteSensorPort, SensorPort

    public interface ADSensorPort

extends BasicSensorPort

An abstraction for a port that supports Analog/Digital sensors.

Author:
  Lawrie Griffiths

Field Summary

Fields inherited from interface lejos.nxt.SensorConstants
`MODE_ANGLESTEP, MODE_BOOLEAN, MODE_CELSIUS, MODE_FARENHEIT, MODE_PCTFULLSCALE, MODE_PERIODCOUNTER, MODE_RAW, MODE_TRANSITIONCNT, TYPE_ANGLE, TYPE_CUSTOM, TYPE_LIGHT_ACTIVE, TYPE_LIGHT_INACTIVE, TYPE_LOWSPEED, TYPE_LOWSPEED_9V, TYPE_NO_SENSOR, TYPE_REFLECTION, TYPE_SOUND_DB, TYPE_SOUND_DBA, TYPE_SWITCH, TYPE_TEMPERATURE`

Method Summary
`boolean` | `readBooleanValue()`
`int` | `readRawValue()`
`int` | `readValue()`

Methods inherited from interface lejos.nxt.BasicSensorPort
`getMode, getType, setMode, setType, setTypeAndMode`

Method Detail

### readBooleanValue

    boolean readBooleanValue()

### readRawValue

    int readRawValue()

### readValue

    int readValue()

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD