Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD

## lejos.nxt
Interface LegacySensorPort

All Superinterfaces:
  ADSensorPort, BasicSensorPort, SensorConstants

All Known Implementing Classes:
  SensorPort

    public interface LegacySensorPort

extends ADSensorPort

Abstraction for a port that supports legacy RCX sensors.

Author:
  Lawrie Griffiths

Field Summary

Fields inherited from interface lejos.nxt.SensorConstants
`MODE_ANGLESTEP, MODE_BOOLEAN, MODE_CELSIUS, MODE_FARENHEIT, MODE_PCTFULLSCALE, MODE_PERIODCOUNTER, MODE_RAW, MODE_TRANSITIONCNT, TYPE_ANGLE, TYPE_CUSTOM, TYPE_LIGHT_ACTIVE, TYPE_LIGHT_INACTIVE, TYPE_LOWSPEED, TYPE_LOWSPEED_9V, TYPE_NO_SENSOR, TYPE_REFLECTION, TYPE_SOUND_DB, TYPE_SOUND_DBA, TYPE_SWITCH, TYPE_TEMPERATURE`

Method Summary
`void` | `activate()`
`void` | `passivate()`

Methods inherited from interface lejos.nxt.ADSensorPort
`readBooleanValue, readRawValue, readValue`

Methods inherited from interface lejos.nxt.BasicSensorPort
`getMode, getType, setMode, setType, setTypeAndMode`

Method Detail

### activate

    void activate()

### passivate

    void passivate()

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV CLASS NEXT CLASS | FRAMES NO FRAMES
SUMMARY: NESTED | FIELD | CONSTR | METHOD | DETAIL: FIELD | CONSTR | METHOD