
 (as)sign <user><pass>[<port>]  :assign current shell to user with
                                 password and optional new receiver port
                                 
 (ch)ec(k) [(f)iles|(s)ystem|   :checks the orbiter installation, the active
            (t)ime|(v)ersion|    solar system, the current MJD, the server
            (v)e(s)sels|<name>|  version, the available vessels, lists
            (l)ocation [<id>]|   information about the given name or ID,
            (g)bodies ]          lists the available location(s) and lists
                                 available celestial objects
                                 
 echo [on|off]                  :start/stop echoing on TCP-channel
 
 GINFO <ID><1><2><3>            :provide info for ID - only info for hosted
                                 IDs will be accepted from a client
                                 
 ip [<address>]                 :set active IP to address or displays
                                 current and remote address
                                 
 (j)oi(n) <user><port><password>:join user on port with password
 
 (l)ea(v)e <user><password>     :leave user with password
 
 (l)i(s)t [(a)ll|(o)wn|         :lists information about all or own users or
           (c)urrent|<name> ]    objects, objects or users of the current or
          [(u)sers|(ob)jects]    named objects in optional detailed or plain
          [   (d)etailed    ]    form

 (n)ic(k) [<name>]              :sets/clears the nickname of current shell
 
 (obs)erve [off] [<ID>]         :observe the vessel with ID, turn it off or
                                 display current observations
                                 
 (pr)ompt <Format>              :sets the prompt format for broadcasts, with
                                 {0} being the message as string and {1} the
                                 server UTC as datetime - example IRC-like:
                                 "({1:HH:mm:ss}) {0}"
                                           
 quit|exit                      :stop TCP-channel
 
 RADIO:<message>                :transmit string as is to every client
 
 REQST <ID>                     :request info for the vessel with ID
 
 (t)alk:<message> | me:<message>:transmit message to every client
 
 (tr)ac(k) [off] [<ID>]         :track the vessel with ID, turn tracking off
                                 or display current trackings
                                 
***** ADMINISTRATORS ONLY *************** ADMINISTRATORS ONLY ****************

 (d)ump [(gl)obals|             :lists global ID, connection or client hash
         (c)o(n)nections|        content as well as some hash statistics,
         (cl)ients|              lists log entries starting with <time> and
         ((l)og <chars>          <chars> per dump step or the last <chars> on
          [last|<time>]) ]       every dump step ('dump' w/o arguments)
                                 
 kick <ip>                      :closes all TCP connections from the
                                 specified IP address
                                 
 kickban [off] [<ip>]           :kicks the specified IP and adds it to the ban
                                 list, or remove the IP from the list if used
                                 with "off" - no argument will display the
                                 list
                                 
 log cut                        :switches current logging file to next part
                                 (serverX.log with X>0)
                                 DISFUNCTIONAL
                                 
 log [<flags>]                  :set logging levels according to flags
                                 (-=none S=screen F=file B=both) or displays
                                 the current logging level status
                                 DISFUNCTIONAL
                                 
 mjd (st)atus                   :displays timestamp and MJD
 mjd (r)eset <date><time><ack>  :calculates MJD with given date and time -
                                 if ack's first character is Yy1, this MJD
                                 will be set as current, else displayed only
                                 
 sync reset|status|data         :resets the synchronization flag, displays
                                 SNTP server status or displays clock hard-
                                 ware information