--- rest25/library/sunaudio.rst	2008-12-19 16:58:07.000000000 +0900
+++ rest262/library/sunaudio.rst	2009-04-05 05:02:09.000000000 +0900
@@ -1,19 +1,24 @@
 
 :mod:`sunaudiodev` --- Access to Sun audio hardware
 ===================================================
 
 .. module:: sunaudiodev
    :platform: SunOS
    :synopsis: Access to Sun audio hardware.
+   :deprecated:
+
+.. deprecated:: 2.6
+   The :mod:`sunaudiodev` module has been deprecated for removal in Python 3.0.
+
 
 
 .. index:: single: u-LAW
 
 This module allows you to access the Sun audio interface. The Sun audio hardware
 is capable of recording and playing back audio data in u-LAW format with a
 sample rate of 8K per second. A full description can be found in the
 :manpage:`audio(7I)` manual page.
 
 .. index:: module: SUNAUDIODEV
 
 The module :mod:`SUNAUDIODEV`  defines constants which may be used with this
@@ -136,21 +141,26 @@
    import fcntl, signal, STROPTS
 
    signal.signal(signal.SIGPOLL, handle_sigpoll)
    fcntl.ioctl(audio_obj.fileno(), STROPTS.I_SETSIG, STROPTS.S_MSG)
 
 
 :mod:`SUNAUDIODEV` --- Constants used with :mod:`sunaudiodev`
 =============================================================
 
 .. module:: SUNAUDIODEV
    :platform: SunOS
    :synopsis: Constants for use with sunaudiodev.
+   :deprecated:
+
+.. deprecated:: 2.6
+   The :mod:`SUNAUDIODEV` module has been deprecated for removal in Python 3.0.
+
 
 
 .. index:: module: sunaudiodev
 
 This is a companion module to :mod:`sunaudiodev` which defines useful symbolic
 constants like :const:`MIN_GAIN`, :const:`MAX_GAIN`, :const:`SPEAKER`, etc. The
 names of the constants are the same names as used in the C include file
 ``<sun/audioio.h>``, with the leading string ``AUDIO_`` stripped.
 
