Palm Tungsten|E PDA (``cheetah``)
=================================

The Palm Tungsten|E PDA (codename \"Cheetah\") emulation includes the
following elements:

-  Texas Instruments OMAP310 System-on-chip (ARM925T core)

-  ROM and RAM memories (ROM firmware image can be loaded with
   -option-rom)

-  On-chip LCD controller

-  On-chip Real Time Clock

-  TI TSC2102i touchscreen controller / analog-digital converter /
   Audio CODEC, connected through MicroWire and |I2S| busses

-  GPIO-connected matrix keypad

-  Secure Digital card connected to OMAP MMC/SD host

-  Three on-chip UARTs
