Raspberry Pi boards (``raspi0``, ``raspi1ap``, ``raspi2b``, ``raspi3ap``, ``raspi3b``)
======================================================================================


QEMU provides models of the following Raspberry Pi boards:

``raspi0`` and ``raspi1ap``
  ARM1176JZF-S core, 512 MiB of RAM
``raspi2b``
  Cortex-A7 (4 cores), 1 GiB of RAM
``raspi3ap``
  Cortex-A53 (4 cores), 512 MiB of RAM
``raspi3b``
  Cortex-A53 (4 cores), 1 GiB of RAM


Implemented devices
-------------------

 * ARM1176JZF-S, Cortex-A7 or Cortex-A53 CPU
 * Interrupt controller
 * DMA controller
 * Clock and reset controller (CPRMAN)
 * System Timer
 * GPIO controller
 * Serial ports (BCM2835 AUX - 16550 based - and PL011)
 * Random Number Generator (RNG)
 * Frame Buffer
 * USB host (USBH)
 * GPIO controller
 * SD/MMC host controller
 * SoC thermal sensor
 * USB2 host controller (DWC2 and MPHI)
 * MailBox controller (MBOX)
 * VideoCore firmware (property)


Missing devices
---------------

 * Peripheral SPI controller (SPI)
 * Analog to Digital Converter (ADC)
 * Pulse Width Modulation (PWM)
