This driver is functional and has been tested on EdgeRouter Lite with
USB mass storage.

TODO:
	- kernel coding style
	- checkpatch warnings
	- dead code elimination
	- device tree bindings
	- possibly eliminate the extra "hardware abstraction layer"

Contact: Aaro Koskinen <aaro.koskinen@iki.fi>
