This tests reception (decryption) of ESP-3DES-MD5 packets with a source 
of encrypted ICMP packets. The SA directs that the packets should be 
received on the mast0 device, instead of the default ipsec0 device.
