Starting UML PATH/start.sh
spawn PATH single
Linux version XXXX
On node 0 totalpages: 8192
Kernel command line:
Calibrating delay loop... XXXX bogomips
Dentry-cache hash table entries: NUMBERS
Inode-cache hash table entries: NUMBERS
Mount-cache hash table entries: NUMBERS
Buffer-cache hash table entries: NUMBERS
Page-cache hash table entries: NUMEBRS
POSIX conformance testing by UNIFIX
Linux NET4.0 for Linux 2.4
Based upon Swansea University Computer Society NET3.039
Initializing RT netlink socket
Starting kswapd
VFS: Diskquotas version dquot_6.4.0 initialized
devfs: VERSION Richard Gooch (rgooch@atnf.csiro.au)
devfs: boot_options Q
pty: 256 Unix98 ptys configured
SLIP: version 0.8.4-NET3.019-NEWTTY (dynamic channels, max=256).
loop: loaded (max 8 devices)
PPP generic driver version VERSION
Universal TUN/TAP device driver VERSION

NET4: Linux TCP/IP 1.0 for NET4.0
IP Protocols: ICMP, UDP, TCP
IP: routing cache hash table of 512 buckets, 4Kbytes
TCP: Hash tables configured (established 2048 bind 2048)
IPv4 over IPv4 tunneling driver
GRE over IPv4 tunneling driver
NET4: Unix domain sockets 1.0/SMP for Linux NET4.0.
Mounted devfs on /dev
INIT: version 2.78 booting
Activating swap...
Calculating module dependancies
done.
Loading modules: LIST

Checking all file systems...
Parallelizing fsck version 1.18 (11-Nov-1999)
Setting kernel variables.
Mounting local filesystems...
/dev/shm on /tmp type tmpfs (rw)
/dev/shm on /var/run type tmpfs (rw)
devpts on /dev/pts type devpts (rw,mode=0622)
none on /usr/share type hostfs (ro)
Enabling packet forwarding: done.
Configuring network interfaces: done.
Cleaning: /tmp /var/lock /var/run.
Initializing random number generator... done.
Recovering nvi editor sessions... done.
Give root password for maintenance
(or type Control-D for normal startup): 
east:~#
 klogd -c 4 -x -f /tmp/klog.log
east:~#
 ipsec spi --clear
east:~#
 ipsec eroute --clear
east:~#
 enckey=0x4043434545464649494a4a4c4c4f4f515152525454575758
east:~#
 authkey=0x87658765876587658765876587658765
east:~#
 lifetime="--life hard-bytes=800"
east:~#
 ipsec spi --af inet --edst 192.1.2.45 --spi 0x12345678 --proto esp --src 192.1.2.23 --esp 3des-md5-96 $lifetime --enckey $enckey --authkey $authkey
east:~#
 ipsec spi --af inet --edst 192.1.2.45 --spi 0x12345678 --proto tun --src 192.1.2.23 --dst 192.1.2.45 --ip4
east:~#
 ipsec spigrp inet 192.1.2.45 0x12345678 tun inet 192.1.2.45 0x12345678 esp 
east:~#
 ipsec eroute --add --eraf inet --src 192.0.2.0/24 --dst 192.0.1.0/24 --said tun0x12345678@192.1.2.45
east:~#
 ipsec tncfg --attach --virtual ipsec0 --physical eth1
east:~#
 ifconfig ipsec0 inet 192.1.2.23 netmask 0xffffff00 broadcast 192.1.2.255 up
east:~#
 arp -s 192.1.2.45 10:00:00:64:64:45
east:~#
 arp -s 192.1.2.254 10:00:00:64:64:45
east:~#
 ipsec look
east NOW
192.0.2.0/24       -> 192.0.1.0/24       => tun0x12345678@192.1.2.45 esp0x12345678@192.1.2.45  (0)
ipsec0->eth1 mtu=16260(1500)->1500
esp0x12345678@192.1.2.45 ESP_3DES_HMAC_MD5: dir=out src=192.1.2.23 iv_bits=64bits iv=0xDEADF00DDEADF00D alen=128 aklen=128 eklen=192 life(c,s,h)=bytes(0,0,800) natencap=none natsport=0 natdport=0 refcount=4 ref=2
tun0x12345678@192.1.2.45 IPIP: dir=out src=192.1.2.23 life(c,s,h)= natencap=none natsport=0 natdport=0 refcount=4 ref=3
ROUTING TABLE
east:~#
 route add -host 192.0.1.1 gw 192.1.2.45 dev ipsec0
east:~#
 mkdir -p /var/run/pluto
east:~#
 ipsec pf_key --daemon /var/run/pluto/pf_key.pid >/tmp/pfkey.txt
east:~#
 echo send packets
send packets
east:~#
 kill `cat /var/run/pluto/pf_key.pid`
east:~#
 cat /tmp/pfkey.txt; echo ===

pfkey v2 msg. type=7(register) seq=1 len=5 pid=987 errno=0 satype=2(AH)
version=2 type=7 errno=0 satype=2 len=5 seq=1 pid=987 {ext=14 len=3 bytes=0x000000000300a000a00000000200800080000000 } 

pfkey v2 msg. type=7(register) seq=2 len=9 pid=987 errno=0 satype=3(ESP)
version=2 type=7 errno=0 satype=3 len=9 seq=2 pid=987 {ext=14 len=4 bytes=0x0000000009008000800000000300a000a00000000200800080000000 } {ext=15 len=3 bytes=0x000000000c808000000100000340a800a8000000 } 

pfkey v2 msg. type=7(register) seq=3 len=4 pid=987 errno=0 satype=9(IPIP)
version=2 type=7 errno=0 satype=9 len=4 seq=3 pid=987 {ext=15 len=2 bytes=0x000000000100200020000000 } 

pfkey v2 msg. type=7(register) seq=4 len=4 pid=987 errno=0 satype=10(COMP)
version=2 type=7 errno=0 satype=10 len=4 seq=4 pid=987 {ext=15 len=2 bytes=0x000000000200010001000000 } 

pfkey v2 msg. type=8(expire) seq=1 len=21 pid=987 errno=0 satype=3(ESP)
version=2 type=8 errno=0 satype=3 len=21 seq=1 pid=987 {ext=1 len=3 spi=78563412 replay=0 state=1 auth=2 encrypt=3 flags=00000000 ref=00000002}{ext=2 len=5 allocations=1 bytes=936 addtime=X usetime=X packets=3 } {ext=3 len=5 allocations=0 bytes=800 addtime=X usetime=X packets=0 } {ext=5 len=3 proto=0 prefixlen=0 addr=0x02000000c00102170000000000000000 } {ext=6 len=3 proto=0 prefixlen=0 addr=0x02000000c001022d0000000000000000 } 
pf_key: Exiting on signal 15
===
east:~#
 ipsec eroute
8          192.0.2.0/24       -> 192.0.1.0/24       => tun0x12345678@192.1.2.45
east:~#
 ipsec setup stop
IPSEC EVENT: KLIPS device ipsec0 shut down.
ipsec_setup: Stopping Openswan IPsec...
ipsec_setup: stop ordered, but IPsec appears to be already stopped!
ipsec_setup: doing cleanup anyway...
east:~#
 kill `cat /var/run/klogd.pid`; cat /tmp/klog.log
klogd 1.3-3#33.1, log source = /proc/kmsg started.
east:~#
 halt -p -f
Power down.

