Starting UML PATH/start.sh
spawn PATH single
Linux version XXXX
On node 0 totalpages: 8192
Kernel command line:
Calibrating delay loop... XXXX bogomips
Dentry-cache hash table entries: NUMBERS
Inode-cache hash table entries: NUMBERS
Mount-cache hash table entries: NUMBERS
Buffer-cache hash table entries: NUMBERS
Page-cache hash table entries: NUMEBRS
POSIX conformance testing by UNIFIX
Linux NET4.0 for Linux 2.4
Based upon Swansea University Computer Society NET3.039
Initializing RT netlink socket
Starting kswapd
VFS: Diskquotas version dquot_6.4.0 initialized
devfs: VERSION Richard Gooch (rgooch@atnf.csiro.au)
devfs: boot_options Q
pty: 256 Unix98 ptys configured
SLIP: version 0.8.4-NET3.019-NEWTTY (dynamic channels, max=256).
loop: loaded (max 8 devices)
PPP generic driver version VERSION
Universal TUN/TAP device driver VERSION

NET4: Linux TCP/IP 1.0 for NET4.0
IP Protocols: ICMP, UDP, TCP
IP: routing cache hash table of 512 buckets, 4Kbytes
TCP: Hash tables configured (established 2048 bind 2048)
IPv4 over IPv4 tunneling driver
GRE over IPv4 tunneling driver
NET4: Unix domain sockets 1.0/SMP for Linux NET4.0.
Mounted devfs on /dev
INIT: version 2.78 booting
Activating swap...
Calculating module dependancies
done.
Loading modules: LIST

Checking all file systems...
Parallelizing fsck version 1.18 (11-Nov-1999)
Setting kernel variables.
Mounting local filesystems...
/dev/shm on /tmp type tmpfs (rw)
/dev/shm on /var/run type tmpfs (rw)
devpts on /dev/pts type devpts (rw,mode=0622)
none on /usr/share type hostfs (ro)
Enabling packet forwarding: done.
Configuring network interfaces: done.
Cleaning: /tmp /var/lock /var/run.
Initializing random number generator... done.
Recovering nvi editor sessions... done.
Give root password for maintenance
(or type Control-D for normal startup): 
west:~#
 klogd -c 4 -x -f /tmp/klog.log
west:~#
 ping -n -c 4 192.0.2.254
PING 192.0.2.254 (192.0.2.254): 56 data bytes
64 bytes from 192.0.2.254: icmp_seq=0 ttl=257 time=999 ms
64 bytes from 192.0.2.254: icmp_seq=1 ttl=257 time=999 ms
64 bytes from 192.0.2.254: icmp_seq=2 ttl=257 time=999 ms
64 bytes from 192.0.2.254: icmp_seq=3 ttl=257 time=999 ms

--- 192.0.2.254 ping statistics ---
4 packets transmitted, 4 packets received, 0% packet loss
round-trip min/avg/max = 3.1/4.5/9.26 ms
west:~#
 iptables -A FORWARD -i eth1 -s 192.0.2.0/24 -j DROP
west:~#
 iptables -A INPUT -i eth1 -s 192.0.2.0/24 -j DROP
west:~#
 ping -n -c 4 192.0.2.254
PING 192.0.2.254 (192.0.2.254): 56 data bytes

--- 192.0.2.254 ping statistics ---
4 packets transmitted, 0 packets received, 100% packet loss
west:~#
 TESTNAME=dh1-pluto-01 
west:~#
 source /testing/pluto/bin/westlocal.sh
west:~#
 ipsec setup start
ipsec_setup: Starting Openswan IPsec VERSION
west:~#
 ipsec auto --add westnet-eastnet-weak
034 esp string error: found modp group id, but not supported, enc_alg="aes", auth_alg="sha1", modp="modp768"
west:~#
 /testing/pluto/basic-pluto-01/eroutewait.sh trap
west:~#
 ipsec auto --up  westnet-eastnet-weak
021 no connection named "westnet-eastnet-weak"
west:~#
 echo done
done
west:~#
 ipsec look
west NOW
0.0.0.0/0          -> 0.0.0.0/0          => %trap
ipsec0->eth1 mtu=16260(9999)->1500
Destination     Gateway         Genmask         Flags   MSS Window  irtt Iface
0.0.0.0         192.1.2.254     0.0.0.0         UG       99 0          0 eth1
0.0.0.0         192.1.2.254     128.0.0.0       UG       99 0          0 ipsec0
128.0.0.0       192.1.2.254     128.0.0.0       UG       99 0          0 ipsec0
192.0.2.0       192.1.2.23      255.255.255.0   UG       99 0          0 eth1
192.1.2.0       0.0.0.0         255.255.255.0   U        99 0          0 eth1
192.1.2.0       0.0.0.0         255.255.255.0   U        99 0          0 ipsec0
west:~#
 echo done
done
west:~#
 

west:~#
 ipsec look
west NOW
0.0.0.0/0          -> 0.0.0.0/0          => %trap
ipsec0->eth1 mtu=16260(9999)->1500
Destination     Gateway         Genmask         Flags   MSS Window  irtt Iface
0.0.0.0         192.1.2.254     0.0.0.0         UG       99 0          0 eth1
0.0.0.0         192.1.2.254     128.0.0.0       UG       99 0          0 ipsec0
128.0.0.0       192.1.2.254     128.0.0.0       UG       99 0          0 ipsec0
192.0.2.0       192.1.2.23      255.255.255.0   UG       99 0          0 eth1
192.1.2.0       0.0.0.0         255.255.255.0   U        99 0          0 eth1
192.1.2.0       0.0.0.0         255.255.255.0   U        99 0          0 ipsec0
west:~#
west:~#
 ipsec setup stop
IPSEC EVENT: KLIPS device ipsec0 shut down.
ipsec_setup: Stopping Openswan IPsec...
west:~#
 kill `cat /var/run/klogd.pid`; cat /tmp/klog.log
klogd 1.3-3#33.1, log source = /proc/kmsg started.
west:~#
 halt -p -f
Power down.

