Starting UML PATH/start.sh
spawn PATH single
Checking PROT_EXEC mmap in /tmp...OK
Linux version XXXX
Built 1 zonelists
Kernel command line:
PID hash table entries: 256 (order: 8, 4096 bytes)
Dentry-cache hash table entries: NUMBERS
Inode-cache hash table entries: NUMBERS
Mount-cache hash table entries: NUMBERS
Checking syscall emulation patch for ptrace...missing
NET: Registered protocol family 16
VFS: Diskquotas version dquot_6.4.0 initialized
Dquot-cache hash table entries: 1024 (order 0, 4096 bytes)
devfs: 2004-01-31 Richard Gooch (rgooch@atnf.csiro.au)
devfs: boot_options Q
io scheduler noop registered
io scheduler anticipatory registered
io scheduler deadline registered
io scheduler cfq registered
loop: loaded (max 8 devices)
nbd: registered device at major 43
PPP generic driver version VERSION
SLIP: version 0.8.4-NET3.019-NEWTTY (dynamic channels, max=256).
tun: Universal TUN/TAP device driver VERSION
tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>
NET: Registered protocol family 2
IP: routing cache hash table of 512 buckets, 4Kbytes
TCP established hash table entries: 2048 (order: 2, 16384 bytes)
TCP bind hash table entries: 2048 (order: 1, 8192 bytes)
TCP: Hash tables configured (established 2048 bind 2048)
NET: Registered protocol family 15
IPv4 over IPv4 tunneling driver
GRE over IPv4 tunneling driver
NET: Registered protocol family 1
NET: Registered protocol family 17
Initialized stdio console driver
Console initialized on /dev/tty0
Mounted devfs on /dev
line_ioctl: tty0: ioctl KDSIGACCEPT called
INIT: version 2.78 booting
Activating swap...
Checking all file systems...
Parallelizing fsck version 1.18 (11-Nov-1999)
Setting kernel variables.
Mounting local filesystems...
/dev/shm on /tmp type tmpfs (rw)
/dev/shm on /var/run type tmpfs (rw)
devpts on /dev/pts type devpts (rw,mode=0622)
none on /usr/share type hostfs (ro)
Enabling packet forwarding: done.
Configuring network interfaces: done.
Cleaning: /tmp /var/lock /var/run.
Initializing random number generator... done.
Recovering nvi editor sessions... done.
Give root password for maintenance
(or type Control-D for normal startup): 
north:~#
 klogd -c 4 -x -f /tmp/klog.log
north:~#
 TESTNAME=nat-dpd-pluto-01 
north:~#
 source /testing/pluto/bin/northlocal.sh
north:~#
 ipsec setup start
ipsec_setup: Starting Openswan IPsec VERSION
north:~#
 /testing/pluto/bin/wait-until-pluto-started
north:~#
 ipsec auto --add northnet--eastnet-nat
north:~#
 echo done
done
north:~#
 ipsec auto --up northnet--eastnet-nat
104 "northnet--eastnet-nat" #1: STATE_MAIN_I1: initiate
003 "northnet--eastnet-nat" #1: received Vendor ID payload [Openswan (this version) cvs2005Mar15_14:43:33  X.509-1.5.4 PLUTO_SENDS_VENDORID PLUTO_USES_KEYRR]
003 "northnet--eastnet-nat" #1: received Vendor ID payload [Dead Peer Detection]
003 "northnet--eastnet-nat" #1: received Vendor ID payload [RFC 3947] method set to=109 
106 "northnet--eastnet-nat" #1: STATE_MAIN_I2: sent MI2, expecting MR2
003 "northnet--eastnet-nat" #1: NAT-Traversal: Result using RFC 3947 (NAT-Traversal): i am NATed
108 "northnet--eastnet-nat" #1: STATE_MAIN_I3: sent MI3, expecting MR3
004 "northnet--eastnet-nat" #1: STATE_MAIN_I4: ISAKMP SA established
117 "northnet--eastnet-nat" #2: STATE_QUICK_I1: initiate
004 "northnet--eastnet-nat" #2: STATE_QUICK_I2: sent QI2, IPsec SA established
north:~#
 echo done
done
north:~#
 

north:~#
north:~#
 ipsec setup stop
IPSEC EVENT: KLIPS device ipsec0 shut down.
ipsec_setup: Stopping Openswan IPsec...
north:~#
 kill `cat /var/run/klogd.pid`; cat /tmp/klog.log
klogd 1.3-3#33.1, log source = /proc/kmsg started.
north:~#
 halt -p -f
Power down.

