| *received whack message
| processing connection marajade--vpsn
| empty esp_info, returning empty
| creating state object #408 at 0x8223dd8
| processing connection marajade--vpsn
| ICOOKIE:  c8 c9 8b 44  19 84 5a 59
| RCOOKIE:  00 00 00 00  00 00 00 00
| peer:  d8 bf 8c 26
| state hash entry 21
| inserting event EVENT_SO_DISCARD, timeout in 0 seconds for #408
| Queuing pending Quick Mode with 216.191.140.38 "marajade--vpsn"
"marajade--vpsn" #408: initiating Main Mode
| **emit ISAKMP Message:
|    initiator cookie:
|   c8 c9 8b 44  19 84 5a 59
|    responder cookie:
|   00 00 00 00  00 00 00 00
|    next payload type: ISAKMP_NEXT_SA
|    ISAKMP version: ISAKMP Version 1.0
|    exchange type: ISAKMP_XCHG_IDPROT
|    flags: none
|    message ID:  00 00 00 00
| no IKE algorithms for this connection 
| ***emit ISAKMP Security Association Payload:
|    next payload type: ISAKMP_NEXT_VID
|    DOI: ISAKMP_DOI_IPSEC
| ****emit IPsec DOI SIT:
|    IPsec DOI SIT: SIT_IDENTITY_ONLY
| out_sa pcn: 0 has 1 valid proposals
| out_sa pcn: 0 pn: 0<1 valid_count: 1
| ****emit ISAKMP Proposal Payload:
|    next payload type: ISAKMP_NEXT_NONE
|    proposal number: 0
|    protocol ID: PROTO_ISAKMP
|    SPI size: 0
|    number of transforms: 4
| *****emit ISAKMP Transform Payload (ISAKMP):
|    next payload type: ISAKMP_NEXT_T
|    transform number: 0
|    transform ID: KEY_IKE
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_LIFE_TYPE
|    length/value: 1
|     [1 is OAKLEY_LIFE_SECONDS]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_LIFE_DURATION
|    length/value: 3600
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_ENCRYPTION_ALGORITHM
|    length/value: 5
|     [5 is OAKLEY_3DES_CBC]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_HASH_ALGORITHM
|    length/value: 1
|     [1 is OAKLEY_MD5]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_AUTHENTICATION_METHOD
|    length/value: 3
|     [3 is OAKLEY_RSA_SIG]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_GROUP_DESCRIPTION
|    length/value: 5
|     [5 is OAKLEY_GROUP_MODP1536]
| emitting length of ISAKMP Transform Payload (ISAKMP): 32
| *****emit ISAKMP Transform Payload (ISAKMP):
|    next payload type: ISAKMP_NEXT_T
|    transform number: 1
|    transform ID: KEY_IKE
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_LIFE_TYPE
|    length/value: 1
|     [1 is OAKLEY_LIFE_SECONDS]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_LIFE_DURATION
|    length/value: 3600
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_ENCRYPTION_ALGORITHM
|    length/value: 5
|     [5 is OAKLEY_3DES_CBC]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_HASH_ALGORITHM
|    length/value: 2
|     [2 is OAKLEY_SHA1]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_AUTHENTICATION_METHOD
|    length/value: 3
|     [3 is OAKLEY_RSA_SIG]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_GROUP_DESCRIPTION
|    length/value: 5
|     [5 is OAKLEY_GROUP_MODP1536]
| emitting length of ISAKMP Transform Payload (ISAKMP): 32
| *****emit ISAKMP Transform Payload (ISAKMP):
|    next payload type: ISAKMP_NEXT_T
|    transform number: 2
|    transform ID: KEY_IKE
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_LIFE_TYPE
|    length/value: 1
|     [1 is OAKLEY_LIFE_SECONDS]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_LIFE_DURATION
|    length/value: 3600
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_ENCRYPTION_ALGORITHM
|    length/value: 5
|     [5 is OAKLEY_3DES_CBC]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_HASH_ALGORITHM
|    length/value: 2
|     [2 is OAKLEY_SHA1]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_AUTHENTICATION_METHOD
|    length/value: 3
|     [3 is OAKLEY_RSA_SIG]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_GROUP_DESCRIPTION
|    length/value: 2
|     [2 is OAKLEY_GROUP_MODP1024]
| emitting length of ISAKMP Transform Payload (ISAKMP): 32
| *****emit ISAKMP Transform Payload (ISAKMP):
|    next payload type: ISAKMP_NEXT_NONE
|    transform number: 3
|    transform ID: KEY_IKE
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_LIFE_TYPE
|    length/value: 1
|     [1 is OAKLEY_LIFE_SECONDS]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_LIFE_DURATION
|    length/value: 3600
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_ENCRYPTION_ALGORITHM
|    length/value: 5
|     [5 is OAKLEY_3DES_CBC]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_HASH_ALGORITHM
|    length/value: 1
|     [1 is OAKLEY_MD5]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_AUTHENTICATION_METHOD
|    length/value: 3
|     [3 is OAKLEY_RSA_SIG]
| ******emit ISAKMP Oakley attribute:
|    af+type: OAKLEY_GROUP_DESCRIPTION
|    length/value: 2
|     [2 is OAKLEY_GROUP_MODP1024]
| emitting length of ISAKMP Transform Payload (ISAKMP): 32
| emitting length of ISAKMP Proposal Payload: 136
| emitting length of ISAKMP Security Association Payload: 148
| ***emit ISAKMP Vendor ID Payload:
|    next payload type: ISAKMP_NEXT_NONE
| emitting 12 raw bytes of Vendor ID into ISAKMP Vendor ID Payload
| Vendor ID  4f 45 45 46  42 79 7f 64  75 7c 5f 5b
| emitting length of ISAKMP Vendor ID Payload: 16
| ***emit ISAKMP Vendor ID Payload:
|    next payload type: ISAKMP_NEXT_NONE
| emitting 16 raw bytes of V_ID into ISAKMP Vendor ID Payload
| V_ID  af ca d7 13  68 a1 f1 c9  6b 86 96 fc  77 57 01 00
| emitting length of ISAKMP Vendor ID Payload: 20
| nat traversal enabled: 1
| nat add vid. port: 1 nonike: 1
| out_vendorid(): sending [RFC 3947]
| ***emit ISAKMP Vendor ID Payload:
|    next payload type: ISAKMP_NEXT_NONE
| emitting 16 raw bytes of V_ID into ISAKMP Vendor ID Payload
| V_ID  4a 13 1c 81  07 03 58 45  5c 57 28 f2  0e 95 45 2f
| emitting length of ISAKMP Vendor ID Payload: 20
| out_vendorid(): sending [draft-ietf-ipsec-nat-t-ike-03]
| ***emit ISAKMP Vendor ID Payload:
|    next payload type: ISAKMP_NEXT_NONE
| emitting 16 raw bytes of V_ID into ISAKMP Vendor ID Payload
| V_ID  7d 94 19 a6  53 10 ca 6f  2c 17 9d 92  15 52 9d 56
| emitting length of ISAKMP Vendor ID Payload: 20
| out_vendorid(): sending [draft-ietf-ipsec-nat-t-ike-02]
| ***emit ISAKMP Vendor ID Payload:
|    next payload type: ISAKMP_NEXT_NONE
| emitting 16 raw bytes of V_ID into ISAKMP Vendor ID Payload
| V_ID  cd 60 46 43  35 df 21 f8  7c fd b2 fc  68 b6 a4 48
| emitting length of ISAKMP Vendor ID Payload: 20
| out_vendorid(): sending [draft-ietf-ipsec-nat-t-ike-02_n]
| ***emit ISAKMP Vendor ID Payload:
|    next payload type: ISAKMP_NEXT_NONE
| emitting 16 raw bytes of V_ID into ISAKMP Vendor ID Payload
| V_ID  90 cb 80 91  3e bb 69 6e  08 63 81 b5  ec 42 7b 1f
| emitting length of ISAKMP Vendor ID Payload: 20
| out_vendorid(): sending [draft-ietf-ipsec-nat-t-ike-00]
| ***emit ISAKMP Vendor ID Payload:
|    next payload type: ISAKMP_NEXT_NONE
| emitting 16 raw bytes of V_ID into ISAKMP Vendor ID Payload
| V_ID  44 85 15 2d  18 b6 bb cd  0b e8 a8 46  95 79 dd cc
| emitting length of ISAKMP Vendor ID Payload: 20
| emitting length of ISAKMP Message: 312
| sending 312 bytes for main_outI1 through eth0:500 to 216.191.140.38:500:
|   c8 c9 8b 44  19 84 5a 59  00 00 00 00  00 00 00 00
|   01 10 02 00  00 00 00 00  00 00 01 38  0d 00 00 94
|   00 00 00 01  00 00 00 01  00 00 00 88  00 01 00 04
|   03 00 00 20  00 01 00 00  80 0b 00 01  80 0c 0e 10
|   80 01 00 05  80 02 00 01  80 03 00 03  80 04 00 05
|   03 00 00 20  01 01 00 00  80 0b 00 01  80 0c 0e 10
|   80 01 00 05  80 02 00 02  80 03 00 03  80 04 00 05
|   03 00 00 20  02 01 00 00  80 0b 00 01  80 0c 0e 10
|   80 01 00 05  80 02 00 02  80 03 00 03  80 04 00 02
|   00 00 00 20  03 01 00 00  80 0b 00 01  80 0c 0e 10
|   80 01 00 05  80 02 00 01  80 03 00 03  80 04 00 02
|   0d 00 00 10  4f 45 45 46  42 79 7f 64  75 7c 5f 5b
|   0d 00 00 14  af ca d7 13  68 a1 f1 c9  6b 86 96 fc
|   77 57 01 00  0d 00 00 14  4a 13 1c 81  07 03 58 45
|   5c 57 28 f2  0e 95 45 2f  0d 00 00 14  7d 94 19 a6
|   53 10 ca 6f  2c 17 9d 92  15 52 9d 56  0d 00 00 14
|   cd 60 46 43  35 df 21 f8  7c fd b2 fc  68 b6 a4 48
|   0d 00 00 14  90 cb 80 91  3e bb 69 6e  08 63 81 b5
|   ec 42 7b 1f  00 00 00 14  44 85 15 2d  18 b6 bb cd
|   0b e8 a8 46  95 79 dd cc
| inserting event EVENT_RETRANSMIT, timeout in 10 seconds for #408
| next event EVENT_RETRANSMIT in 2 seconds for #407
