Basic pluto with IKEv2 on the responder (east).

This test does not actually do IKEv2, as the initiator doesn't ask for it,
but the responder, being able to do it, should send an appropriate NOTIFY.


