
  Electric Fence 2.1 Copyright (C) 1987-1998 Bruce Perens.

version 2.0

config setup


# begin conn mytestconn
conn mytestconn
	left=192.168.1.101
	leftrsakey=0sabcdabcdabcd
	leftrsakey2=0s23489234ba28934243
	leftcert=/my/cert/file
	leftsourceip=192.168.2.102
	right=%defaultroute
	dpddelay=60
	connalias="anotheralias"
	auto=ignore
	type=transport
	compress=yes
	pfs=yes
	rekey=yes
	authby=never
	phase2=esp
	ikev2=never
# end conn mytestconn

# end of config
