Program invoked with PATH/start.sh test01.sh

Starting UML PATH/start.sh
spawn PATH single
tracing thread pid = XXXXX
Linux version XXXX
On node 0 totalpages: 8192
Kernel command line:
Calibrating delay loop... XXXX bogomips
Memory: 32212k available
Dentry-cache hash table entries: 4096 (order: 3, 32768 bytes)
Inode-cache hash table entries: 2048 (order: 2, 16384 bytes)
Mount-cache hash table entries: 512 (order: 0, 4096 bytes)
Buffer-cache hash table entries: 1024 (order: 0, 4096 bytes)
Page-cache hash table entries: 8192 (order: 3, 32768 bytes)
POSIX conformance testing by UNIFIX
Linux NET4.0 for Linux 2.4
Based upon Swansea University Computer Society NET3.039
Initializing RT netlink socket
Starting kswapd v1.8
VFS: Diskquotas version dquot_6.4.0 initialized
devfs: v0.107 (20010709) Richard Gooch (rgooch@atnf.csiro.au)
devfs: boot_options: 0x2
pty: 256 Unix98 ptys configured
block: 64 slots per queue, batch=8
RAMDISK driver initialized: 16 RAM disks of 4096K size 1024 blocksize
Netdevice 0 : daemon backend- ethernet address = 10:0:0:dc:bc:ff

Netdevice 1 : daemon backend- ethernet address = 10:0:0:64:64:23

SLIP: version 0.8.4-NET3.019-NEWTTY (dynamic channels, max=256).
loop: loaded (max 8 devices)
PPP generic driver version 2.4.1
Universal TUN/TAP device driver 1.4 (C)1999-2001 Maxim Krasnyansky
NET4: Linux TCP/IP 1.0 for NET4.0
IP Protocols: ICMP, UDP, TCP
IP: routing cache hash table of 512 buckets, 4Kbytes
TCP: Hash tables configured (established 2048 bind 2048)
IPv4 over IPv4 tunneling driver
GRE over IPv4 tunneling driver
klips_info:ipsec_init: KLIPS startup, FreeS/WAN IPSec version: XXXX
NET4: Unix domain sockets 1.0/SMP for Linux NET4.0.
VFS: Mounted root (root hostfs filesystem) readonly.
Mounted devfs on /dev
INIT: version 2.78 booting
Activating swap...
Calculating module dependancies
done.
Loading modules: LIST

Checking all file systems...
Parallelizing fsck version 1.18 (11-Nov-1999)
Setting kernel variables.
Mounting local filesystems...
/dev/ubd/1 on /usr/share type hostfs (ro,/usr/share)
/dev/shm on /tmp type tmpfs (rw)
/dev/shm on /var/run type tmpfs (rw)
devpts on /dev/pts type devpts (rw,mode=0622)
Enabling packet forwarding: done.
Configuring network interfaces: done.
Cleaning: /tmp /var/lock /var/run.
Initializing random number generator... done.
Recovering nvi editor sessions... done.
Give root password for maintenance
(or type Control-D for normal startup): Logging in


east:~# 
east:~# ipsec spi --clear
east:~# ipsec eroute --clear
east:~# 
east:~# enckey=0x4043434545464649494a4a4c4c4f4f515152525454575758
east:~# authkey=0x87658765876587658765876587658765
east:~# 
east:~# 
east:~# ipsec spi --af inet --edst 192.1.2.45 --spi 0x12345678 --proto esp --src  192.1.2.23 --esp 3des-md5-96 --life soft-allocations=2 --enckey $enckey --authk ey $authkey
east:~# 
east:~# ipsec spi --af inet --edst 192.1.2.45 --spi 0x12345678 --proto tun --src  192.1.2.23 --dst 192.1.2.45 --ip4
east:~# 
east:~# ipsec spigrp inet 192.1.2.45 0x12345678 tun inet 192.1.2.45 0x12345678 e sp 
/usr/local/lib/ipsec/spigrp: pfkey write failed, returning -1 with errno=2.
device does not exist.  See FreeS/WAN installation procedure.
east:~# 
east:~# ipsec eroute --add --eraf inet --src 192.0.2.0/24 --dst 192.0.1.0/24 --s aid tun0x12345678@192.1.2.45
east:~# 
east:~# ipsec tncfg --attach --virtual ipsec0 --physical eth1
east:~# ifconfig ipsec0 inet 192.1.2.23 netmask 0xffffff00 broadcast 192.1.2.255  up
east:~# 
east:~# arp -s 192.1.2.45 10:00:00:64:64:45
east:~# arp -s 192.1.2.254 10:00:00:64:64:45
east:~# 
east:~# ipsec look
east NOW
192.0.2.0/24       -> 192.0.1.0/24       => tun0x12345678@192.1.2.45  (0)
ipsec0->eth1 mtu=16260(1500)->1500
tun0x12345678@192.1.2.45 IPIP: dir=out src=192.1.2.23 life(c,s,h)=alloc(1,0,0)add(0,0,0)
ROUTING TABLE
east:~# 
east:~# route add -host 192.0.1.1 gw 192.1.2.45 dev ipsec0
east:~# 
east:~# Initialization done

ipsec pf_key
pfkey v2 msg. type=7 seq=1 len=5 pid=133 errno=0 satype=2
pfkey_lib_debug:pfkey_msg_parse: parsing message ver=2, type=7, errno=0, satype=2(AH), len=5, res=0, seq=1, pid=987.
pfkey_lib_debug:pfkey_msg_parse: remain=3
pfkey_lib_debug:pfkey_msg_parse: extensions permitted=0000c001, required=00000001.
pfkey_lib_debug:pfkey_msg_parse: parsing ext type=14 remain=3.
pfkey_lib_debug:pfkey_msg_parse: About to parse extension 14 0x9ffffbec with parser 0x804aabc.
pfkey_lib_debug:pfkey_msg_parse: Extension 14 parsed.
pfkey_lib_debug:pfkey_msg_parse: extensions permitted=0000c001, seen=00004001, required=00000001.
pf_key: parseable PF_KEY message.
pfkey v2 msg. type=7 seq=2 len=7 pid=133 errno=0 satype=3
pfkey_lib_debug:pfkey_msg_parse: parsing message ver=2, type=7, errno=0, satype=3(ESP), len=7, res=0, seq=2, pid=987.
pfkey_lib_debug:pfkey_msg_parse: remain=5
pfkey_lib_debug:pfkey_msg_parse: extensions permitted=0000c001, required=00000001.
pfkey_lib_debug:pfkey_msg_parse: parsing ext type=14 remain=5.
pfkey_lib_debug:pfkey_msg_parse: About to parse extension 14 0x9ffffbec with parser 0x804aabc.
pfkey_lib_debug:pfkey_msg_parse: Extension 14 parsed.
pfkey_lib_debug:pfkey_msg_parse: parsing ext type=15 remain=2.
pfkey_lib_debug:pfkey_msg_parse: About to parse extension 15 0x9ffffc04 with parser 0x804aabc.
pfkey_lib_debug:pfkey_msg_parse: Extension 15 parsed.
pfkey_lib_debug:pfkey_msg_parse: extensions permitted=0000c001, seen=0000c001, required=00000001.
pf_key: parseable PF_KEY message.
pfkey v2 msg. type=7 seq=3 len=4 pid=133 errno=0 satype=9
pfkey_lib_debug:pfkey_msg_parse: parsing message ver=2, type=7, errno=0, satype=9(IPIP), len=4, res=0, seq=3, pid=987.
pfkey_lib_debug:pfkey_msg_parse: remain=2
pfkey_lib_debug:pfkey_msg_parse: extensions permitted=0000c001, required=00000001.
pfkey_lib_debug:pfkey_msg_parse: parsing ext type=15 remain=2.
pfkey_lib_debug:pfkey_msg_parse: About to parse extension 15 0x9ffffbec with parser 0x804aabc.
pfkey_lib_debug:pfkey_msg_parse: Extension 15 parsed.
pfkey_lib_debug:pfkey_msg_parse: extensions permitted=0000c001, seen=00008001, required=00000001.
pf_key: parseable PF_KEY message.
pfkey v2 msg. type=7 seq=4 len=4 pid=133 errno=0 satype=10
pfkey_lib_debug:pfkey_msg_parse: parsing message ver=2, type=7, errno=0, satype=10(COMP), len=4, res=0, seq=4, pid=987.
pfkey_lib_debug:pfkey_msg_parse: remain=2
pfkey_lib_debug:pfkey_msg_parse: extensions permitted=0000c001, required=00000001.
pfkey_lib_debug:pfkey_msg_parse: parsing ext type=15 remain=2.
pfkey_lib_debug:pfkey_msg_parse: About to parse extension 15 0x9ffffbec with parser 0x804aabc.
pfkey_lib_debug:pfkey_msg_parse: Extension 15 parsed.
pfkey_lib_debug:pfkey_msg_parse: extensions permitted=0000c001, seen=00008001, required=00000001.
pf_key: parseable PF_KEY message.
nbd: module cleaned up.

