

WORK in progress, needs review

Starting UML /btmp/antony/ikev2/2008_01_14/UMLPOOL/east/start-netkey.sh
spawn /btmp/antony/ikev2/2008_01_14/UMLPOOL/east/start-netkey.sh single
Checking that ptrace can change system call numbers...OK
Checking syscall emulation patch for ptrace...OK
Checking advanced syscall emulation patch for ptrace...OK
Checking for tmpfs mount on /dev/shm...OK
Checking PROT_EXEC mmap in /dev/shm/...OK
Checking for the skas3 patch in the host:
  - /proc/mm...not found
  - PTRACE_FAULTINFO...not found
  - PTRACE_LDT...not found
UML running in SKAS0 mode
Checking that ptrace can change system call numbers...OK
Checking syscall emulation patch for ptrace...OK
Checking advanced syscall emulation patch for ptrace...OK
Linux version 2.6.18.6 (antony@sal) (gcc version 4.2.3 20080114 (prerelease) (Debian 4.2.2-7)) #6 Wed Feb 13 11:18:26 EST 2008
Built 1 zonelists.  Total pages: 8192
Kernel command line: initrd=/btmp/antony/ikev2/2008_01_14/UMLPOOL/initrd.uml umlroot=/btmp/antony/ikev2/2008_01_14/UMLPOOL/east/root root=/dev/ram0 rw ssl=pty eth0=daemon,10:00:00:dc:bc:ff,unix,/tmp/umljZyuOz.d/east/ctl,/tmp/umljZyuOz.d/east/data eth1=daemon,10:00:00:64:64:23,unix,/tmp/umljZyuOz.d/public/ctl,/tmp/umljZyuOz.d/public/data eth2=daemon,10:00:00:32:64:23,unix,/tmp/umljZyuOz.d/admin/ctl,/tmp/umljZyuOz.d/admin/data init=/linuxrc single
PID hash table entries: 256 (order: 8, 1024 bytes)
Dentry cache hash table entries: 4096 (order: 2, 16384 bytes)
Inode-cache hash table entries: 2048 (order: 1, 8192 bytes)
Memory: 27028k available
Mount-cache hash table entries: 512
Checking for host processor cmov support...Yes
Checking for host processor xmm support...No
Checking that host ptys support output SIGIO...Yes
Checking that host ptys support SIGIO on close...No, enabling workaround
checking if image is initramfs...it isn't (bad gzip magic numbers); looks like an initrd
Freeing initrd memory: 1212k freed
Using 2.6 host AIO
NET: Registered protocol family 16
NET: Registered protocol family 2
IP route cache hash table entries: 256 (order: -2, 1024 bytes)
TCP established hash table entries: 1024 (order: 0, 4096 bytes)
TCP bind hash table entries: 512 (order: -1, 2048 bytes)
TCP: Hash tables configured (established 1024 bind 512)
TCP reno registered
daemon_setup : Ignoring data socket specification
Netdevice 0 (10:00:00:dc:bc:ff) : daemon backend (uml_switch version 3) - unix:/tmp/umljZyuOz.d/east/ctl
daemon_setup : Ignoring data socket specification
Netdevice 1 (10:00:00:64:64:23) : daemon backend (uml_switch version 3) - unix:/tmp/umljZyuOz.d/public/ctl
daemon_setup : Ignoring data socket specification
Netdevice 2 (10:00:00:32:64:23) : daemon backend (uml_switch version 3) - unix:/tmp/umljZyuOz.d/admin/ctl
Checking host MADV_REMOVE support...OK
mconsole (version 2) initialized on /home/antony/.uml/east/mconsole
Host TLS support detected
Detected host type: i386
VFS: Disk quotas dquot_6.5.1
Dquot-cache hash table entries: 1024 (order 0, 4096 bytes)
Initializing Cryptographic API
io scheduler noop registered
io scheduler anticipatory registered (default)
io scheduler deadline registered
io scheduler cfq registered
RAMDISK driver initialized: 16 RAM disks of 4096K size 1024 blocksize
loop: loaded (max 8 devices)
nbd: registered device at major 43
PPP generic driver version 2.4.2
SLIP: version 0.8.4-NET3.019-NEWTTY (dynamic channels, max=256).
tun: Universal TUN/TAP device driver, 1.6
tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>
Netfilter messages via NETLINK v0.30.
IPv4 over IPv4 tunneling driver
GRE over IPv4 tunneling driver
ip_conntrack version 2.4 (211 buckets, 1688 max) - 224 bytes per conntrack
ctnetlink v0.90: registering with nfnetlink.
ip_conntrack_pptp version 3.1 loaded
ip_nat_pptp version 3.0 loaded
ip_tables: (C) 2000-2006 Netfilter Core Team
ClusterIP Version 0.8 loaded successfully
arp_tables: (C) 2002 David S. Miller
TCP bic registered
TCP westwood registered
TCP highspeed registered
TCP hybla registered
TCP htcp registered
TCP vegas registered
TCP scalable registered
Initializing IPsec netlink socket
NET: Registered protocol family 1
NET: Registered protocol family 17
NET: Registered protocol family 15
Initialized stdio console driver
Console initialized on /dev/tty0
Initializing software serial port version 1
Failed to open 'root_fs', errno = 2
RAMDISK: cramfs filesystem found at block 0
RAMDISK: Loading 1212KiB [1 disk] into ram disk... |/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\done.
VFS: Mounted root (cramfs filesystem) readonly.
MOUNTING /btmp/antony/ikev2/2008_01_14/UMLPOOL/east/root for UML testing root.
Mounting a tmpfs over /dev...done.
Creating initial device nodes...done.
Invoked with Arguments: single
Creating initial device nodes...done.
crw-r--r--    1 root     root       5,   1 Feb 14 00:12 /dev/console
line_ioctl: tty0: ioctl KDSIGACCEPT called

INIT: version 2.78 booting

/dev/root on / type hostfs (rw)
proc on /proc type proc (rw)
devpts on /dev/pts type devpts (rw,gid=5,mode=620)
/dev/shm on /tmp type tmpfs (rw)
/dev/shm on /var/run type tmpfs (rw)
none on /usr/share type hostfs (ro)
none on /testing type hostfs (ro,/home/antony/ikev2/testing)
none on /usr/src type hostfs (ro,/home/antony/ikev2)
none on /usr/obj type hostfs (ro,/home/antony/ikev2/OBJ.linux.i386)
none on /usr/local type hostfs (rw,/btmp/antony/ikev2/2008_01_14/UMLPOOL/east/root/usr/local)
none on /var/tmp type hostfs (rw,/btmp/antony/ikev2/2008_01_14/UMLPOOL/east/root/var/tmp)
none on /proc type proc (rw)
crw-r--r--    1 root     root       5,   1 Feb 14 00:12 /dev/console
mount: proc already mounted
Activating swap...
Checking all file systems...
Parallelizing fsck version 1.18 (11-Nov-1999)
Setting kernel variables.
Mounting local filesystems...
mount: devpts already mounted on /dev/pts
/dev/shm on /tmp type tmpfs (rw)
/dev/shm on /var/run type tmpfs (rw)
none on /usr/share type hostfs (ro)
none on /testing type hostfs (ro,/home/antony/ikev2/testing)
none on /usr/src type hostfs (ro,/home/antony/ikev2)
none on /usr/obj type hostfs (ro,/home/antony/ikev2/OBJ.linux.i386)
none on /usr/local type hostfs (rw,/btmp/antony/ikev2/2008_01_14/UMLPOOL/east/root/usr/local)
none on /var/tmp type hostfs (rw,/btmp/antony/ikev2/2008_01_14/UMLPOOL/east/root/var/tmp)
Enabling packet forwarding: done.
Configuring network interfaces: done.
Cleaning: /tmp /var/lock /var/run.
Initializing random number generator... done.
Recovering nvi editor sessions... done.
Give root password for maintenance
(or type Control-D for normal startup): 
east:~# echo Starting loading module
Starting loading module
east:~# exec bash --noediting
east:~# ulimit -c unlimited
east:~# echo Finished loading module
Finished loading module
east:~# klogd -c 4 -x -f /tmp/klog.log
east:~# : ==== start ====
east:~# TESTNAME=netkey-pluto-02
east:~# source /testing/pluto/bin/eastlocal.sh
east:~# ipsec setup start
ipsec_setup: Starting Openswan IPsec U2.5.testing-g21680e0d-dirty/K2.6.18.6...
ipsec_setup: Trying hardware random, this may fail, which is okay.
ipsec_setup: Trying to load all NETKEY modules:xfrm6_tunnel xfrm6_mode_tunnel xfrm6_mode_beet xfrm6_mode_ro xfrm6_mode_transport xfrm4_mode_transport xfrm4_mode_tunnel xfrm4_tunnel xfrm4_mode_beet esp4 esp6 ah4 ah6 ipcomp ipcomp6 af_key 
ipsec_setup: Trying VIA padlock driver, this may fail, which is okay.
ipsec_setup: Trying to load Crypto API modules, some may fail, which is okay.
ipsec_setup: aes-x86_64 aes des sha512 sha256 md5 cbc xcbc ecb twofish blowfish serpent 
east:~# ipsec auto --add westnet-eastnet
east:~# ipsec whack --debug-control --debug-controlmore --debug-crypt
east:~# /testing/pluto/bin/wait-until-pluto-started
east:~# : === NETJIG start of WEST westrun.sh 
east:~# 

east:~# : ==== cut ====
east:~# ipsec auto --status
000 using kernel interface: netkey
000 interface eth0/eth0 192.0.2.254
000 interface eth1/eth1 192.1.2.23
000 interface eth2/eth2 192.9.2.23
000 interface lo/lo 127.0.0.1
000 %myid = (none)
000 debug crypt+control+controlmore
000  
000 algorithm ESP encrypt: id=2, name=ESP_DES, ivlen=8, keysizemin=64, keysizemax=64
000 algorithm ESP encrypt: id=3, name=ESP_3DES, ivlen=8, keysizemin=192, keysizemax=192
000 algorithm ESP encrypt: id=7, name=ESP_BLOWFISH, ivlen=8, keysizemin=40, keysizemax=448
000 algorithm ESP encrypt: id=11, name=ESP_NULL, ivlen=0, keysizemin=0, keysizemax=0
000 algorithm ESP encrypt: id=12, name=ESP_AES, ivlen=8, keysizemin=128, keysizemax=256
000 algorithm ESP encrypt: id=252, name=ESP_SERPENT, ivlen=8, keysizemin=128, keysizemax=256
000 algorithm ESP encrypt: id=253, name=ESP_TWOFISH, ivlen=8, keysizemin=128, keysizemax=256
000 algorithm ESP auth attr: id=1, name=AUTH_ALGORITHM_HMAC_MD5, keysizemin=128, keysizemax=128
000 algorithm ESP auth attr: id=2, name=AUTH_ALGORITHM_HMAC_SHA1, keysizemin=160, keysizemax=160
000 algorithm ESP auth attr: id=5, name=AUTH_ALGORITHM_HMAC_SHA2_256, keysizemin=256, keysizemax=256
000 algorithm ESP auth attr: id=251, name=(null), keysizemin=0, keysizemax=0
000  
000 algorithm IKE encrypt: id=3, name=OAKLEY_BLOWFISH_CBC, blocksize=8, keydeflen=128
000 algorithm IKE encrypt: id=5, name=OAKLEY_3DES_CBC, blocksize=8, keydeflen=192
000 algorithm IKE encrypt: id=7, name=OAKLEY_AES_CBC, blocksize=16, keydeflen=128
000 algorithm IKE encrypt: id=65004, name=OAKLEY_SERPENT_CBC, blocksize=16, keydeflen=128
000 algorithm IKE encrypt: id=65005, name=OAKLEY_TWOFISH_CBC, blocksize=16, keydeflen=128
000 algorithm IKE encrypt: id=65289, name=OAKLEY_TWOFISH_CBC_SSH, blocksize=16, keydeflen=128
000 algorithm IKE hash: id=1, name=OAKLEY_MD5, hashsize=16
000 algorithm IKE hash: id=2, name=OAKLEY_SHA1, hashsize=20
000 algorithm IKE hash: id=4, name=OAKLEY_SHA2_256, hashsize=32
000 algorithm IKE hash: id=6, name=OAKLEY_SHA2_512, hashsize=64
000 algorithm IKE dh group: id=2, name=OAKLEY_GROUP_MODP1024, bits=1024
000 algorithm IKE dh group: id=5, name=OAKLEY_GROUP_MODP1536, bits=1536
000 algorithm IKE dh group: id=14, name=OAKLEY_GROUP_MODP2048, bits=2048
000 algorithm IKE dh group: id=15, name=OAKLEY_GROUP_MODP3072, bits=3072
000 algorithm IKE dh group: id=16, name=OAKLEY_GROUP_MODP4096, bits=4096
000 algorithm IKE dh group: id=17, name=OAKLEY_GROUP_MODP6144, bits=6144
000 algorithm IKE dh group: id=18, name=OAKLEY_GROUP_MODP8192, bits=8192
000  
000 stats db_ops: {curr_cnt, total_cnt, maxsz} :context={0,0,0} trans={0,0,0} attrs={0,0,0} 
000  
000 "westnet-eastnet": 192.0.2.0/24===192.1.2.23<192.1.2.23>[@east,S=C]...192.1.2.45<192.1.2.45>[@west,S=C]===192.0.1.0/24; prospective erouted; eroute owner: #0
000 "westnet-eastnet":     myip=unset; hisip=unset;
000 "westnet-eastnet":   ike_life: 3600s; ipsec_life: 28800s; rekey_margin: 540s; rekey_fuzz: 100%; keyingtries: 3
000 "westnet-eastnet":   policy: RSASIG+ENCRYPT+TUNNEL+PFS+IKEv2ALLOW; prio: 24,24; interface: eth1; 
000 "westnet-eastnet":   newest ISAKMP SA: #0; newest IPsec SA: #0; 
000 "westnet-eastnet":   ESP algorithms wanted: 3DES(3)_000-MD5(1); flags=-strict
000 "westnet-eastnet":   ESP algorithms loaded: 3DES(3)_192-MD5(1)_128
000  
000  
east:~# cat /tmp/pluto.log
Plutorun started on Thu Feb 14 00:12:26 GMT 2008
Starting Pluto (Openswan Version 2.5.testing-g21680e0d-dirty; Vendor ID OEGJMMweP{pQ) pid:920
Setting NAT-Traversal port-4500 floating to off
   port floating activation criteria nat_t=0/port_float=1
   including NAT-Traversal patch (Version 0.6c) [disabled]
using /dev/urandom as source of random entropy
ike_alg_register_enc(): Activating OAKLEY_TWOFISH_CBC_SSH: Ok (ret=0)
ike_alg_register_enc(): Activating OAKLEY_TWOFISH_CBC: Ok (ret=0)
ike_alg_register_enc(): Activating OAKLEY_SERPENT_CBC: Ok (ret=0)
ike_alg_register_enc(): Activating OAKLEY_AES_CBC: Ok (ret=0)
ike_alg_register_enc(): Activating OAKLEY_BLOWFISH_CBC: Ok (ret=0)
ike_alg_register_hash(): Activating OAKLEY_SHA2_512: Ok (ret=0)
ike_alg_register_hash(): Activating OAKLEY_SHA2_256: Ok (ret=0)
starting up 1 cryptographic helpers
using /dev/urandom as source of random entropy
started helper pid=925 (fd:6)
Using Linux 2.6 IPsec interface code on 2.6.18.6 (experimental code)
Changed path to directory '/tmp/netkey-pluto-02/ipsec.d/cacerts'
  loaded CA cert file 'otherca.crt' (1428 bytes)
  loaded CA cert file 'caCert.pem' (4854 bytes)
  loaded CA cert file 'ca.crt' (1184 bytes)
  RSA modulus too small for security: less than 512 bits
  error in X.509 certificate
Changed path to directory '/tmp/netkey-pluto-02/ipsec.d/aacerts'
Changed path to directory '/tmp/netkey-pluto-02/ipsec.d/ocspcerts'
Changing to directory '/tmp/netkey-pluto-02/ipsec.d/crls'
  loaded crl file 'othercacrl.pem' (556 bytes)
  loaded crl file 'nic.crl' (642 bytes)
  loaded crl file 'crashcrl-3.pem' (690 bytes)
crl issuer cacert not found for (file:///tmp/netkey-pluto-02/ipsec.d/crls/crashcrl-3.pem)
  loaded crl file 'crashcrl-2.pem' (528 bytes)
crl issuer cacert not found for (file:///tmp/netkey-pluto-02/ipsec.d/crls/crashcrl-2.pem)
  loaded crl file 'crashcrl-1.pem' (1053 bytes)
crl issuer cacert not found for (file:///tmp/netkey-pluto-02/ipsec.d/crls/crashcrl-1.pem)
  loaded crl file 'cacrlvalid.pem' (581 bytes)
crl issuer cacert not found for (file:///tmp/netkey-pluto-02/ipsec.d/crls/cacrlvalid.pem)
  loaded crl file 'cacrlnotyetvalid.pem' (552 bytes)
crl issuer cacert not found for (file:///tmp/netkey-pluto-02/ipsec.d/crls/cacrlnotyetvalid.pem)
  loaded crl file 'cacrlexpired.pem' (552 bytes)
crl issuer cacert not found for (file:///tmp/netkey-pluto-02/ipsec.d/crls/cacrlexpired.pem)
listening for IKE messages
adding interface lo/lo 127.0.0.1:500
adding interface eth2/eth2 192.9.2.23:500
adding interface eth1/eth1 192.1.2.23:500
adding interface eth0/eth0 192.0.2.254:500
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
added connection description "westnet-eastnet"
| base debugging = crypt+control+controlmore
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 119 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x81425f8) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x81425f8) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 119 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x81439d8) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x81439d8) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 117 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x81439d8) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x81439d8) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 115 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 113 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 111 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 109 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 106 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 104 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 102 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 100 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 98 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 96 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 94 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 92 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 90 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 88 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 86 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 83 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x8142130) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x8142130) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 81 seconds
|  
| *received whack message
listening for IKE messages
| found eth0 with address 192.0.2.254
| found eth1 with address 192.1.2.23
| found eth2 with address 192.9.2.23
| found lo with address 127.0.0.1
| could not open /proc/net/if_inet6
forgetting secrets
loading secrets from "/tmp/netkey-pluto-02/ipsec.secrets"
loaded private key for keyid: PPK_RSA:AQN3cn11F
| id type added to secret(0x814fbb8) 1: C=ca, ST=Ontario, O=Xelerance, CN=east.xelerance.com, E=testing@xelerance.com
| id type added to secret(0x814fbb8) 1: %any
  loaded private key file '/etc/ipsec.d/private/east.key' (464 bytes)
|   decrypting file using 'DES-EDE3-CBC'
"/tmp/netkey-pluto-02/ipsec.secrets" line 25: RSA modulus too small for security: less than 512 bits
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 79 seconds
|  
| *received 404 bytes from 192.1.2.45:500 on eth1 (port=500)
|  processing version=1.0 packet with exchange type=ISAKMP_XCHG_IDPROT (2)
packet from 192.1.2.45:500: received Vendor ID payload [Openswan (this version) 2.5.testing-g21680e0d-dirty ]
packet from 192.1.2.45:500: received Vendor ID payload [Dead Peer Detection]
| find_host_connection called from main_inI1_outR1, me=192.1.2.23:500 him=192.1.2.45:500 policy=none
| find_host_pair: comparing to 192.1.2.23:500 192.1.2.45:500 
| find_host_pair_conn (find_host_connection2): 192.1.2.23:500 192.1.2.45:500 -> hp:westnet-eastnet 
| find_host_connection returns westnet-eastnet
| creating state object #1 at 0x81505a0
| processing connection westnet-eastnet
| ICOOKIE:  64 87 18 2d  ee 7c ff fb
| RCOOKIE:  75 7b 48 54  0a 79 92 ea
| state hash entry 11
| inserting state object #1 on chain 11
| inserting event EVENT_SO_DISCARD, timeout in 0 seconds for #1
"westnet-eastnet" #1: responding to Main Mode
| Oakley Transform 0 accepted
| sender checking NAT-t: 0 and 0
| complete state transition with STF_OK
"westnet-eastnet" #1: transition from state STATE_MAIN_R0 to state STATE_MAIN_R1
| sending reply packet to 192.1.2.45:500 (from port 500)
| sending 116 bytes for STATE_MAIN_R0 through eth1:500 to 192.1.2.45:500 (using #1)
| inserting event EVENT_RETRANSMIT, timeout in 10 seconds for #1
"westnet-eastnet" #1: STATE_MAIN_R1: sent MR1, expecting MI2
| modecfg pull: noquirk policy:push not-client
| phase 1 is done, looking for phase 2 to unpend
| * processed 0 messages from cryptographic helpers 
| next event EVENT_RETRANSMIT in 10 seconds for #1
|  
| *received 308 bytes from 192.1.2.45:500 on eth1 (port=500)
|  processing version=1.0 packet with exchange type=ISAKMP_XCHG_IDPROT (2)
| ICOOKIE:  64 87 18 2d  ee 7c ff fb
| RCOOKIE:  75 7b 48 54  0a 79 92 ea
| state hash entry 11
| v1 peer and cookies match on #1, provided msgid 00000000 vs 00000000
| v1 state object #1 found, in STATE_MAIN_R1
| processing connection westnet-eastnet
| DH public value received:
|   c1 8a 5b 2b  fc 9e e0 5b  90 b0 81 ea  cd 98 c8 cf
|   20 04 e5 db  2a 7a 3e ba  84 23 e8 39  16 02 47 f1
|   83 56 50 06  5b a6 88 85  50 a1 c5 31  14 06 2e b8
|   a3 b9 c4 c3  51 41 0f d6  46 a3 20 4c  33 5a 1e 62
|   e3 ed 99 ef  14 59 7a 2a  31 20 13 1c  64 71 66 3d
|   40 d3 13 42  97 53 76 4d  83 6d 98 bf  a5 ca ab c5
|   61 f0 50 f3  ef 77 84 97  27 8a ca 64  48 ee bf c1
|   98 bd 30 ab  79 aa 3d 78  1a 3b fc 87  a5 96 09 f2
|   44 4c 59 64  bf d1 da f8  4d ea 96 f2  36 ee ca a1
|   6b 0a b1 55  ec 69 3f f2  40 11 99 a2  9c 35 38 f0
|   6a 12 2c 18  18 00 83 12  ac 68 a9 57  5d 64 65 da
|   12 da cc ba  a0 e2 1b 73  5b a8 cf 6a  7c ad 5e d3
|   b7 cb 36 05  60 52 13 70  46 10 8f d6  63 76 3a 27
|   51 c0 51 3a  e6 a4 e3 ca  4d 07 a7 ed  13 1c 0c 14
|   92 ff 9b 3c  ae ea a2 d4  fb ca cf a2  6d 02 03 be
|   2b 26 7a c0  b8 26 5c d4  40 ba 13 5a  6c f4 35 84
| inI2: checking NAT-t: 0 and 0
| 0: w->pcw_dead: 0 w->pcw_work: 0 cnt: 1
| asking helper 0 to do build_kenonce op on seq: 1 (len=2668, pcw_work=1)
| crypto helper write of request: cnt=2668<wlen=2668.  
| inserting event EVENT_CRYPTO_FAILED, timeout in 300 seconds for #1
| complete state transition with STF_SUSPEND
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 54 seconds
|  
| helper 0 has finished work (cnt now 1)
| helper 0 replies to id: q#1
| calling callback function 0x806a25f
| main inI2_outR2: calculated ke+nonce, sending R2
| processing connection westnet-eastnet
| main inI2_outR2: starting async DH calculation (group=14)
| started looking for secret for @east->@west of kind PPK_PSK
| actually looking for secret for @east->@west of kind PPK_PSK
| line 8: key type PPK_PSK(@east) to type PPK_RSA 
| concluding with best_match=0 best=(nil) (lineno=-1)
| parent1 type: 7 group: 14 len: 2668 
| 0: w->pcw_dead: 0 w->pcw_work: 0 cnt: 1
| asking helper 0 to do compute dh+iv op on seq: 2 (len=2668, pcw_work=1)
| crypto helper write of request: cnt=2668<wlen=2668.  
| inserting event EVENT_CRYPTO_FAILED, timeout in 300 seconds for #1
| started dh_secretiv, returned: stf=STF_SUSPEND 
| complete state transition with STF_OK
"westnet-eastnet" #1: transition from state STATE_MAIN_R1 to state STATE_MAIN_R2
| sending reply packet to 192.1.2.45:500 (from port 500)
| sending 308 bytes for STATE_MAIN_R1 through eth1:500 to 192.1.2.45:500 (using #1)
| inserting event EVENT_RETRANSMIT, timeout in 10 seconds for #1
"westnet-eastnet" #1: STATE_MAIN_R2: sent MR2, expecting MI3
| modecfg pull: noquirk policy:push not-client
| phase 1 is done, looking for phase 2 to unpend
| * processed 1 messages from cryptographic helpers 
| next event EVENT_RETRANSMIT in 10 seconds for #1
|  
| helper 0 has finished work (cnt now 1)
| helper 0 replies to id: q#2
| calling callback function 0x806a665
| main inI2_outR2: calculated DH finished
| processing connection westnet-eastnet
| * processed 1 messages from cryptographic helpers 
| next event EVENT_RETRANSMIT in 10 seconds for #1
|  
| *received 300 bytes from 192.1.2.45:500 on eth1 (port=500)
|  processing version=1.0 packet with exchange type=ISAKMP_XCHG_IDPROT (2)
| ICOOKIE:  64 87 18 2d  ee 7c ff fb
| RCOOKIE:  75 7b 48 54  0a 79 92 ea
| state hash entry 11
| v1 peer and cookies match on #1, provided msgid 00000000 vs 00000000
| v1 state object #1 found, in STATE_MAIN_R2
| processing connection westnet-eastnet
| received encrypted packet from 192.1.2.45:500
| decrypting 272 bytes using algorithm OAKLEY_AES_CBC
| decrypted:
|   09 00 00 0c  02 00 00 00  77 65 73 74  00 00 01 04
|   19 2a fb 07  03 e5 c5 cb  53 d8 7a 67  1f fe 9a 1a
|   b5 12 ee 3c  ab 70 86 77  de 22 28 44  66 4b 3c bc
|   b7 08 41 40  e2 03 22 e3  eb b9 21 40  8d f2 39 be
|   01 db 14 6f  7d f6 c7 c3  82 1b 29 8a  eb 4e 87 33
|   83 dd f6 15  13 9d dd 57  2e 94 ad 29  c5 2e 2e e3
|   3b 1b 05 29  e4 8e 85 e5  a6 c6 89 94  f4 df b7 3f
|   5a da 05 ef  f8 82 b5 72  a5 8e bd ef  ea b1 03 b1
|   ba 1c 90 ce  52 a0 1b 32  40 94 ab 57  77 4f a2 d7
|   0b 50 11 fa  cc 99 a1 3f  41 30 ac 53  80 05 9e 31
|   99 9d a2 56  52 0a 46 d6  53 0d 7f 3a  7d f0 63 94
|   cb 9a ce a8  a3 f2 16 c8  5d 54 ed bf  67 12 28 0c
|   b5 65 bd f0  4c ae 0a d3  a0 a8 b8 10  6b ca bc f5
|   85 e6 34 ba  5f b6 84 86  60 55 e7 18  60 b6 6d 2e
|   31 db 01 db  9b 1b fb 8e  e3 d5 d6 7c  af 93 e4 5f
|   f1 43 3d e7  ca 84 41 0d  9a eb 06 63  6d d3 e1 38
|   e1 f6 b2 3a  1a 6f 8a cc  4d 60 78 27  8d 23 89 34
| next IV:  ad 44 4f 68  0e 37 ac 9c  86 25 1b 3b  87 0d 53 9d
"westnet-eastnet" #1: Main mode peer ID is ID_FQDN: '@west'
| refine_connection: starting with westnet-eastnet
|    match_id a=@west
|             b=@west
|    results  matched
|   trusted_ca called with a=(empty) b=(empty)
| refine_connection: checking westnet-eastnet against westnet-eastnet, best=(none) with match=1(id=1/ca=1/reqca=1)
| refine_connection: checked westnet-eastnet against westnet-eastnet, now for see if best
| started looking for secret for @east->@west of kind PPK_RSA
| actually looking for secret for @east->@west of kind PPK_RSA
| line 8: key type PPK_RSA(@east) to type PPK_RSA 
| 1: compared key (none) to @east / @west -> 6
| 2: compared key (none) to @east / @west -> 6
| line 8: match=6 
| best_match 0>6 best=0x8144e10 (line=8)
| concluding with best_match=6 best=0x8144e10 (lineno=8)
| offered CA: '%none'
| hashing 336 bytes of SA
| required CA is '%any'
|   trusted_ca called with a=(empty) b=(empty)
| key issuer CA is '%any'
| an RSA Sig check passed with *AQNzGEFs1 [preloaded key]
| authentication succeeded
| thinking about whether to send my certificate:
|   I have RSA key: OAKLEY_RSA_SIG cert.type: CERT_NONE 
|   sendcert: CERT_ALWAYSSEND and I did not get a certificate request 
|   so do not send cert.
| I did not send a certificate because I do not have one.
| hashing 336 bytes of SA
| started looking for secret for @east->@west of kind PPK_RSA
| actually looking for secret for @east->@west of kind PPK_RSA
| line 8: key type PPK_RSA(@east) to type PPK_RSA 
| 1: compared key (none) to @east / @west -> 6
| 2: compared key (none) to @east / @west -> 6
| line 8: match=6 
| best_match 0>6 best=0x8144e10 (line=8)
| concluding with best_match=6 best=0x8144e10 (lineno=8)
| signing hash with RSA Key *AQN3cn11F
| encrypting:
|   09 00 00 0c  02 00 00 00  65 61 73 74  00 00 01 04
|   40 6e 2d 6d  6c 7a 51 84  1a 16 36 08  dd 3d 25 ac
|   62 42 06 e2  70 d3 39 4d  04 fa 3e 7a  e0 59 bf ef
|   d1 53 18 78  01 d1 62 e9  14 fc 0c e8  10 ca 71 f3
|   c1 65 5f bd  db 9d 11 d3  17 57 33 17  2a 85 2b 6f
|   9f 33 36 7a  a5 7a 48 68  09 cb fd 02  95 eb 9f 40
|   e3 ce 3f ca  ce 26 1d ee  f4 e1 44 a4  13 78 95 c1
|   c7 ad ee 4e  01 63 e0 99  09 33 74 39  72 9d 4b 21
|   f3 fa 5f 76  25 a0 e4 02  06 31 ba 91  f6 6a e8 5e
|   e6 08 ab a5  d1 c6 54 80  24 a2 69 b1  24 6a ff 46
|   f6 a0 89 dd  04 26 6f f7  17 db b4 65  30 1c 20 c1
|   5d 2c 1e 2e  5c 28 46 b7  d7 77 0c 82  03 2c 31 89
|   d8 59 d3 dd  ab 99 26 22  5c 1b ee 47  de 93 0b 37
|   29 0c f2 0a  d8 39 a7 da  94 f3 b1 96  ee a3 0e 4f
|   88 20 73 c4  62 44 85 2e  72 f5 12 0d  cd 0a 07 5a
|   7d 63 55 d3  d3 6e 90 32  26 c1 7a 39  db 45 f9 20
|   f4 6e 89 85  60 14 e2 11  79 89 b4 f0  7e 74 27 1f
| IV:
|   ad 44 4f 68  0e 37 ac 9c  86 25 1b 3b  87 0d 53 9d
| unpadded size is: 272
| encrypting 272 using OAKLEY_AES_CBC
| next IV:  65 38 7f d7  47 6d 4f 56  db 39 5d 6a  c8 f6 d4 e2
| last encrypted block of Phase 1:
|   65 38 7f d7  47 6d 4f 56  db 39 5d 6a  c8 f6 d4 e2
| complete state transition with STF_OK
"westnet-eastnet" #1: transition from state STATE_MAIN_R2 to state STATE_MAIN_R3
| sending reply packet to 192.1.2.45:500 (from port 500)
| sending 300 bytes for STATE_MAIN_R2 through eth1:500 to 192.1.2.45:500 (using #1)
| inserting event EVENT_SA_REPLACE, timeout in 3330 seconds for #1
"westnet-eastnet" #1: STATE_MAIN_R3: sent MR3, ISAKMP SA established {auth=OAKLEY_RSA_SIG cipher=aes_128 prf=oakley_sha group=modp2048}
| modecfg pull: noquirk policy:push not-client
| phase 1 is done, looking for phase 2 to unpend
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 54 seconds
|  
| *received 428 bytes from 192.1.2.45:500 on eth1 (port=500)
|  processing version=1.0 packet with exchange type=ISAKMP_XCHG_QUICK (32)
| ICOOKIE:  64 87 18 2d  ee 7c ff fb
| RCOOKIE:  75 7b 48 54  0a 79 92 ea
| state hash entry 11
| v1 peer and cookies match on #1, provided msgid c58116b4 vs 00000000
| v1 state object not found
| ICOOKIE:  64 87 18 2d  ee 7c ff fb
| RCOOKIE:  75 7b 48 54  0a 79 92 ea
| state hash entry 11
| v1 peer and cookies match on #1, provided msgid 00000000 vs 00000000
| v1 state object #1 found, in STATE_MAIN_R3
| processing connection westnet-eastnet
| last Phase 1 IV:  65 38 7f d7  47 6d 4f 56  db 39 5d 6a  c8 f6 d4 e2
| current Phase 1 IV:  65 38 7f d7  47 6d 4f 56  db 39 5d 6a  c8 f6 d4 e2
| computed Phase 2 IV:
|   17 9f 64 78  b1 7b 8a 86  96 cb 56 64  d9 6c 64 19
|   ea e3 2e da
| received encrypted packet from 192.1.2.45:500
| decrypting 400 bytes using algorithm OAKLEY_AES_CBC
| decrypted:
|   01 00 00 18  2c 96 f3 3e  d4 c1 37 64  13 8b 49 11
|   ec f4 fc c4  99 31 4b 9a  0a 00 00 34  00 00 00 01
|   00 00 00 01  00 00 00 28  00 03 04 01  08 e4 af 15
|   00 00 00 1c  00 03 00 00  80 03 00 0e  80 04 00 01
|   80 01 00 01  80 02 70 80  80 05 00 01  04 00 00 14
|   8b ff 7a 2a  93 76 17 ba  6f 4a 91 10  49 46 b9 06
|   05 00 01 04  b5 b5 e0 9f  03 49 01 f7  cd ed db a0
|   76 38 65 1e  cb ef bd 16  44 47 5d d8  83 b3 bd eb
|   bc 4a 65 a7  61 e6 c3 ac  54 a2 3e a8  71 67 52 a0
|   a2 11 7c ed  66 fd 18 44  6c a0 3a 1a  1b 62 42 c6
|   a4 24 ed 96  d5 e6 e8 ad  6f 0b e8 68  b7 08 38 ad
|   c7 83 dc 20  6a 9c 3a 05  3a d6 0b 78  79 a1 db 4c
|   18 4a 8b cd  70 9c 2e db  d7 46 a3 58  18 a1 fd ac
|   37 e5 88 c9  9e d5 b8 3c  3c 27 8d 2e  31 97 cf 60
|   b1 e1 f9 41  16 c0 b7 60  71 c2 8d 29  14 74 00 ad
|   89 2b d3 28  47 a1 84 a7  03 50 be 8d  cb b9 8b c0
|   3b bb 58 c0  e8 df c6 44  21 cf cf 75  2a 51 98 a4
|   47 68 ba d8  14 8e 07 b1  d3 50 8c ec  bd 1d 0f 7a
|   05 3b 0c 7a  3d 53 85 d4  25 ad 69 43  b2 f1 c1 7d
|   1b b7 e3 ae  04 dd f2 a8  ec 8f f1 52  72 72 e0 d7
|   37 79 4f 6c  8d 8c 55 6b  53 1f c6 d3  02 5f 98 b9
|   0f 08 e3 06  c5 e9 af 18  e0 15 e7 31  72 f5 04 dc
|   98 49 d2 bf  05 00 00 10  04 00 00 00  c0 00 01 00
|   ff ff ff 00  00 00 00 10  04 00 00 00  c0 00 02 00
|   ff ff ff 00  00 00 00 00  00 00 00 00  00 00 00 00
| next IV:  ee d6 e2 18  6a 0c 22 e5  b4 ab c6 36  7e 3c b8 aa
| HASH(1) computed:
|   2c 96 f3 3e  d4 c1 37 64  13 8b 49 11  ec f4 fc c4
|   99 31 4b 9a
| peer client is subnet 192.0.1.0/24
| peer client protocol/port is 0/0
| our client is subnet 192.0.2.0/24
| our client protocol/port is 0/0
"westnet-eastnet" #1: the peer proposed: 192.0.2.0/24:0/0 -> 192.0.1.0/24:0/0
| find_client_connection starting with westnet-eastnet
|   looking for 192.0.2.0/24:0/0 -> 192.0.1.0/24:0/0
|   concrete checking against sr#0 192.0.2.0/24 -> 192.0.1.0/24
|    match_id a=@west
|             b=@west
|    results  matched
|   trusted_ca called with a=(empty) b=(empty)
|   fc_try trying westnet-eastnet:192.0.2.0/24:0/0 -> 192.0.1.0/24:0/0 vs westnet-eastnet:192.0.2.0/24:0/0 -> 192.0.1.0/24:0/0
|   fc_try concluding with westnet-eastnet [128]
|   fc_try westnet-eastnet gives westnet-eastnet
|   concluding with d = westnet-eastnet
| duplicating state object #1
| creating state object #2 at 0x8151690
| processing connection westnet-eastnet
| ICOOKIE:  64 87 18 2d  ee 7c ff fb
| RCOOKIE:  75 7b 48 54  0a 79 92 ea
| state hash entry 11
| inserting state object #2 on chain 11
| inserting event EVENT_SO_DISCARD, timeout in 0 seconds for #2
| DH public value received:
|   b5 b5 e0 9f  03 49 01 f7  cd ed db a0  76 38 65 1e
|   cb ef bd 16  44 47 5d d8  83 b3 bd eb  bc 4a 65 a7
|   61 e6 c3 ac  54 a2 3e a8  71 67 52 a0  a2 11 7c ed
|   66 fd 18 44  6c a0 3a 1a  1b 62 42 c6  a4 24 ed 96
|   d5 e6 e8 ad  6f 0b e8 68  b7 08 38 ad  c7 83 dc 20
|   6a 9c 3a 05  3a d6 0b 78  79 a1 db 4c  18 4a 8b cd
|   70 9c 2e db  d7 46 a3 58  18 a1 fd ac  37 e5 88 c9
|   9e d5 b8 3c  3c 27 8d 2e  31 97 cf 60  b1 e1 f9 41
|   16 c0 b7 60  71 c2 8d 29  14 74 00 ad  89 2b d3 28
|   47 a1 84 a7  03 50 be 8d  cb b9 8b c0  3b bb 58 c0
|   e8 df c6 44  21 cf cf 75  2a 51 98 a4  47 68 ba d8
|   14 8e 07 b1  d3 50 8c ec  bd 1d 0f 7a  05 3b 0c 7a
|   3d 53 85 d4  25 ad 69 43  b2 f1 c1 7d  1b b7 e3 ae
|   04 dd f2 a8  ec 8f f1 52  72 72 e0 d7  37 79 4f 6c
|   8d 8c 55 6b  53 1f c6 d3  02 5f 98 b9  0f 08 e3 06
|   c5 e9 af 18  e0 15 e7 31  72 f5 04 dc  98 49 d2 bf
| 0: w->pcw_dead: 0 w->pcw_work: 0 cnt: 1
| asking helper 0 to do build_kenonce op on seq: 3 (len=2668, pcw_work=1)
| crypto helper write of request: cnt=2668<wlen=2668.  
| inserting event EVENT_CRYPTO_FAILED, timeout in 300 seconds for #2
| complete state transition with STF_SUSPEND
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 54 seconds
|  
| helper 0 has finished work (cnt now 1)
| helper 0 replies to id: q#3
| calling callback function 0x8072677
| quick inI1_outR1: calculated ke+nonce, calculating DH
| processing connection westnet-eastnet
| started looking for secret for @east->@west of kind PPK_PSK
| actually looking for secret for @east->@west of kind PPK_PSK
| line 8: key type PPK_PSK(@east) to type PPK_RSA 
| concluding with best_match=0 best=(nil) (lineno=-1)
| 0: w->pcw_dead: 0 w->pcw_work: 0 cnt: 1
| asking helper 0 to do compute dh(p2) op on seq: 4 (len=2668, pcw_work=1)
| crypto helper write of request: cnt=2668<wlen=2668.  
| inserting event EVENT_CRYPTO_FAILED, timeout in 300 seconds for #2
| * processed 1 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 54 seconds
|  
| helper 0 has finished work (cnt now 1)
| helper 0 replies to id: q#4
| calling callback function 0x8072946
| quick inI1_outR1: calculated DH, sending R1
| processing connection westnet-eastnet
"westnet-eastnet" #2: responding to Quick Mode {msgid:b41681c5}
| HASH(2) computed:
|   5b 3d 30 c0  dd 28 5f bf  c3 64 21 1e  b8 b0 a6 98
|   a7 eb 91 64
| ESP KEYMAT 
|   KEYMAT computed:
|   65 d0 94 fd  d2 72 44 0f  23 f4 9c ca  23 8b b4 53
|   8b d6 89 b6  ab 42 5b 1b  a9 69 66 30  ea 84 07 f4
|   3a 52 76 ef  48 ca df 62
|   Peer KEYMAT computed:
|   52 ce b2 09  41 72 22 45  3b 7b 3a 2a  02 e2 7d 56
|   87 c4 e6 2e  11 c7 e9 13  1f 51 31 b9  91 f7 f2 df
|   8c 07 be 36  ff b9 86 2d
| route owner of "westnet-eastnet" unrouted: NULL
| install_inbound_ipsec_sa() checking if we can route
| route owner of "westnet-eastnet" unrouted: NULL; eroute owner: NULL
| could_route called for westnet-eastnet (kind=CK_PERMANENT)
| looking for alg with transid: 3 keylen: 0 auth: 1 
| checking transid: 11 keylen: 0 auth: 1 
| checking transid: 11 keylen: 0 auth: 2 
| checking transid: 2 keylen: 8 auth: 0 
| checking transid: 2 keylen: 8 auth: 1 
| checking transid: 2 keylen: 8 auth: 2 
| checking transid: 3 keylen: 24 auth: 0 
| checking transid: 3 keylen: 24 auth: 1 
| looking for alg with transid: 3 keylen: 0 auth: 1 
| checking transid: 11 keylen: 0 auth: 1 
| checking transid: 11 keylen: 0 auth: 2 
| checking transid: 2 keylen: 8 auth: 0 
| checking transid: 2 keylen: 8 auth: 1 
| checking transid: 2 keylen: 8 auth: 2 
| checking transid: 3 keylen: 24 auth: 0 
| checking transid: 3 keylen: 24 auth: 1 
| add inbound eroute 192.0.1.0/24:0 --0-> 192.0.2.0/24:0 => tun.10000@192.1.2.23 (raw_eroute)
| raw_eroute result=1 
| encrypting:
|   01 00 00 18  5b 3d 30 c0  dd 28 5f bf  c3 64 21 1e
|   b8 b0 a6 98  a7 eb 91 64  0a 00 00 34  00 00 00 01
|   00 00 00 01  00 00 00 28  00 03 04 01  6e 20 ef 9a
|   00 00 00 1c  00 03 00 00  80 03 00 0e  80 04 00 01
|   80 01 00 01  80 02 70 80  80 05 00 01  04 00 00 14
|   da 84 6a e3  ed 3e c7 f9  a9 d2 51 9c  70 c7 79 0a
|   05 00 01 04  a5 a5 b7 29  fd 47 0d 6d  0f bc 7d d4
|   c1 2c 73 31  a0 23 c8 3d  9d 60 7c a7  30 42 62 c8
|   c5 f6 1d 43  74 3c 9d ba  6b 69 7a 38  92 cd d0 3d
|   6c 88 ca 7b  f0 76 a9 a3  2c ee 63 55  39 24 75 cb
|   37 5b 9f 8f  2c 9c 24 48  85 d9 d0 22  13 db 74 72
|   84 c4 1f 23  78 18 09 ff  4f e9 07 e3  8a 8a 8e 11
|   a2 03 7f 72  99 c3 bc f4  4e 1d 16 1c  61 16 83 e9
|   2f 51 74 12  2f 8e e2 84  1e 09 05 58  d2 ee 48 b0
|   3e 0e 8e 9e  ad 11 b0 16  9e ea 30 c5  7e 53 e1 9d
|   3a 90 d3 7e  d2 db 4c 73  10 0d da d3  da 6f c6 67
|   97 c6 41 e3  9e 1b 41 35  5b 75 52 78  10 0b ac 05
|   ca 8b 62 02  2b f1 d5 1a  65 b7 8a e8  18 e1 aa 0f
|   e6 2e a4 6e  79 6b 48 2c  ab 03 3a f9  bd 7b 2a dd
|   e2 1c 76 a3  06 ba 2a 6b  00 ee e6 46  e1 37 ba aa
|   2b e1 bd e6  d1 f1 4d 91  34 29 24 a9  62 1d 2b 99
|   95 67 df d3  97 c1 cc 80  da a2 9c 63  13 eb ca 5c
|   fb 7e d0 ad  05 00 00 10  04 00 00 00  c0 00 01 00
|   ff ff ff 00  00 00 00 10  04 00 00 00  c0 00 02 00
|   ff ff ff 00
| IV:
|   ee d6 e2 18  6a 0c 22 e5  b4 ab c6 36  7e 3c b8 aa
| unpadded size is: 388
| encrypting 400 using OAKLEY_AES_CBC
| next IV:  fc c3 d1 c9  79 f2 6d 30  57 fc 15 5a  8b 9d 0e 49
| finished processing quick inI1
| complete state transition with STF_OK
"westnet-eastnet" #2: transition from state STATE_QUICK_R0 to state STATE_QUICK_R1
| sending reply packet to 192.1.2.45:500 (from port 500)
| sending 428 bytes for STATE_QUICK_R0 through eth1:500 to 192.1.2.45:500 (using #2)
| inserting event EVENT_RETRANSMIT, timeout in 10 seconds for #2
"westnet-eastnet" #2: STATE_QUICK_R1: sent QR1, inbound IPsec SA installed, expecting QI2
| modecfg pull: noquirk policy:push not-client
| phase 1 is done, looking for phase 2 to unpend
| * processed 1 messages from cryptographic helpers 
| next event EVENT_RETRANSMIT in 10 seconds for #2
|  
| *received 60 bytes from 192.1.2.45:500 on eth1 (port=500)
|  processing version=1.0 packet with exchange type=ISAKMP_XCHG_QUICK (32)
| ICOOKIE:  64 87 18 2d  ee 7c ff fb
| RCOOKIE:  75 7b 48 54  0a 79 92 ea
| state hash entry 11
| v1 peer and cookies match on #2, provided msgid c58116b4 vs c58116b4
| v1 state object #2 found, in STATE_QUICK_R1
| processing connection westnet-eastnet
| received encrypted packet from 192.1.2.45:500
| decrypting 32 bytes using algorithm OAKLEY_AES_CBC
| decrypted:
|   00 00 00 18  2b e4 39 e9  d3 07 c4 54  81 52 53 96
|   5f 40 02 5f  89 c4 87 a9  00 00 00 00  00 00 00 00
| next IV:  38 22 eb d4  df dd 42 12  cd 30 06 3d  eb 38 0f 44
| HASH(3) computed:  2b e4 39 e9  d3 07 c4 54  81 52 53 96  5f 40 02 5f
| HASH(3) computed:  89 c4 87 a9
| install_ipsec_sa() for #2: outbound only
| route owner of "westnet-eastnet" unrouted: NULL; eroute owner: NULL
| could_route called for westnet-eastnet (kind=CK_PERMANENT)
| sr for #2: unrouted
| route owner of "westnet-eastnet" unrouted: NULL; eroute owner: NULL
| route_and_eroute with c: westnet-eastnet (next: none) ero:null esr:{(nil)} ro:null rosr:{(nil)} and state: 2
| eroute_connection add eroute 192.0.2.0/24:0 --0-> 192.0.1.0/24:0 => tun.0@192.1.2.45 (raw_eroute)
| raw_eroute result=1 
| command executing up-client
|   trusted_ca called with a=(empty) b=(empty)
| executing up-client: 2>&1 PLUTO_VERSION='2.0' PLUTO_VERB='up-client' PLUTO_CONNECTION='westnet-eastnet' PLUTO_NEXT_HOP='192.1.2.45' PLUTO_INTERFACE='eth1' PLUTO_ME='192.1.2.23' PLUTO_MY_ID='@east' PLUTO_MY_CLIENT='192.0.2.0/24' PLUTO_MY_CLIENT_NET='192.0.2.0' PLUTO_MY_CLIENT_MASK='255.255.255.0' PLUTO_MY_PORT='0' PLUTO_MY_PROTOCOL='0' PLUTO_PEER='192.1.2.45' PLUTO_PEER_ID='@west' PLUTO_PEER_CLIENT='192.0.1.0/24' PLUTO_PEER_CLIENT_NET='192.0.1.0' PLUTO_PEER_CLIENT_MASK='255.255.255.0' PLUTO_PEER_PORT='0' PLUTO_PEER_PROTOCOL='0' PLUTO_PEER_CA='' PLUTO_STACK='netkey' PLUTO_CONN_POLICY='RSASIG+ENCRYPT+TUNNEL+PFS+IKEv2ALLOW' PLUTO_XAUTH_USERNAME=''  ipsec _updown
| route_and_eroute: firewall_notified: true
| command executing prepare-client
|   trusted_ca called with a=(empty) b=(empty)
| executing prepare-client: 2>&1 PLUTO_VERSION='2.0' PLUTO_VERB='prepare-client' PLUTO_CONNECTION='westnet-eastnet' PLUTO_NEXT_HOP='192.1.2.45' PLUTO_INTERFACE='eth1' PLUTO_ME='192.1.2.23' PLUTO_MY_ID='@east' PLUTO_MY_CLIENT='192.0.2.0/24' PLUTO_MY_CLIENT_NET='192.0.2.0' PLUTO_MY_CLIENT_MASK='255.255.255.0' PLUTO_MY_PORT='0' PLUTO_MY_PROTOCOL='0' PLUTO_PEER='192.1.2.45' PLUTO_PEER_ID='@west' PLUTO_PEER_CLIENT='192.0.1.0/24' PLUTO_PEER_CLIENT_NET='192.0.1.0' PLUTO_PEER_CLIENT_MASK='255.255.255.0' PLUTO_PEER_PORT='0' PLUTO_PEER_PROTOCOL='0' PLUTO_PEER_CA='' PLUTO_STACK='netkey' PLUTO_CONN_POLICY='RSASIG+ENCRYPT+TUNNEL+PFS+IKEv2ALLOW' PLUTO_XAUTH_USERNAME=''  ipsec _updown
| command executing route-client
|   trusted_ca called with a=(empty) b=(empty)
| executing route-client: 2>&1 PLUTO_VERSION='2.0' PLUTO_VERB='route-client' PLUTO_CONNECTION='westnet-eastnet' PLUTO_NEXT_HOP='192.1.2.45' PLUTO_INTERFACE='eth1' PLUTO_ME='192.1.2.23' PLUTO_MY_ID='@east' PLUTO_MY_CLIENT='192.0.2.0/24' PLUTO_MY_CLIENT_NET='192.0.2.0' PLUTO_MY_CLIENT_MASK='255.255.255.0' PLUTO_MY_PORT='0' PLUTO_MY_PROTOCOL='0' PLUTO_PEER='192.1.2.45' PLUTO_PEER_ID='@west' PLUTO_PEER_CLIENT='192.0.1.0/24' PLUTO_PEER_CLIENT_NET='192.0.1.0' PLUTO_PEER_CLIENT_MASK='255.255.255.0' PLUTO_PEER_PORT='0' PLUTO_PEER_PROTOCOL='0' PLUTO_PEER_CA='' PLUTO_STACK='netkey' PLUTO_CONN_POLICY='RSASIG+ENCRYPT+TUNNEL+PFS+IKEv2ALLOW' PLUTO_XAUTH_USERNAME=''  ipsec _updown
| route_and_eroute: instance "westnet-eastnet", setting eroute_owner {spd=0x8142740,sr=0x8142740} to #2 (was #0) (newest_ipsec_sa=#0)
| inI2: instance westnet-eastnet[0], setting newest_ipsec_sa to #2 (was #0) (spd.eroute=#2)
| complete state transition with STF_OK
"westnet-eastnet" #2: transition from state STATE_QUICK_R1 to state STATE_QUICK_R2
| inserting event EVENT_SA_REPLACE, timeout in 28530 seconds for #2
"westnet-eastnet" #2: STATE_QUICK_R2: IPsec SA established tunnel mode {ESP=>0x08e4af15 <0x6e20ef9a xfrm=3DES_0-HMAC_MD5 NATOA=<invalid> NATD=<invalid>:500 DPD=enabled}
| modecfg pull: noquirk policy:push not-client
| phase 1 is done, looking for phase 2 to unpend
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 53 seconds
|  
| *received 76 bytes from 192.1.2.45:500 on eth1 (port=500)
|  processing version=1.0 packet with exchange type=ISAKMP_XCHG_INFO (5)
| ICOOKIE:  64 87 18 2d  ee 7c ff fb
| RCOOKIE:  75 7b 48 54  0a 79 92 ea
| state hash entry 11
| peer and cookies match on #2, provided msgid 00000000 vs c58116b4/00000000
| peer and cookies match on #1, provided msgid 00000000 vs 00000000/00000000
| p15 state object #1 found, in STATE_MAIN_R3
| processing connection westnet-eastnet
| last Phase 1 IV:  65 38 7f d7  47 6d 4f 56  db 39 5d 6a  c8 f6 d4 e2
| current Phase 1 IV:  65 38 7f d7  47 6d 4f 56  db 39 5d 6a  c8 f6 d4 e2
| computed Phase 2 IV:
|   2b cd 70 50  51 c1 b7 81  96 1b 71 5c  d4 84 48 f9
|   cf 0d 54 ae
| received encrypted packet from 192.1.2.45:500
| decrypting 48 bytes using algorithm OAKLEY_AES_CBC
| decrypted:
|   0c 00 00 18  1f 16 2c 6a  a8 4b f9 3a  a8 38 e4 fe
|   0d 75 65 2f  ac d5 45 8c  00 00 00 10  00 00 00 01
|   03 04 00 01  08 e4 af 15  00 00 00 00  00 00 00 00
| next IV:  7f 05 67 58  5d 10 d7 c2  52 4a 7c ed  87 3a 9d 93
| processing connection westnet-eastnet
"westnet-eastnet" #1: received Delete SA(0x08e4af15) payload: deleting IPSEC State #2
| deleting state #2
| processing connection westnet-eastnet
| HASH(1) computed:
|   7d 8c 3e be  ee 70 62 d3  e1 ee 70 de  00 55 aa 87
|   d9 5f 89 17
| last Phase 1 IV:  65 38 7f d7  47 6d 4f 56  db 39 5d 6a  c8 f6 d4 e2
| current Phase 1 IV:  65 38 7f d7  47 6d 4f 56  db 39 5d 6a  c8 f6 d4 e2
| computed Phase 2 IV:
|   ef 35 0f c7  60 d2 c4 d7  ed 6d 15 66  bd 82 e0 15
|   b6 37 6c c3
| encrypting:
|   0c 00 00 18  7d 8c 3e be  ee 70 62 d3  e1 ee 70 de
|   00 55 aa 87  d9 5f 89 17  00 00 00 10  00 00 00 01
|   03 04 00 01  6e 20 ef 9a
| IV:
|   ef 35 0f c7  60 d2 c4 d7  ed 6d 15 66  bd 82 e0 15
|   b6 37 6c c3
| unpadded size is: 40
| encrypting 48 using OAKLEY_AES_CBC
| next IV:  24 ca f3 e8  73 57 21 d2  a0 9e a1 72  bd 23 b5 3a
| sending 76 bytes for delete notify through eth1:500 to 192.1.2.45:500 (using #1)
| no suspended cryptographic state for 2 
| ICOOKIE:  64 87 18 2d  ee 7c ff fb
| RCOOKIE:  75 7b 48 54  0a 79 92 ea
| state hash entry 11
| command executing down-client
|   trusted_ca called with a=(empty) b=(empty)
| executing down-client: 2>&1 PLUTO_VERSION='2.0' PLUTO_VERB='down-client' PLUTO_CONNECTION='westnet-eastnet' PLUTO_NEXT_HOP='192.1.2.45' PLUTO_INTERFACE='eth1' PLUTO_ME='192.1.2.23' PLUTO_MY_ID='@east' PLUTO_MY_CLIENT='192.0.2.0/24' PLUTO_MY_CLIENT_NET='192.0.2.0' PLUTO_MY_CLIENT_MASK='255.255.255.0' PLUTO_MY_PORT='0' PLUTO_MY_PROTOCOL='0' PLUTO_PEER='192.1.2.45' PLUTO_PEER_ID='@west' PLUTO_PEER_CLIENT='192.0.1.0/24' PLUTO_PEER_CLIENT_NET='192.0.1.0' PLUTO_PEER_CLIENT_MASK='255.255.255.0' PLUTO_PEER_PORT='0' PLUTO_PEER_PROTOCOL='0' PLUTO_PEER_CA='' PLUTO_STACK='netkey' PLUTO_CONN_POLICY='RSASIG+ENCRYPT+TUNNEL+PFS+IKEv2ALLOW' PLUTO_XAUTH_USERNAME=''  ipsec _updown
"westnet-eastnet" #2: request to replace with shunt a prospective erouted policy with netkey kernel --- not yet implemented
| delete inbound eroute 192.0.1.0/24:0 --0-> 192.0.2.0/24:0 => unk255.10000@192.1.2.23 (raw_eroute)
| raw_eroute result=1 
"westnet-eastnet" #1: received and ignored informational message
| complete state transition with STF_IGNORE
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 52 seconds
|  
| *received 92 bytes from 192.1.2.45:500 on eth1 (port=500)
|  processing version=1.0 packet with exchange type=ISAKMP_XCHG_INFO (5)
| ICOOKIE:  64 87 18 2d  ee 7c ff fb
| RCOOKIE:  75 7b 48 54  0a 79 92 ea
| state hash entry 11
| peer and cookies match on #1, provided msgid 00000000 vs 00000000/00000000
| p15 state object #1 found, in STATE_MAIN_R3
| processing connection westnet-eastnet
| last Phase 1 IV:  65 38 7f d7  47 6d 4f 56  db 39 5d 6a  c8 f6 d4 e2
| current Phase 1 IV:  65 38 7f d7  47 6d 4f 56  db 39 5d 6a  c8 f6 d4 e2
| computed Phase 2 IV:
|   06 96 2a 54  2b ea 36 c4  08 ad d0 2a  fe c1 38 36
|   04 85 d7 a4
| received encrypted packet from 192.1.2.45:500
| decrypting 64 bytes using algorithm OAKLEY_AES_CBC
| decrypted:
|   0c 00 00 18  94 b9 57 6f  48 87 6d 06  63 08 ac e6
|   ff ea f8 80  08 25 2c 7a  00 00 00 1c  00 00 00 01
|   01 10 00 01  64 87 18 2d  ee 7c ff fb  75 7b 48 54
|   0a 79 92 ea  00 00 00 00  00 00 00 00  00 00 00 00
| next IV:  7d e7 7f c6  c7 7b 99 73  a3 41 43 0c  68 4b 6a bc
| ICOOKIE:  64 87 18 2d  ee 7c ff fb
| RCOOKIE:  75 7b 48 54  0a 79 92 ea
| state hash entry 11
| v1 peer and cookies match on #1, provided msgid 00000000 vs 00000000
| v1 state object #1 found, in STATE_MAIN_R3
| processing connection westnet-eastnet
"westnet-eastnet" #1: received Delete SA payload: deleting ISAKMP State #1
| deleting state #1
| processing connection westnet-eastnet
| HASH(1) computed:
|   61 23 57 4f  67 3a 5e 1b  8a 02 95 0c  25 67 49 81
|   a3 b1 e2 a3
| last Phase 1 IV:  65 38 7f d7  47 6d 4f 56  db 39 5d 6a  c8 f6 d4 e2
| current Phase 1 IV:  65 38 7f d7  47 6d 4f 56  db 39 5d 6a  c8 f6 d4 e2
| computed Phase 2 IV:
|   46 3b 32 52  1d f0 b7 58  1a 85 4a 63  12 0e 5e 4e
|   72 58 31 4c
| encrypting:
|   0c 00 00 18  61 23 57 4f  67 3a 5e 1b  8a 02 95 0c
|   25 67 49 81  a3 b1 e2 a3  00 00 00 1c  00 00 00 01
|   01 10 00 01  64 87 18 2d  ee 7c ff fb  75 7b 48 54
|   0a 79 92 ea
| IV:
|   46 3b 32 52  1d f0 b7 58  1a 85 4a 63  12 0e 5e 4e
|   72 58 31 4c
| unpadded size is: 52
| encrypting 64 using OAKLEY_AES_CBC
| next IV:  b1 3e d0 11  90 f2 e9 f4  fd aa 4d 7a  62 09 b6 dd
| sending 92 bytes for delete notify through eth1:500 to 192.1.2.45:500 (using #1)
| no suspended cryptographic state for 1 
| ICOOKIE:  64 87 18 2d  ee 7c ff fb
| RCOOKIE:  75 7b 48 54  0a 79 92 ea
| state hash entry 11
| unreference key: 0x8141c60 @west cnt 2--
packet from 192.1.2.45:500: received and ignored informational message
| complete state transition with STF_IGNORE
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 52 seconds
|  
| *received kernel message
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 49 seconds
|  
| *received whack message
| kernel_alg_esp_auth_keylen(auth=1, sadb_aalg=2): a_keylen=16
| * processed 0 messages from cryptographic helpers 
| next event EVENT_PENDING_PHASE2 in 45 seconds
east:~# : ==== tuc ====
east:~# if [ -f /tmp/core ]; then echo CORE FOUND; mv /tmp/core /var/tmp; fi
east:~# : ==== end ====
east:~# ipsec setup stop
ipsec_setup: Stopping Openswan IPsec...
east:~# kill `cat /var/run/klogd.pid`; cat /tmp/klog.log
klogd 1.3-3#33.1, log source = /proc/kmsg started.
<5>Linux version 2.6.18.6 (antony@sal) (gcc version 4.2.3 20080114 (prerelease) (Debian 4.2.2-7)) #6 Wed Feb 13 11:18:26 EST 2008
<7>On node 0 totalpages: 8192
<7>  DMA zone: 8192 pages, LIFO batch:1
<4>Built 1 zonelists.  Total pages: 8192
<5>Kernel command line: initrd=/btmp/antony/ikev2/2008_01_14/UMLPOOL/initrd.uml umlroot=/btmp/antony/ikev2/2008_01_14/UMLPOOL/east/root root=/dev/ram0 rw ssl=pty eth0=daemon,10:00:00:dc:bc:ff,unix,/tmp/umljZyuOz.d/east/ctl,/tmp/umljZyuOz.d/east/data eth1=daemon,10:00:00:64:64:23,unix,/tmp/umljZyuOz.d/public/ctl,/tmp/umljZyuOz.d/public/data eth2=daemon,10:00:00:32:64:23,unix,/tmp/umljZyuOz.d/admin/ctl,/tmp/umljZyuOz.d/admin/data init=/linuxrc single
<4>PID hash table entries: 256 (order: 8, 1024 bytes)
<4>Dentry cache hash table entries: 4096 (order: 2, 16384 bytes)
<4>Inode-cache hash table entries: 2048 (order: 1, 8192 bytes)
<6>Memory: 27028k available
<7>Calibrating delay loop... 2949.12 BogoMIPS (lpj=14745600)
<4>Mount-cache hash table entries: 512
<4>Checking for host processor cmov support...Yes
<4>Checking for host processor xmm support...No
<4>Checking that host ptys support output SIGIO...Yes
<4>Checking that host ptys support SIGIO on close...No, enabling workaround
<6>checking if image is initramfs...it isn't (bad gzip magic numbers); looks like an initrd
<4>Freeing initrd memory: 1212k freed
<4>Using 2.6 host AIO
<6>NET: Registered protocol family 16
<6>NET: Registered protocol family 2
<4>IP route cache hash table entries: 256 (order: -2, 1024 bytes)
<4>TCP established hash table entries: 1024 (order: 0, 4096 bytes)
<4>TCP bind hash table entries: 512 (order: -1, 2048 bytes)
<6>TCP: Hash tables configured (established 1024 bind 512)
<6>TCP reno registered
<4>daemon_setup : Ignoring data socket specification
<6>Netdevice 0 (10:00:00:dc:bc:ff) : daemon backend (uml_switch version 3) - unix:/tmp/umljZyuOz.d/east/ctl
<4>daemon_setup : Ignoring data socket specification
<6>Netdevice 1 (10:00:00:64:64:23) : daemon backend (uml_switch version 3) - unix:/tmp/umljZyuOz.d/public/ctl
<4>daemon_setup : Ignoring data socket specification
<6>Netdevice 2 (10:00:00:32:64:23) : daemon backend (uml_switch version 3) - unix:/tmp/umljZyuOz.d/admin/ctl
<4>Checking host MADV_REMOVE support...OK
<4>mconsole (version 2) initialized on /home/antony/.uml/east/mconsole
<6>Host TLS support detected
<6>Detected host type: i386
<5>VFS: Disk quotas dquot_6.5.1
<4>Dquot-cache hash table entries: 1024 (order 0, 4096 bytes)
<6>Initializing Cryptographic API
<6>io scheduler noop registered
<6>io scheduler anticipatory registered (default)
<6>io scheduler deadline registered
<6>io scheduler cfq registered
<4>RAMDISK driver initialized: 16 RAM disks of 4096K size 1024 blocksize
<6>loop: loaded (max 8 devices)
<6>nbd: registered device at major 43
<6>PPP generic driver version 2.4.2
<6>SLIP: version 0.8.4-NET3.019-NEWTTY (dynamic channels, max=256).
<6>tun: Universal TUN/TAP device driver, 1.6
<6>tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>
<4>Netfilter messages via NETLINK v0.30.
<6>IPv4 over IPv4 tunneling driver
<6>GRE over IPv4 tunneling driver
<4>ip_conntrack version 2.4 (211 buckets, 1688 max) - 224 bytes per conntrack
<4>ctnetlink v0.90: registering with nfnetlink.
<4>ip_conntrack_pptp version 3.1 loaded
<4>ip_nat_pptp version 3.0 loaded
<4>ip_tables: (C) 2000-2006 Netfilter Core Team
<5>ClusterIP Version 0.8 loaded successfully
<4>arp_tables: (C) 2002 David S. Miller
<6>TCP bic registered
<6>TCP westwood registered
<6>TCP highspeed registered
<6>TCP hybla registered
<6>TCP htcp registered
<6>TCP vegas registered
<6>TCP scalable registered
<6>Initializing IPsec netlink socket
<6>NET: Registered protocol family 1
<6>NET: Registered protocol family 17
<6>NET: Registered protocol family 15
<6>Initialized stdio console driver
<4>Console initialized on /dev/tty0
<6>Initializing software serial port version 1
<4>Failed to open 'root_fs', errno = 2
<5>RAMDISK: cramfs filesystem found at block 0
<5>RAMDISK: Loading 1212KiB [1 disk] into ram disk... |/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\|/-\done.
<4>VFS: Mounted root (cramfs filesystem) readonly.
<6>line_ioctl: tty0: ioctl KDSIGACCEPT called
east:~# halt -p -f
System halted.

