west:~#
 TESTNAME=pluto-algo-01
west:~#
 source /testing/pluto/bin/westlocal.sh
west:~#
 ipsec setup start
ipsec_setup: Starting Openswan IPsec VERSION
west:~#
 ipsec auto --add westnet-eastnet-cross
west:~#
 /testing/pluto/bin/wait-until-pluto-started
west:~#
 ipsec auto --up  westnet-eastnet-cross
104 "westnet-eastnet-cross" #1: STATE_MAIN_I1: initiate
003 "westnet-eastnet-cross" #1: received Vendor ID payload [Openswan 
003 "westnet-eastnet-cross" #1: received Vendor ID payload [Dead Peer Detection]
106 "westnet-eastnet-cross" #1: STATE_MAIN_I2: sent MI2, expecting MR2
108 "westnet-eastnet-cross" #1: STATE_MAIN_I3: sent MI3, expecting MR3
004 "westnet-eastnet-cross" #1: STATE_MAIN_I4: ISAKMP SA established {auth=OAKLEY_RSA_SIG cipher=oakley_3des_cbc_192 prf=oakley_md5 group=modp1536}
117 "westnet-eastnet-cross" #2: STATE_QUICK_I1: initiate
004 "westnet-eastnet-cross" #2: STATE_QUICK_I2: sent QI2, IPsec SA established tunnel mode
west:~#
 echo done
done
west:~#
 ipsec look
west NOW
192.0.1.0/24       -> 192.0.2.0/24       => tun0xIPIP@192.1.2.23 esp0xESPSPI@192.1.2.23
ipsec0->eth1 mtu=16260(9999)->1500
tun0xTUN#@192.1.2.23 IPIP: dir=out src=192.1.2.45 natencap=none natsport=0 natdport=0  
esp0xKLIPSPIK@192.1.2.23 ESP_3DES_HMAC_SHA1: dir=out src=192.1.2.45 iv_bits=64bits iv=0xIVISFORRANDOM000 ooowin=64 alen=160 aklen=160 eklen=192 natencap=none natsport=0 natdport=0  
esp0xKLIPSPIK@192.1.2.45 ESP_3DES_HMAC_SHA1: dir=in  src=192.1.2.23 iv_bits=64bits iv=0xIVISFORRANDOM000 ooowin=64 alen=160 aklen=160 eklen=192 natencap=none natsport=0 natdport=0  
tun0xTUN#@192.1.2.45 IPIP: dir=in  src=192.1.2.23 policy=192.0.2.0/24->192.0.1.0/24 flags=0x8<> natencap=none natsport=0 natdport=0  
ROUTING TABLE
192.1.2.0/24 dev eth1  proto kernel  scope link  src 192.1.2.45 
192.1.2.0/24 dev ipsec0  proto kernel  scope link  src 192.1.2.45 
192.0.2.0/24 dev ipsec0  scope link 
default via 192.1.2.254 dev eth1 
west:~#
 echo done
done
west:~#
 

west:~#
 ipsec look
west NOW
192.0.1.0/24       -> 192.0.2.0/24       => tun0xIPIP@192.1.2.23 esp0xESPSPI@192.1.2.23
ipsec0->eth1 mtu=16260(9999)->1500
tun0xTUN#@192.1.2.23 IPIP: dir=out src=192.1.2.45 natencap=none natsport=0 natdport=0  
esp0xKLIPSPIK@192.1.2.23 ESP_3DES_HMAC_SHA1: dir=out src=192.1.2.45 iv_bits=64bits iv=0xIVISFORRANDOM000 ooowin=64 alen=160 aklen=160 eklen=192 natencap=none natsport=0 natdport=0  
tun0xTUN#@192.1.2.23 IPIP: dir=out src=192.1.2.45 natencap=none natsport=0 natdport=0  
esp0xKLIPSPIK@192.1.2.23 ESP_3DES_HMAC_SHA1: dir=out src=192.1.2.45 iv_bits=64bits iv=0xIVISFORRANDOM000 ooowin=64 alen=160 aklen=160 eklen=192 natencap=none natsport=0 natdport=0  
esp0xKLIPSPIK@192.1.2.45 ESP_3DES_HMAC_SHA1: dir=in  src=192.1.2.23 iv_bits=64bits iv=0xIVISFORRANDOM000 ooowin=64   alen=160 aklen=160 eklen=192  natencap=none natsport=0 natdport=0  
tun0xTUN#@192.1.2.45 IPIP: dir=in  src=192.1.2.23 policy=192.0.2.0/24->192.0.1.0/24 flags=0x8<>  natencap=none natsport=0 natdport=0  
ROUTING TABLE
192.1.2.0/24 dev eth1  proto kernel  scope link  src 192.1.2.45 
192.1.2.0/24 dev ipsec0  proto kernel  scope link  src 192.1.2.45 
192.0.2.0/24 dev ipsec0  scope link 
default via 192.1.2.254 dev eth1 

