Virtual Electron Microscope Client

The EM Image

The EM-Image from instrument.

Input
Output

Mode
DL

Absolute coordinate

move x
move y
move z
tilt a

Brightnessset(0～200)

Voltageset (0～120kV)

Eucentric Height
max:
speed:
zshift:

TEM Control Command

The EM-control commandset.

Current condition

Position:
Magnificant:
Brightness:
Contrast:
Focus:
Voltage:

Set Lenz

C1:% C2:%
C3:% C4:%
Obj1:% Int1:%