mx51 "Babbage" evalutation board
Required root node properties:
    - compatible = "fsl,mx51-babbage", "fsl,mx51";

mx53 "Loco" evaluation board
Required root node properties:
    - compatible = "fsl,mx53-loco", "fsl,mx53";
