* Freescale 83xx and 512x PCI bridges

Freescale 83xx and 512x SOCs include the same pci bridge core.

83xx/512x specific notes:
- reg: should contain two address length tuples
    The first is for the internal pci bridge registers
    The second is for the pci config space access registers

Example (MPC8313ERDB)
	pci0: pci@e0008500 {
		cell-index = <1>;
		interrupt-map-mask = <0xf800 0x0 0x0 0x7>;
		interrupt-map = <
				/* IDSEL 0x0E -mini PCI */
				 0x7000 0x0 0x0 0x1 &ipic 18 0x8
				 0x7000 0x0 0x0 0x2 &ipic 18 0x8
				 0x7000 0x0 0x0 0x3 &ipic 18 0x8
				 0x7000 0x0 0x0 0x4 &ipic 18 0x8

				/* IDSEL 0x0F - PCI slot */
				 0x7800 0x0 0x0 0x1 &ipic 17 0x8
				 0x7800 0x0 0x0 0x2 &ipic 18 0x8
				 0x7800 0x0 0x0 0x3 &ipic 17 0x8
				 0x7800 0x0 0x0 0x4 &ipic 18 0x8>;
		interrupt-parent = <&ipic>;
		interrupts = <66 0x8>;
		bus-range = <0x0 0x0>;
		ranges = <0x02000000 0x0 0x90000000 0x90000000 0x0 0x10000000
			  0x42000000 0x0 0x80000000 0x80000000 0x0 0x10000000
			  0x01000000 0x0 0x00000000 0xe2000000 0x0 0x00100000>;
		clock-frequency = <66666666>;
		#interrupt-cells = <1>;
		#size-cells = <2>;
		#address-cells = <3>;
		reg = <0xe0008500 0x100		/* internal registers */
		       0xe0008300 0x8>;		/* config space access registers */
		compatible = "fsl,mpc8349-pci";
		device_type = "pci";
	};
