What:		/sys/bus/usb/devices/<busnum>-<devnum>:<config num>.<interface num>/<hid-bus>:<vendor-id>:<product-id>.<num>/kovaplus/roccatkovaplus<minor>/actual_cpi
Date:		January 2011
Contact:	Stefan Achatz <erazor_de@users.sourceforge.net>
Description:	The integer value of this attribute ranges from 1-4.
		When read, this attribute returns the number of the active
		cpi level.
		This file is readonly.
Users:		http://roccat.sourceforge.net

What:		/sys/bus/usb/devices/<busnum>-<devnum>:<config num>.<interface num>/<hid-bus>:<vendor-id>:<product-id>.<num>/kovaplus/roccatkovaplus<minor>/actual_profile
Date:		January 2011
Contact:	Stefan Achatz <erazor_de@users.sourceforge.net>
Description:	The integer value of this attribute ranges from 0-4.
		When read, this attribute returns the number of the active
		profile.
		When written, the mouse activates this profile immediately.
		The profile that's active when powered down is the same that's
		active when the mouse is powered on.
Users:		http://roccat.sourceforge.net

What:		/sys/bus/usb/devices/<busnum>-<devnum>:<config num>.<interface num>/<hid-bus>:<vendor-id>:<product-id>.<num>/kovaplus/roccatkovaplus<minor>/actual_sensitivity_x
Date:		January 2011
Contact:	Stefan Achatz <erazor_de@users.sourceforge.net>
Description:	The integer value of this attribute ranges from 1-10.
		When read, this attribute returns the number of the actual
		sensitivity in x direction.
		This file is readonly.
Users:		http://roccat.sourceforge.net

What:		/sys/bus/usb/devices/<busnum>-<devnum>:<config num>.<interface num>/<hid-bus>:<vendor-id>:<product-id>.<num>/kovaplus/roccatkovaplus<minor>/actual_sensitivity_y
Date:		January 2011
Contact:	Stefan Achatz <erazor_de@users.sourceforge.net>
Description:	The integer value of this attribute ranges from 1-10.
		When read, this attribute returns the number of the actual
		sensitivity in y direction.
		This file is readonly.
Users:		http://roccat.sourceforge.net

What:		/sys/bus/usb/devices/<busnum>-<devnum>:<config num>.<interface num>/<hid-bus>:<vendor-id>:<product-id>.<num>/kovaplus/roccatkovaplus<minor>/firmware_version
Date:		January 2011
Contact:	Stefan Achatz <erazor_de@users.sourceforge.net>
Description:	When read, this file returns the raw integer version number of the
		firmware reported by the mouse. Using the integer value eases
		further usage in other programs. To receive the real version
		number the decimal point has to be shifted 2 positions to the
		left. E.g. a returned value of 121 means 1.21
		This file is readonly.
Users:		http://roccat.sourceforge.net

What:		/sys/bus/usb/devices/<busnum>-<devnum>:<config num>.<interface num>/<hid-bus>:<vendor-id>:<product-id>.<num>/kovaplus/roccatkovaplus<minor>/profile_buttons
Date:		January 2011
Contact:	Stefan Achatz <erazor_de@users.sourceforge.net>
Description:	The mouse can store 5 profiles which can be switched by the
		press of a button. A profile is split in settings and buttons.
		profile_buttons holds information about button layout.
		When written, this file lets one write the respective profile
		buttons back to the mouse. The data has to be 23 bytes long.
		The mouse will reject invalid data.
		Which profile to write is determined by the profile number
		contained in the data.
		This file is writeonly.
Users:		http://roccat.sourceforge.net

What:		/sys/bus/usb/devices/<busnum>-<devnum>:<config num>.<interface num>/<hid-bus>:<vendor-id>:<product-id>.<num>/kovaplus/roccatkovaplus<minor>/profile[1-5]_buttons
Date:		January 2011
Contact:	Stefan Achatz <erazor_de@users.sourceforge.net>
Description:	The mouse can store 5 profiles which can be switched by the
		press of a button. A profile is split in settings and buttons.
		profile_buttons holds information about button layout.
		When read, these files return the respective profile buttons.
		The returned data is 23 bytes in size.
		This file is readonly.
Users:		http://roccat.sourceforge.net

What:		/sys/bus/usb/devices/<busnum>-<devnum>:<config num>.<interface num>/<hid-bus>:<vendor-id>:<product-id>.<num>/kovaplus/roccatkovaplus<minor>/profile_settings
Date:		January 2011
Contact:	Stefan Achatz <erazor_de@users.sourceforge.net>
Description:	The mouse can store 5 profiles which can be switched by the
		press of a button. A profile is split in settings and buttons.
		profile_settings holds information like resolution, sensitivity
		and light effects.
		When written, this file lets one write the respective profile
		settings back to the mouse. The data has to be 16 bytes long.
		The mouse will reject invalid data.
		Which profile to write is determined by the profile number
		contained in the data.
		This file is writeonly.
Users:		http://roccat.sourceforge.net

What:		/sys/bus/usb/devices/<busnum>-<devnum>:<config num>.<interface num>/<hid-bus>:<vendor-id>:<product-id>.<num>/kovaplus/roccatkovaplus<minor>/profile[1-5]_settings
Date:		January 2011
Contact:	Stefan Achatz <erazor_de@users.sourceforge.net>
Description:	The mouse can store 5 profiles which can be switched by the
		press of a button. A profile is split in settings and buttons.
		profile_settings holds information like resolution, sensitivity
		and light effects.
		When read, these files return the respective profile settings.
		The returned data is 16 bytes in size.
		This file is readonly.
Users:		http://roccat.sourceforge.net
