FREESCALE MX28EVK
==================

Supported hardware: only MX28EVK rev D is supported in U-boot.

Files of the MX28EVK port
--------------------------

arch/arm/cpu/arm926ejs/mxs/	- The CPU support code for the Freescale i.MX28
arch/arm/include/asm/arch-mxs/	- Header files for the Freescale i.MX28
board/freescale/mx28evk/	- MX28EVK board specific files
include/configs/mx28evk.h	- MX28EVK configuration file

Jumper configuration
---------------------

To boot MX28EVK from an SD card, set the boot mode DIP switches as:

   * Boot Mode Select: 1 0 0 1 (Boot from SD card Slot 0 - U42)
   * JTAG PSWITCH RESET: To the right (reset disabled)
   * Battery Source: Down
   * Wall 5V: Up
   * VDD 5V: To the left (off)
   * Hold Button: Down (off)

Follow the instructions from doc/README.mx28_common to generate a bootable SD
card.

Insert the SD card in slot 0, power up the board and U-boot will boot.
