U-Boot for Freescale i.MX6

This file contains information for the port of U-Boot to the Freescale i.MX6
SoC.

1. CONVENTIONS FOR FUSE ASSIGNMENTS
-----------------------------------

1.1 MAC Address: It is stored in fuse bank 4, with the 32 lsbs in word 2 and the
    16 msbs in word 3.
