ST33TPHF20 SPI TPMv2.0 bindings
-------------------------------

Required properties:
- compatible		: Should be "tis,tpm2-spi"
- reg			: SPI Chip select

Optional properties:
- gpio-reset		: Reset GPIO (if not connected to the SoC reset line)
- spi-max-frequency	: See spi-bus.txt

Example:

	tpm@1 {
		compatible = "tis,tpm2-spi";
		reg = <1>;
		spi-max-frequency = <10000000>;
	};
