.. SPDX-License-Identifier: GPL-2.0+
..  (C) Copyright 2019 Xilinx, Inc.

U-Boot device tree bindings
----------------------------

All the device tree bindings used in U-Boot are specified in Linux
kernel. Please refer dt bindings from below specified paths in Linux
kernel.

* ata
	- Documentation/devicetree/bindings/ata/ahci-ceva.txt
* gpio
	- Documentation/devicetree/bindings/gpio/gpio-xilinx.txt
	- Documentation/devicetree/bindings/gpio/gpio-zynq.txt
* i2c
	- Documentation/devicetree/bindings/i2c/i2c-xiic.txt
	- Documentation/devicetree/bindings/i2c/i2c-cadence.txt
* mmc
	- Documentation/devicetree/bindings/mmc/arasan,sdhci.txt
* net
	- Documentation/devicetree/bindings/net/macb.txt
	- Documentation/devicetree/bindings/net/xilinx_axienet.txt
	- Documentation/devicetree/bindings/net/xilinx_emaclite.txt
* serial
	- Documentation/devicetree/bindings/serial/cdns,uart.txt
	- Documentation/devicetree/bindings/serial/xlnx,opb-uartlite.txt
* spi
	- Documentation/devicetree/bindings/spi/spi-cadence.txt
	- Documentation/devicetree/bindings/spi/spi-xilinx.txt
	- Documentation/devicetree/bindings/spi/spi-zynqmp-qspi.txt
	- Documentation/devicetree/bindings/spi/spi-zynq-qspi.txt
* usb
	- Documentation/devicetree/bindings/usb/dwc3-xilinx.txt
	- Documentation/devicetree/bindings/usb/dwc3.txt
	- Documentation/devicetree/bindings/usb/ci-hdrc-usb2.txt
* wdt
	- Documentation/devicetree/bindings/watchdog/of-xilinx-wdt.txt
